|  |
| --- |
|  |
| Info Sheet for Motor vehicles |
|  |
|  |
|  |
|  |

 Please have a look at the Tender video instruction and tender user guide to learn how to add your products, optional equipment and discounts into UN Web Buy Plus tender portal.

Below, we provide you with some additional information for each product profile tab, tailored to your products.

1. **Main Details**

* **Catalogue:** Motor vehicles
* **Category:** You can choose from the dropdown menu, which contains all the twelve categories for this tender**.**
* Ambulance Advanced
* Ambulance
* Bus
* Cargo Van
* Electric Vehicle
* Hybrid Vehicle
* Minibus
* Mobile Clinic
* Multi-Purpose Vehicle
* Pick-Up
* Sedan
* SUV
* **Product Name:** In the Product Name field, you can choose a name for your product that will both be displayed on the product page in large and which will be searchable.

To give clear and concise name to the products, bidders are advised to use the below product names:

* 2WD Sedan/hatchback small
* 2WD Sedan large
* 2WD Sedan/hatchback mini
* 2WD Sedan/hatchback medium
* 2WD Station Wagon small
* 2WD Station Wagon large
* 2/4WD SUV
* 4WD SUV
* 4WD SUV
* 4WD SUV
* 2WD Pick-Up Single Cab
* 2WD Pick-Up Double Cab
* 4WD Pick-Up Single Cab
* 4WD Pick-Up Double Cab
* 4WD Pick-Up Single/Double Cab
* 2WD Minibus
* 4WD Minibus
* 2WD Multi-Purpose Vehicle
* 2WD Hybrid Vehicle (HEV)/Plug-in hybrid vehicle (PHEV)
* 2WD Bus
* 2/4WD Cargo Van /cargo Box vehicle
* 2/4WD Cooler Cargo Van /Cooler cargo Box vehicle
* 2WD Ambulance Advanced van/box type
* 4WD Ambulance on/off road type
* 2WD Ambulance van type
* 4WD Ambulance van type
* 2WD Mobile Clinic van type
* 4WD Mobile Clinic van type
* 2/4WD Electric Vehicle
* **Ordering Code (Product Code**): This is your own ordering code, which is used by your company to identify the purchased product.
* **Unit of Measure**: Please select “Each” as unit of measure and ‘’ Each’’ as sales unit
* The **minimum warranty** is set by default, but you can add a higher warranty and specify whether after-sales service is available at the “Warranty” tab

1. **Price**

* Each price should reflect the unit price. You can add a volume discount (e.g. 10 units +) at the discount tab.
* Price validity begins as of the next day

1. **Descriptions**

* Short Description: One sentence about the main purpose of the vehicles
* Long Description: It is supposed to explain to clients the purpose of a product, the environment it can be used in and restrictions to it, the product’s benefits, and summary of the main features. Please note that you can upload a full description of the unit to the “Documents” tab.

1. **Images**

* Please add pictures of the vehicles from different perspectives
* Name: Overall view, component 1, component 2, etc.
* Description: Vehicle overall view, available components may vary from represented image
* In total six images can be uploaded
* Please refer to the tender user guide, how to add, write name and description of pictures

1. **Specifications**

* Please fill out specifications as per the technical requirement in the tender documents

1. **Equipment**

Please note that when you add new products, the minimum required standard equipment is automatically inserted under the “standard equipment” tab. When adding new products via Excel, it is automatically inserted in the standard equipment cell of the first raw. When adding new rows you can copy/paste the equipment from the first row.

For those bidders who have current LTAs with UNOPS, the products were copied over from your previous LTA. **Please ensure that you update the standard equipment of each product to meet the requirements of the new ITB**. For that purpose, you can use the standard equipment lists provided for each category under point 14. Please make sure to use the correct lists for the respective categories. This applies when updating products one by one and in bulk through the Excel sheet.

1. **Shipping**

* Please add shipping dimensions (Length, Height and Width in millimeters (mm) as well as the Weight in kilograms (kg)), country of origin, port(s) of delivery, delivery time and Incoterm (as per the tender requirement).
* Add any specific/ additional information to the “shipping descriptions” field, for example how the product is packed (delivered fully/partially disassembled, etc.)

1. **Availability**

You can either enter the availability for each product in the product profile or assign it in bulk to several products at the end. Please see “Bulk Assignment box” below for more information.

1. **Warranty**

Add warranty (with after-sales service = with local representative, without after-sales service = without local representative). Like the availability, either you can enter the warranty for each unit, or you can set a warranty in bulk at the end. Please see “Bulk Assignment box” below for more information.

Please note that if no warranty is specified for a country where the vehicle is made available, the system will automatically assign the minimum warranty required in the ITB. It is not possible to offer vehicles without warranty.

Set countries where selected warranty and product combination are available.

*Please have a look into the Tender instruction videos and tender user guide for bulk availability assignment and warrant for more information.*

***For bulk assignment of availability and warranty:***

*Go to the “Assign Product Availability” menu (under “Products” tab) and assign availability to all products with the same availability. Afterwards, go to the “Set Warranty” menu (under “Products” tab) and assign the warranty to all products that have the same warranty and/or local representation.*

1. **Documents**

* Add a pdf file of product data sheet or product catalogue or product brochures
* Add the lists of spare parts kit and corresponding break down costs
* Any other relevant document in pdf format

1. **Optional Equipment**

* Please complete the available optional equipment as per the tender requirement

When adding optional equipment, please enter the price and, if applicable, indicate whether the option increases the shipping dimensions and/ or the delivery time of the unit.

Please do not forget to assign the added optional equipment to their respective product. To do this, follow the Tender instruction videos and tender user guide.

1. **Discounts**

* Please have a look into the Tender instruction videos and tender user guide how to add discounts.

Click on the Add new discount button.

**Type a name for the discount**. This name is solely displayed to you, so you are free to choose a name you like.

**Ranges:** You can select the scaling of the discount table on the left side called Ranges. Type a number of sales units in the Quantity column to indicate the lower threshold for the percentage discount. In the same row, indicate the percentage discount in the column on the right, Percentage, which you would like to associate with an order of a quantity equal to or larger than the quantity indicated.

You may add another level to the discount scaling by clicking on the white plus (  ) on the left column. A second row will appear in which a higher threshold has to be inserted and an associated percentage discount.

1. **Check FAQs**

**Go to** [**https://unwebbuyplus.org/#/faq**](https://unwebbuyplus.org/#/faq)

**Or click on the Support button **

1. **Standard equipment per category**
2. **Sedan- Category**

* 2WD Sedan/hatchback, small - 1000-1600 cc; WB 2400 - 2599 mm
* 2WD Sedan, large – 1595 -3500 cc; WB 2751 – 3100 mm
* 2WD Sedan/hatchback, mini 900 – 1600 cc; WB 1800 – 2399 mm
* 2WD Sedan/hatchback, medium – 1495 – 1800 cc, WB 2600 – 2750 mm

Air bags, minimum driver and passenger

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size. Emergency spare wheel or repair kit with air compressor accepted instead of the full size spare wheel.

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

1. **SUV- Category**

* 2WD Station Wagon, small - 1000-1600 cc; WB 2400 – 2599 mm
* 2WD Station Wagon, large - 1595-3500 cc; WB 2751 – 3100 mm
* 2/4WD SUV - 1290-2149 cc; WB 2000 - 2700 mm
* 4WD SUV - 2150-3200 cc; WB 2300 - 2699 mm
* 4WD SUV - 2150-3200 cc; WB 2700 - 3100 mm
* 4WD SUV - 3201-5600 cc; WB 2700 - 3200 mm

Air bags, minimum driver and passenger

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

1. **Pick-Up -Category**

* 2WD Pick-Up Single Cab - 1790-3200 cc; WB 2700 - 3600 mm
* 2WD Pick-Up Double Cab - 1790-3200 cc; WB 2700 - 3600 mm
* 4WD Pick-Up Single Cab - 1790-3200 cc; WB 2700 - 3600 mm
* 4WD Pick-Up Double Cab - 1790-3200 cc; WB 2700 - 3600 mm
* 4WD Pick-Up Single/Double Cab - 3201-5600 cc; WB 2700 - 3600 mm

Air bags, minimum driver and passenger

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

1. **Minibus -Category**

* 2WD Minibus - 1850-5600 cc; WB 2300 - 4500 mm
* 4WD Minibus - 1850-5600 cc; WB 2300 - 4500 mm

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

1. **Multi-Purpose Vehicle -Category**

* 2WD MPV (Multi-Purpose Vehicle) - 1790-3000 cc; WB 2300 - 3200 mm

Air bags, minimum driver and passenger

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

1. **Hybrid Vehicle-Category**

* 2WD Hybrid Vehicle (HEV)/Plug-in hybrid vehicle (PHEV) - 900-2500 cc; WB 2000 - 3100 mm

Air bags, minimum driver and passenger

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size. Emergency spare wheel or repair kit with air compressor accepted instead of the full size spare wheel.

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

Charge cable(s)

Charge station for vehicle

1. **Bus -Category**

* 2WD Bus, general purpose overland - 3490 -6000 cc; WB 3200 - 6000 mm

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

1. **Cargo Van -Category**

* 2/4WD Cargo Van /cargo Box vehicle 1850-5600 cc; WB 2300 - 4500 mm
* 2/4WD Cooler Cargo Van /Cooler cargo Box vehicle 1850-5600 cc; WB 2300 - 4500 mm

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

Van or closed cargo box, dust proof, made from steel, aluminum or composite material, with minimum rear gate, with lock

Cooler version only: Refrigeration cooler unit in cargo room, driven by the vehicle engine or standalone function. Must be insulated to maintain 2 C degrees or below at tropical conditions.

Light in cargo room

Cooler version only: Food grade material on all surfaces. Easily washable. Sealed in all corners and to the floor.

Sturdy floor made from hardwood, stainless steel or aluminum

Cargo fixing eyes/hooks along sides, inside cargo room

1. **Ambulance Advanced-Category**

* 2WD Ambulance Advanced; van/box type -1850-5600 cc; WB 2300-4500 mm

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

Extended first aid kit

Flashing beacon - red or blue – to be determined when ordering

IV – hangers, minimum 2

Light inside patient compartment

Red cross/red crescent, sides rear & roof

Seat for attendant

Siren & PA system with microphone

Stretcher main, with caster

Wipe clean interior panels including partition wall with sliding window & linoleum floor

5 kg fire extinguisher, minimum

Adult splint kit

Air condition, front & rear

Battery charge function from AC grid with socket, to keep batteries always fully charged while garaged

Beacon lamp, minimum single, color TBD. Mounted at the rear of the roof.

First aid kit

Fixed oxygen system with wall plug and bottles to be installed into a cupboard with sign ‘Oxygen bottles’. Connection norm TBD in case

Flood working lamp, mounted at rear gate doors.

Fog lamps, 2 front and minimum 1 rear

Front mounted strobe lamps integrated in front grill; color TBD.

Owner’s manual for all installed equipment, language TBD

Portable oxygen equipment

Power locking doors, all doors, remote controlled

Pulse oximeter (saturometer)

RCP board

Side flood lamp, min. 1 each side

Side LED strobe lamps on side of vehicle; color TBD, minimum 3 each side

Siren with ‘yelp’ function & PA system with microphone

Spinal board

Spot lamp, inside, with flexible arm

Bench for attendance with storage room underneath

Blood pressure unit

Defibrillator with monitor

Dual battery with automatic split charge function & DC to AC inverter to match installed standard equipment + 50%

Durable vinyl floor or equivalent, easily washable.

Electric sockets, minimum 4 x 12V DC & 4 x 220/230/240V AC

Emergency blanket

Emergency respiration unit

Female & male plastic wedge

Frosted glass 2/3 rear compartment

Harness type Spider

Heater, front & rear

Inside roof rail/hand grabs

IV hooks, minimum 3

Light inside patient compartment, min. 4 x 36W tubes or equivalent LED

Manual suction pump

Monitor – ECG, SpO2, NIBP, Temp., respiration with minimum 4-hour battery.

Multi Flashing Beacon bar mounted at front of the roof – color TBD

Reading lamp in driver cabin

Rear seat for attendant

Red cross/red crescent, sides rear & roof

Resuscitator, manual for adults and children

Resuscitator, portable

Reverse warning buzzer

Roof ventilation, 12V, with open/close function

Shelves & cupboards, full sidewall, with sliding transparent hatches. Minimum one cupboard lockable.

Short spine immobilizer

Stethoscope

Stretcher, main, with washable mattress and tilt able head, fixing belts and automatic undercarriage operation when taken in and out of ambulance. Head immobilizer. Locking system to floor.

Sub stretcher, foldable

Torch, wall mounted charger

Transverse roof strobe warning light bar, color TBD. Mounted in front of the roof

Trauma kit

Water tank minimum 3 liters, wash basin with electric pump and tap, heated water.

Wipe clean interior panels including partition wall & floor. Slide able window between driver and patient compartment.

1. **Ambulance -Category**

* 4WD Ambulance, on/off road type -2400-5600 cc WB 2700 - 3200 mm
* 2WD Ambulance; van type - 1850-5600 cc; WB 2300 - 4500 mm
* 4WD Ambulance, van type -1850-5600 cc; WB 2300 - 4500 mm

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

Extended first aid kit

Flashing beacon - red or blue – to be determined when ordering

IV – hangers, minimum 2

Light inside patient compartment

Red cross/red crescent, sides rear & roof

Seat for attendant

Siren & PA system with microphone

Stretcher main, with caster

Wipe clean interior panels including partition wall with sliding window & linoleum floor

1. **Mobile Clinic -Category**

* 2WD Mobile Clinic; van type -1850-5600 cc, WB 2300 - 4500 mm
* 4WD Mobile Clinic; van type -1850-5600 cc, WB 2300 - 4500 mm

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

5 kg fire extinguisher, minimum

Air condition, front & rear while engine is running.

Battery charge function from AC grid with socket, to keep batteries always fully charged while garaged

Drawers, minimum 4 and one cupboard under the working table. Minimum one with lock.

Dual battery with automatic split charge function & DC to AC inverter to match installed standard equipment + 50%

Durable vinyl floor or equivalent, easily washable.

Electric sockets, min. 4 x 110/115/120V or 220/230/240V AC. Min 2 x 12V DC outlet in rear department. Inverter DC/AC minimum 1000W. Voltage TBD. Actual wall plugs TBD

First aid kit.

Frosted glass 2/3 in rear compartment or tinted, TBD

Hand cleaner dispensers wall mounted and hook for towel

IV hooks, minimum 2

Light inside patient compartment, minimum AC 2 x 800 lumen and DC 2 x 400 lumen, LED

Owner’s manual for all installed equipment, language TBD

Patient comfortable chair (car type), multi adjustable, for one-person minimum

Petrol generator set, kVA = 2 x load of standard equipment and in any case be able to meet all installed equipment. With electric start. Minimum 25 m heavy-duty rubber extension cord. Outside vehicle plug, which can also plug electricity from the external grid. Must be securely stored inside the vehicle during transport and easily lifted in and out. 50/60Hz TBD

Rear bench seat parallel against wall with backrest and storage in bench box

Refrigerator, 50 liters capacity minimum capable to keep 2 °C at tropical conditions. With lock. To be operated by AC and 12 V DC. With outside temperature display.

Roof ventilation, 12V, with open/close function

Spot lamp, inside rear cabin, with flexible arm

Staff/examiners chair, to be secured while driving the vehicle.

Torch, LED, wall mounted with charger

Water tank minimum 3 liters, wash basin with electric pump and tap, heated water.

Wipe clean interior panels incl. partition wall & floor. Slide able window between driver and patient compartment

Working table, angled: Plate 1: min L: 0.80 x W: 0.40 m + plate 2: min. L: 0.40 x W: 0.40 m, both with hard surface like Formica or equivalent

1. **Electric Vehicle-Category**

* 2/4WD Electric Vehicle (EV), N/A cc; WB 2000 - 3100 mm

Air bags, minimum driver and passenger

Air condition (non CFC) (A/C) & heater

Fire extinguisher, 1 kg minimum

Door mirrors, left & right

First aid kit

Headrests, front

Lockable fuel tank lid/cap

Owner’s manual

Power steering

Radio, AM/FM

Seat belts, front and rear

Spare wheel full size. Emergency spare wheel or repair kit with air compressor accepted instead of the full size spare wheel.

Sun visors, 2 pcs

Tool kit with jack

Towing eye/hook or other provision for towing of the vehicle, front & rear

Warning triangle

12 V socket at front seats

Homologated/approved for country of destination

Charge cable(s)

Charge station for vehicle

1. **Matching UN Web Buy Plus Category and Lot/Category under Section II of Schedule of Requirements**

|  |  |  |
| --- | --- | --- |
| **UN Web Buy Plus Category** | **Name of products** | **Section II: Schedule of Requirements- Lot/Category** |
| Sedan | * 2WD Sedan/hatchback, small - 1000-1600 cc; WB 2400 - 2599 mm * 2WD Sedan, large – 1595 -3500 cc; WB 2751 – 3100 mm * 2WD Sedan/hatchback, mini 900 – 1600 cc; WB 1800 – 2399 mm * 2WD Sedan/hatchback, medium – 1495 – 1800 cc, WB 2600 – 2750 mm | 1, 2,27,28 |
| SUV | * 2WD Station Wagon, small - 1000-1600 cc; WB 2400 – 2599 mm * 2WD Station Wagon, large - 1595-3500 cc; WB 2751 – 3100 mm * 2/4WD SUV - 1290-2149 cc; WB 2000 - 2700 mm * 4WD SUV - 2150-3200 cc; WB 2300 - 2699 mm * 4WD SUV - 2150-3200 cc; WB 2700 - 3100 mm * 4WD SUV - 3201-5600 cc; WB 2700 - 3200 mm | 3,4,5,6,7,8 |
| Pick-Up | * 2WD Pick-Up Single Cab - 1790-3200 cc; WB 2700 - 3600 mm * 2WD Pick-Up Double Cab - 1790-3200 cc; WB 2700 - 3600 mm * 4WD Pick-Up Single Cab - 1790-3200 cc; WB 2700 - 3600 mm * 4WD Pick-Up Double Cab - 1790-3200 cc; WB 2700 - 3600 mm * 4WD Pick-Up Single/Double Cab - 3201-5600 cc; WB 2700 - 3600 mm | 9,10,11,12,13 |
| Minibus | * 2WD Minibus - 1850-5600 cc; WB 2300 - 4500 mm * 4WD Minibus - 1850-5600 cc; WB 2300 - 4500 mm | 14,15 |
| Multi-Purpose Vehicle | * 2WD MPV (Multi-Purpose Vehicle) - 1790-3000 cc; WB 2300 - 3200 mm | 16 |
| Hybrid Vehicle | * 2WD Hybrid Vehicle (HEV)/Plug-in hybrid vehicle (PHEV) - 900-2500 cc; WB 2000 - 3100 mm | 17 |
| Bus | * 2WD Bus, general purpose overland - 3490 -6000 cc; WB 3200 - 6000 mm | 18 |
| Cargo Van | * 2/4WD Cargo Van /cargo Box vehicle 1850-5600 cc; WB 2300 - 4500 mm * 2/4WD Cooler Cargo Van /Cooler cargo Box vehicle 1850-5600 cc; WB 2300 - 4500 mm | 19, 26 |
| Ambulance Advanced | * 2WD Ambulance Advanced; van/box type -1850-5600 cc; WB 2300-4500 mm | 20 |
| Ambulance | * 4WD Ambulance, on/off road type -2400-5600 cc WB 2700 - 3200 mm * 2WD Ambulance; van type - 1850-5600 cc; WB 2300 - 4500 mm * 4WD Ambulance, van type -1850-5600 cc; WB 2300 - 4500 mm | 21,22,23 |
| Mobile Clinic | * 2WD Mobile Clinic; van type -1850-5600 cc, WB 2300 - 4500 mm * 4WD Mobile Clinic; van type -1850-5600 cc, WB 2300 - 4500 mm | 24,25 |
| Electric Vehicle | * 2/4WD Electric Vehicle (EV), N/A cc; WB 2000 - 3100 mm | 29 |