**Section II: Schedule of Requirements**

**eSourcing reference:** RFQ/2021/21414

**Technical specifications for Goods and Comparative Data Table:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item No** | **UNOPS minimum technical requirements** | **QTY** | **Is bid compliant? Bidder to complete** | **Details of goods offered. Bidder to complete**  Insert details of goods offered, including specifications and brand/model offered if applicable |
| 1 | **Outdoor Playground Size 1 (Medium Size) with the following specifications:** | **6** | ☐ Yes ☐ No |  |
| 1.a | **Material:**  **Plastic Parts:**  Linear low density Polyethylene (LLDPE)  6mm minimum wall thickness  UV stabilized pigments  Anti – static inhibitors- non- toxic lead free paint. | ☐ Yes ☐ No |  |
| 1.b | **Metal Parts:**  Black carbon steel pipes (various sizes 1” to 3”), internal thickness (1.8mm to 3mm)  Pre-treatment wash primer or sandblasting to remove all rust  Powder coat finish (see below) | ☐ Yes ☐ No |  |
| 1.c | **Deck & Stair case:**  Color powder coating or PVC coating.  14 gauge (1.8 to 2mm) HR steel  CNC Perforated surface – 12.5mm diameter perforations  Pre-treatment wash primer or sandblasting to remove all rust  Anti-slip polyurethane paint finish | ☐ Yes ☐ No |  |
| 1.d | **Component:**  2 Grove Single slide  Platforms  Roof  Stairs  Tunnel  2 Different Climbers: Rock or Horizontal Leader or Net  Crawl Tubes  Suspension Bridge with Chains | ☐ Yes ☐ No |  |
| 1.e | **Height:**  Between 3 – 3.5 meter | ☐ Yes ☐ No |  |
| 1.f | **Capacity:**  35 Student (Age Group from 4- 12 Year) | ☐ Yes ☐ No |  |
| 1.g | **Colours:**  The supplier shall present options for available colours of the apparatus; so that the designer may choose from. | ☐ Yes ☐ No |  |
| 1.h | **Warranty:**  Lifetime against structural failure  10 years on materials and workmanship |  |  |  |
| 1.i | **Installation:**  The supplier shall execute the foundations of the apparatus and provide materials & labor, as per the weight and size of the unit |  |  |  |
| 2 | **Outdoor Playground Size 2 (Small Size) with the following specifications:** | **2** | ☐ Yes ☐ No |  |
| 2.a | **Material:**  **Plastic Parts:**  Linear low density Polyethylene (LLDPE)  6mm minimum wall thickness  UV stabilized pigments  Anti – static inhibitors- non- toxic lead free paint. |  | ☐ Yes ☐ No |  |
| 2.b | **Metal Parts:**  Black carbon steel pipes (various sizes 1” to 3”), internal thickness (1.8mm to 3mm)  Pre-treatment wash primer or sandblasting to remove all rust  Powder coat finish (see below) | ☐ Yes ☐ No |  |
| 2.c | **Deck & Stair case:**  Color powder coating or PVC coating.  14 gauge (1.8 to 2mm) HR steel  CNC Perforated surface – 12.5mm diameter perforations  Pre-treatment wash primer or sandblasting to remove all rust  Anti-slip polyurethane paint finish | ☐ Yes ☐ No |  |
| 2.d | **Component:**  2 Grove Single slide  Platforms  Roof  Stairs  Tunnel  1 Climbers: Rock or Horizontal Leader or Net  Crawl Tubes | ☐ Yes ☐ No |  |
| 2.e | **Height:**  Between 3 – 3.5 meter | ☐ Yes ☐ No |  |
| 2.f | **Capacity:**  25 Student (Age Group from 4- 12 Year) | ☐ Yes ☐ No |  |
| 2.g | **Colours:**  The supplier shall present options for available colours of the apparatus; so that the designer may choose from. |  |  |
| 2.h | **Warranty:**  Lifetime against structural failure  10 years on materials and workmanship | ☐ Yes ☐ No |  |
| 2.i | **Installation:**  The supplier shall execute the foundations of the apparatus and provide materials & labor, as per the weight and size of the unit | ☐ Yes ☐ No |  |
|  | | **The picture is for indicative purpose only** | | |

**Delivery requirements and Comparative Data Table:**

|  |  |  |  |
| --- | --- | --- | --- |
| **UNOPS Requirements** | | **Is quotation compliant?** Bidder to complete | **Details**  Bidder to complete |
| **Delivery time** | Bidder shall deliver the goods  8-10 weeks after Contract signature. | ☐ Yes ☐ No | Insert details |
| **Delivery place and Incoterms rules** | DAP- as per the distribution list | ☐ Yes ☐ No | Insert details |
| **Consignee details** | TBC | ☐ Yes ☐ No | Insert details |
| **UNOPS Right to vary requirements** | At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- [50%] , without any change in the unit prices or other terms and conditions of the RFQ. | ☐ Yes ☐ No | Insert details |

**Notes**

**Notes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **#** | **UNOPS Requirements** | **Is quotation compliant?** Bidder to complete | **Details**  Bidder to complete |
| **1** | The Supplier shall provide all required fixation to the playground equipment as required from the Manufacturer, and subject to the UNOPS approval. | ☐ Yes ☐ No | Insert details |
| **2** | Suggested designs (layout) shall be submitted one week later after awarding the contract. | ☐ Yes ☐ No | Insert details |
| **3** | UNOPS reserves the right to have some minor changes such as removing the roofs, changing the height or colores under the same price. | ☐ Yes ☐ No | Insert details |
| **4** | An assessment visit to the site shall be done before supplying the goods. | ☐ Yes ☐ No | Insert details |
| **5** | The supplier will remain liable for the safety of apparatus and equipment until UNOPS conducts the final inspection visit. (He shall secure the equipment during the installation period). | ☐ Yes ☐ No | Insert details |
| **6** | The delivery date might change and the supplier shall accommodate this change. | ☐ Yes ☐ No | Insert details |
| **7** | The supplier must have a storage facility to accommodate the equipment until delivery takes place. | ☐ Yes ☐ No | Insert details |
| **8** | The locations are in several governorates in Jordan not only in Amman | ☐ Yes ☐ No | Insert details |
| **9** | The supplier shall provide after sale services and spare parts within a month when needed. | ☐ Yes ☐ No | Insert details |