# Schedule of Requirements

*STATEMENT OF NEED: for driver transportation and easy access to office for air port shuttles, staff shuttles and driver mode of transport to get home.*

**Technical Specifications for Goods:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Item No** | **Minimum Technical Requirements** | **Unit** | **Quantity** |
| 1 | Engine size: 249 Cylinders:1 hp/kW:18/13, 20/15 Vehicle weight (kg):148 Valve clearance (intake):KALT 0,05 MM Valve clearance (exhaust):KALT 0,08 MM Engine idle speed:1300 ± 100 U/MIN Carburettor air screw:2 AUSDREHUNGEN Tyre pressure (front):1,5 BAR Tyre pressure (rear):1,5 BAR Spark plug 1:NGK DR8ES-L Spark plug 2:NGK DR8EIX Electrode gap:0,6 MM Fork tube diam.:35 MM TELEGABEL Front/rear sprockets:14/53 ZÄHNE Chain/Final drive:102 GLIEDER  Capacities\* Fork oil per rod:190 ML Engine oil w/o filter:1,1 L SAE 10W-40 Engine oil with filter:1,3 LITER Brake fluid:MECH.TROMMELBREMS. Fuel:9,5 LITER Coolant:LUFTGEKÜHLT   Complete built unit along with all standard mounting and accessories e.g.2 helmets, tool kit, leg guard, mud flaps,seat covers and standard fitments | each | 3 |
| 2 | Warranty & After sales service | each | 3 |