**Bassinet**

Product description

Cot, baby, hospital, with bassinet, on castors

Specifications

Mobile baby cot with removable bassinet

Mounted on 4 swivel castors, heavy duty, 2 with brake

With aeration holes

With position TR/RTR

Transfer bars connect all lower distal portions of the 4 legs, providing maximal structural strength

With padded mattress, detachable for easy cleaning

Mattress cover removable via side zipper

Basinet sets and removes smoothly from cart frame

Materials:

High resistance to corrosion (tropical environment)

Frame: epoxy coated tubular steel.

Mattress: high-density polyurethane foam, density 18-22kg/m3.

Cover: plastic, flexible highly tear resistant, anti-static, disinfectant- and liquid proof, washable

Caster frame/bracket: steel or nylon

Caster brake: total-lock type (wheel and rotational lock)

Caster wheel: single wheel, mold-on type, non-hooded (for easy maintenance)

Wheel bearing: sealed bearing in the swivel and the wheel

Dimensions:

Frame: 72-88x40-50x81-99cm (l x w x h)

Bassinet: 63-77x36-44x27-33cm (l x w x h)

Frame: 2.5-3.5cm (outside, across), 1.35-1.65mm (thickness)

Swivel castor wheels: 2-3 x 7-8cm (w x diameter)

Mattress: 6-8cm (h)

Carrying capacity: 27-33kg

Knockdown construction: yes

Supplied with

1 x complete set of tools required for assembly

1 x fitting removable mattress with cover

List of accessories and parts

Detailed step-by-step instructions for assembly and safe use, text-free pictorial based (i.e. line-drawings only)

Packaging, labelling, instructions:

One (1) unit per box

Dimensions:

Unit Weight in Kg (including its packaging)

Unit Volume in M3 (including its packaging)

Dimensions of box, length x width x height in cm

Dimensions of box, length x width x height in cm

Labelling:

Compliance with EAN 128 bar code requirements

**Special Notes:**

Note: All dimensions are to be interpreted with 10 % manufacturing tolerance.