**Bed, labor/delivery, with 3-pce mattress**

Gynecological examination and delivery table, 3 sections

Mounted on 4 sturdy supports, all finished with height adjustable feet

All sections fitted with non-removable padded upholstery

Robust mechanics allow for manual repositioning of all sections between gynecological and obstetric use

Transfer bars connect all lower distal portions of the 4 supports, providing maximal structural strength

Back section:

Adjustable via secured pawl and gear ratchet, safe for patient and operator

Pelvic section:

Can be tilted to Trendelenburg position with lever handle

Sides of this section are fit with vertical handgrips, length 20 cm

Padded knee crutches are height and width adjustable, set with robust clamps with heavy knob

Fixing of the crutch holders is solid steel and welded to the frame of the bed

This section integrates a support for a slide-out basin-tray

Leg section:

Recesses entirely downwards, 90 degrees

When elevated and fully extended, all sections align to perfectly flat surface.

**Materials**:

High resistance to corrosion (tropical environment)

Frame: epoxy coated tubular steel

Adjustable feet: rubber or nylon

Sliders/fixtures for the knee crutches: tubular steel, welded to the bed frame

Padded upholstery: high-density polyurethane foam, density 27-33 kg/m3

Cover: plastic, flexible highly tear resistant, anti-static, flame retardant, disinfectant- and liquid proof, washable

Basin-tray: Austenitic stainless steel, 18/10

**Dimensions**:

All 3 sections extended, including padding: 162-198x72-88x72-88cm (l x w x h)

Frame: 2.7-3.3cm (outside, across), 1.8-2.2mm (thickness)

Padded upholstery: 4.5-7.5cm (h)

Carrying capacity: 135-165 kg

Slide-out basin-tray, capacity: 4L

Knockdown construction: yes

**Items supplied with:**

1 x complete set of tools required for assembly

2 x leg holders with canvas straps, adjustable height and width

2 x knee crutches, adjustable height and width

1 x basin-tray

List of accessories and parts

Detailed step-by-step instructions for assembly and safe use, text-free pictorial based (i.e. line-drawings only)

**Packaging and labeling:**

One (1) unit per box

**Weight and volume:** 51.5 Kg, 0.35 M3

Compliance with EAN 128 bar code requirements