|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S/n** | **Item description** | **Minimum Acceptable Specifications** | **Quantity** | **UoM** | **Picture** |
| 1. | **PA300 electric siren manufactured by Federal Signal Corporation.** | This siren should provide 200-Watt output to meet or exceed SAE J1849 and Class A requirements for  sound when paired with a Federal Signal high-power speaker.  The siren unit must have (5) basic siren tones, TAP II (horn-ring transfer), PA, radio rebroadcast and air horn sound with siren override. TAP II allows for effective intersection traffic clearing capability.  Electrical System  The siren operates from any 12- or 24-volt negative ground vehicle electrical system. The PA300 can be powered directly by the car’s battery or through secondary power distribution centers.  Features:   * 690010 690000 that is 12-volt, 200-watt version. * MNCT-SD Microphone, noise-canceling, PA/Radio * AUDIO OUTPUT POWER 200 W * INPUT VOLTAGE 11/15 Vdc (690010) 24/28 Vdc (690009) * NOMINAL OUTPUT VOLTAGE 64 V peak-to-peak * STANDBY CURRENT 120 mA * INPUT CURRENT, OPERATING 10 A max (690010) 5 A max (690009) * OPERATING TEMP. -22˚ to +149˚ F (-30˚ to + 65˚ C) * POLARITY Negative ground only. * FREQUENCY RANGE 725 to 1800 Hz * LENGTH 8.5 in (21.6 cm) * WIDTH 6.5 in (16.5 cm) * HEIGHT 2.5 in (6.4 cm) | 1 | EA |  |
| 2. | **Federal Signal Navigator vehicle emergency light bar** | NVG45Z-NFPA20 45" Navigator, Convergence Network, (4) QL64 Red/White, (4) QL64 Red/Amber with SML integration, (2) QL43 Red/White, (2)  QL73 Red, (2) QL73 Red/White, Clear domes, Clear bulkheads and a Hook mount. | 1 |  |  |
| 3. | **Rumbler Low-Frequency Siren for Police Vehicles (M2045)** | RBKIT2-COMPACT: Pair of Rumbler Compact low frequency speakers for use with sirens with integrated Rumbler capability.  Model: M2045.  Features:  Audio Output Power: 80 W  Input Voltage: 9/15 Vdc  Nominal Output Voltage: 64 V peak-to-peak  Standby Current: 0.025 A  Input Current, Operating: 12 A max.  Operating Temp. -22˚ to +149˚ F (-30˚ to + +65˚C)  Polarity: Negative ground only  Frequency Range; 182 to 400 Hz | 1 |  |  |

|  |  |
| --- | --- |
| Delivery time | Immediately |
| **TERMS OF WARRANTY** | |
| Warranty accepted | Minimum one year. |
| **DELIVERY TERMS** | |
| Applicable INCOTERMS: | DAP |
| Final Delivery Place: | UNHCR, Sub Office Ogoja |

\***General requirements:**

1. Pictures used above are indicative only and do not represent the actually requested items; they are used only for purposes of illustration and to give an idea of the requested items.
2. Installation, transportation, assembly, and installation loading and offloading and any other miscellaneous cost shall be quoted all-inclusive in the offer.