OTF-28 - Bed with washable mattress cover

**Description**

*Mechanical bed with mattress.*

**Reference Picture**

*Note: The images below are intended solely as a guiding support and should be considered as purely indicative and not restrictive of the expected item characteristics*



| Brand / Marque | |  | |
| --- | --- | --- | --- |
| Model / Modèle | |  | |
| Model code as per manufacturer classification / Numéro de référence du produit fournisseur | |  | |
| Manufacturer name / Nom du Fabricant | |  | |
| Manufacturing site / Site du Fabricant | |  | |
| Country of manufacturing / Pays de fabrication | |  | |
| Country of origin / Pays d'origine | |  | |

|  | **UNOPS Minimum technical requirements // Exigences techniques minimales de l'UNOPS** | **Complies (Yes/No) // Conforme (Oui/Non)** | **Comments/ Technical data //**  **Commentaires/Données techniques** |
| --- | --- | --- | --- |
| **A** | **Functionality and Performance / Fonctionnalité et performances** |  |  |
| 1 | Made up of 2 sections. |  |  |
| 2 | Working load of at least 200 kg. |  |  |
| 3 | Platform dimension (LxW): 2000 X 900 +/- 15%. |  |  |
| 4 | Adjustable backrest inclination: at least 0-45° by manual rod (crank). |  |  |
| 5 | Structure material: stainless steel AISI 304 or epoxy coated tubular steel (or similar finish), resistant to hospital-grade disinfectant products or equivalent material. |  |  |
| 6 | Bed sheet tops made from perforated stainless steel AISI 304, epoxy powder coated (or similar finish) or equivalent material resistant to hospital-grade disinfectant products. |  |  |
| 7 | Head & Footboard: stainless steel AISI 304 or epoxy coated steel (or similar finish) or ABS or equivalent material resistant to hospital-grade disinfectant products. |  |  |
| 8 | Side Rails: two collapsible or foldable stainless steel AISI 304, epoxy powder coated or aluminum alloy side rails. |  |  |
| 9 | Intravenous fluid pole: stainless steel, at least 2 hooks |  |  |
| 10 | Mattress:   * Suitable for the bed, two sections; * High density polyurethane foam interior: at least 28kg/m3; * With a steady (stable) pressure reduction surface at all body points. * Flame-retardant; * Dimensions (W x L): 900 mm x 2000 mm +/- 15 % as bed platform size; * Thickness: at least 14 cm; * Cover: plastic, flexible, tear resistant, anti-static, anti-bacteria, flame-retardant, non-absorbing, waterproof and cleanable with hospital-grade disinfection products. Removable via zipper. |  |  |
| 11 | All materials resistant to corrosion and the use of hospital-grade disinfectants. |  |  |
| **B** | **Certifications and post sales included in the offered price** |  |  |
| 1 | The Supplier, included in the offered price, will provide the post sales services described in the document “OT-PS Type II post sales requirements for Medical Devices”. |  |  |
| C | **Supplied with** |  |  |
| 1 | Detailed step-by-step instructions for assembly and cleaning in pictograms. |  |  |
| 2 | Tools required for assembly. |  |  |
| **D** | **ANY DEVIATIONS OR SUPERIOR CHARACTERISTICS MUST BE INDICATED BELOW // TOUTE DÉVIATION OU CARACTÉRISTIQUE SUPÉRIEURE DOIT ÊTRE INDIQUÉE CI-DESSOUS\* :** | | |
|  | | |