OTF-14 - Instrument trolley

**Description**

*Instrument trolley with two shelves. Cart for transporting instruments, medicines, healing materials and supplies for healing procedures in hospitals.*

**Reference Picture:**

*Note: The images below are intended solely as a guiding support and should be considered as purely indicative and not restrictive of the expected item characteristics*



| Brand / Marque | |  | |
| --- | --- | --- | --- |
| Model / Modèle | |  | |
| Model code as per manufacturer classification / Numéro de référence du produit fournisseur | |  | |
| Manufacturer name / Nom du Fabricant | |  | |
| Manufacturing site / Site du Fabricant | |  | |
| Country of manufacturing / Pays de fabrication | |  | |
| Country of origin / Pays d'origine | |  | |

|  | **UNOPS Minimum technical requirements // Exigences techniques minimales de l'UNOPS** | **Complies (Yes/No) // Conforme (Oui/Non)** | **Comments/ Technical data //**  **Commentaires/Données techniques** |
| --- | --- | --- | --- |
| **A** | **Functionality and Performance / Fonctionnalité et performances** |  |  |
| 1 | Dimensions: width: 1300\*700\*800mm (L\*W\*H) +/- 15%. |  |  |
| 2 | Two (2) shelves. Smooth finishing for easy cleaning. With guard rails, at least on three sides: one long side and both short sides. |  |  |
| 3 | Height between shelves: not less than 400 mm. |  |  |
| 4 | Material of frame and shelves: stainless steel at least grade AISI 304. |  |  |
| 5 | Mounted on 4 anti-static swivel castors, rubber or similar material. Minimum diameter 100 mm. At least two with brakes. |  |  |
| 6 | All materials resistant to corrosion and the use of hospital-grade disinfectants. |  |  |
| **B** | **Certifications and post sales included in the offered price** |  |  |
| 1 | The Supplier, included in the offered price, will provide the post sales services described in the document “*OT-PS Type 0 post sales requirements for Non Medical Items*”. |  |  |
| C | **Supplied with** |  |  |
| 1 | Detailed step-by-step instructions for assembly and cleaning in pictograms. |  |  |
| 2 | Tools required for assembly. |  |  |
| **D** | **ANY DEVIATIONS OR SUPERIOR CHARACTERISTICS MUST BE INDICATED BELOW // TOUTE DÉVIATION OU CARACTÉRISTIQUE SUPÉRIEURE DOIT ÊTRE INDIQUÉE CI-DESSOUS\* :** | | |
|  | | |