**Annex – 3**

**Product Item Overview Form**

|  |  |  |  |
| --- | --- | --- | --- |
| **Item No.** | **Description and minimum /mandatory specifications** | **Description of items offered and Bidder’s statements on deviations**  (To be completed by the bidder) | **Compliant? (Y/N)**  (To be completed by UNFPA during evaluation) |
|  | **Year of manufacturing:**   * Not earlier than 2023 |  |  |
|  | **Body**:   * Type - crossover. * Color - white. * Number of seats (inc. driver), pcs. - at least 5 |  |  |
|  | **Engine**:   * Type - gasoline, diesel, hybrid. * The working volume of the engine, cm3 - from 1450 to 3000 * maximum engine power, hp. - at least 100 * Maximum speed, km/h. - at least 160 * Emission standard - Minimum Euro 5. |  |  |
|  | **Transmission**:   * Gearbox- Automatic * Number of gears: At least 6 |  |  |
|  | **Chassis and suspension:**   * Discs- light alloy, tires R17 * Wheel drive- 4WD (4 х 4) * Clearance (mm)- At least 180 * Front suspension- Independent, spring with MacPherson struts and anti-roll bar * Rear suspension- Independent, spring with two double wishbones and anti-roll bar |  |  |
|  | **Steering**:   * Power steering- Electrical * Steering orientation- Left Side |  |  |
|  | **Braking system:**   * Type- Hydraulic with amplifier * Front wheels- Brake discs * Rear wheels- Brake discs |  |  |
|  | **Climate in the cabin:**   * Front seats - Climate control * Back seat - Climate control (optional and will be considered as an asset) |  |  |
|  | **Safety:**   * Anti-lock braking system (ABS); * Airbags- For the driver and passenger (at least 4 pcs.) * Reinforced bumpers- Protective front arches or reinforced bumper * Engine Protection- Metal engine compartment protection |  |  |
|  | **Additional Equipment:**   * Spare Wheel: Full-size (Disc diameter at least 17 inches) * Anti-theft device Immobilizer. * Central door lock: With remote control * Parking assistance: Parktronic (safe parking device) * Windows: Armored anti-shock film (4 mil) * Threshold protection: Protective film (200 microns) |  |  |
|  | **Other Features:**   * The seats must be equipped with covers made of wear-resistant materials and basic safety belts with fasteners. * sound and light (LED) signal devices (signal-loud-speaking device, LED bar with blue and red strobe lights) with capacity of 100 Wt at least mounted on a special console on the roof; * Searchlight: Electrical or mechanical control - next to the seats, in an easily accessible and convenient place, installed a control unit with special light and sound signaling devices and the device for electric or mechanical control of the searchlight. * Multimedia system/Car Play/Android Auto with GPS navigation + GPS Tracker * Radio: VHF car radio station (Range: 148 – 174 MHz) , Range of operating frequencies MHz:148 – 174 ( the radio wave range to be additional agreed with local police department): * Programming of the grid pitch: 12.5 kHz and 25 kHz with frequency deviation +/- 2.5 kHz and 5 kHz, respectively · Sensitivity of the receiver not worse than 0.25 μV at a signal to noise ratio (SINAD) 12 dB· * Cameras: Front and rear video recording during movement * ·Winter tires: Must be provided |  |  |
|  | * **Warranty obligations:** * Duration: minimum two years or 100,000 km from the date of delivery and commissioning * Repair and Maintenance: Warranty services should include regular maintenance checks and repair services at no additional cost. * Authorized Service Centers: Warranty services must be carried out by authorized service centers in Ukraine. The bidder must provide a list of these authorized centers along with their locations and contact details. * Documentation: * -The supplier must provide an official letter indicating the authorized local dealer that will provide warranty services, after-sales support, installation (where applicable), and commissioning. * -The supplier must provide a detailed warranty document outlining the terms and conditions, claim procedures, and contact information for warranty services. * -A warranty card must be included with each vehicle, indicating the start date of the warranty period. |  |  |