**Annex 1 (Returnable Bidding from)**

**Schedule of Requirements**

Note to Bidders: The following returnable forms are part of this RFQ and must be completed and returned by bidders as part of their quotation. Instructions to complete each Form are highlighted in Yellow in each Form. Please complete the Returnable Bidding Forms as instructed and return them as part of your quotation.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **ITEM**  **NO.** | DESCRIPTION OF GOODS AND/OR SERVICES | UNIT | QTY | **CURRENCY** | |  | **IQD** |
| **UNIT PRICE** | | **Total AMOUNT** | |
| **1.** | **Lot 1: Bricklaying materials** | | | | | | |
| 1.1 | High-quality sand for construction is required, thoroughly inspected to ensure quality. The sand must be free from impurities such as clay or organic materials and must comply with standard construction specifications | M³ | 10 |  | |  | |
| 1.2 | Ordinary Portland Cement (OPC) is required, with each bag weighing 50 kg and compliant with standard specifications such as ASTM C150 or EN 197-1. | Ton | 2 |  | |  | |
| 1.3 | Concrete block, good quality with dimensions (20\*20\*40) cm | PCS | 1000 |  | |  | |
| 1.4 | PVC door (2\*1) M, good quality | PCS | 3 |  | |  | |
| 1.5 | Electrical concrete mixer, excellent quality, with engine model specifications: GX200, cylinder volume 350 liters, productivity 14 cubic meters per 10 hours, number of wheels 4, mixing speed 30rL/Min, manual and electric rotation system, rated output 6.5 hp | PCS | 1 |  | |  | |
| **2** | **Lot 2: PPE** | | | | | | |
| 2.1 | Work gloves coated with nitrile and made of polyester are required, available in various sizes (S, M, L, XL). The gloves must comply with safety standards such as EN 388 or EN 420. They should be suitable for construction work. | PCS | 75 |  | |  | |
| 2.2 | A roll-up measuring 160×70 cm, designed to be retractable, easy to assemble, and portable. It can be rolled into a metallic or plastic base for convenient storage when not in use. | PCS | 4 |  | |  | |
| **3** | **Lot 3: ELECTRICAL INSTALLATION** | | | | | | |
| 3.1 | LED LAMP 50W (SNOW), good quality with insurance for one year | PCS | 24 |  | |  | |
| 3.2 | LED LAMP 50W (SOLAR), good quality with insurance for one year | PCS | 24 |  | |  | |
| 3.3 | LED LAMP (SECONDARY ROOF )3 STEPS, good quality with insurance one year | PCS | 20 |  | |  | |
| 3.4 | LED LAMP (SECONDARY ROOF )3 STEPS USP | PCS | 25 |  | |  | |
| 3.5 | RIVET GUN, weight 0.4 kg, length 200mm, Made in Japan | PCS | 4 |  | |  | |
| 3.6 | RIVET NAIL 5MM | Box | 3 |  | |  | |
| 3.7 | MATERIAL STORE Metal Locker Storage Cabinet with Doors and Shelves Metal Lockers with four doors and four shelves | PCS | 2 |  | |  | |
| 3.8 | MATERIAL STORE Metal Locker Storage Cabinet with Doors and Shelves Metal Lockers with 2 doors and 3 shelves | PCS | 2 |  | |  | |
| 3.9 | LED LIGHT PROIJECTOR 300W, outdoor | PCS | 5 |  | |  | |
| 3.10 | CIRCUIT BREARER SWITCH 3PHDSE 250A, Circuit breaker, PowerPacT J, 250A, 3 pole, 600VAC, 50kA, I-Line, Micrologic 3.2S | PCS | 1 |  | |  | |
| 3.11 | CIRCUIT BREARER SWITCH 3PHDSE 160A, Circuit breaker, PowerPact J, 160A, 3 pole, 600VAC, 50kA, I-Line, Micrologic 3.2S | PCS | 1 |  | |  | |
| 3.12 | ELECTRICITY TRAMMEL 25 MM (HEAVY) | PCS | 15 |  | |  | |
| 3.13 | ELECTRICITY TRAMMEL 16 MM (HEAVY) | PCS | 15 |  | |  | |
| 3.14 | Cable 4x25 mm, made of pure copper to ensure excellent electrical conductivity and high quality. | M.L | 35 |  | |  | |
| 3.15 | Round cable 2 × 4 mm, made of pure copper to ensure excellent electrical conductivity and high quality. | M.L | 90 |  | |  | |
| 3.16 | PVC Tray Cable 50\*50MM | PCS | 15 |  | |  | |
| 3.17 | Carpentry screw 2" | Box | 2 |  | |  | |
| 3.18 | CIRCUIT BREAKER SWITCH 3PHDSE 24 circuit | PCS | 2 |  | |  | |
| 3.19 | CIRCUIT BREAKER SWITCH 30 A, Circuit breaker, PowerPact J, 30A, I-Line | PCS | 12 |  | |  | |
| **4** | **Lot 4: Carpentry materials** | | | | | | |
| 4.1 | Plywood (120\*240\*2.5) cm manufactured by multi-layers usually used for frames of doors and furniture | PCS | 10 |  | |  | |
| 4.2 | Nails for carpentry work 2.5 inch | KG | 5 |  | |  | |
| 4.3 | Cutter for steel bars for carpenter | PCS | 1 |  | |  | |
| **5** | **Lot 5: IT & Furniture** | | | | | | |
| 5.1 | Rotated chair, leather and Metallic chrome, - with a double lifting pump on the right to move up and down and one on the left to move front and back, supported by a metal backrest | PCS | 2 |  | |  | |
| 5.2 | desks with dimensions of 120 x 100 x 90 cm. Desk Width with 3-drawer | PCS | 1 |  | |  | |
| 5.3 | HP LaserJet Tank MFP 2606sdw, Wireless, Print, Copy, Scan, 40-Sheet ADF, Hi-Speed USB 2.0, Ethernet, Bluetooth LE, up to 22 ppm, 250-sheet Input Tray, 1-Year Warranty, Black and White | PCS | 1 |  | |  | |
| 5.4 | Printing certificates for trainees according to the selection criteria for the coordinator of TVET | PCS | 150 |  | |  | |
| **TOTAL PRICE DAP** | | | | |  |  | |

|  |
| --- |
| NAME: |
| TITLE: |
| STAMP AND SIGNATURE |
| DATE: [Insert submission date] |