**RFQ Price List Word Format / GP 600242**

**Annex 1**

**TABLE 1: Offer to Supply Goods Compliant with Technical Specifications and Requirements**

***(This Form must be submitted only using the Supplier’s Official Letterhead/Stationery[[1]](#footnote-1))***

We, the undersigned, hereby accept in full the UNDP General Terms and Conditions, and hereby offer to supply the items listed below in conformity with the specification and requirements of UNDP as per RFQ Reference No. 600242:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | |
|
| **LOT** | **#** | **Item/ Description** | **Unit** | **Quantity per batch** | **Specifications** | **Unit Price** | **Total** |
|
|  | 1 | Tactical Vest with shot-proof shoulders and arm protection | Unit | 200 | Material: Mesh Fabric  Weight: Min 1.8kg/pc  shoulders and arm protection:  Detachable  can protect against shot and rubber bullet  Protector armor fixed and connected by solid nails  The vest should be adjustable and fixed by elastic belt. |  |  |
| 2 | Anti-Riot Shield | Unit | 200 | Material: transparent polycarbonate with Eva foam padding  Light transmittance: 84%  Feature: anti-riot, anti-stab ,  The grip connection strength: >500N  Arm belt connection strength: >500N |  |  |
| 3 | Baton | Unit | 200 | Material: pp  Length: Min 590mm  Length of grip: Min 125mm  Diameter: Min 30mm  weight: Min 0.41kg |  |  |
| 4 | Gas Mask with Canister | Unit | 200 | Cyanogen chloride life: ≮50 minutes at 30L/min, 1.5mg/L and 80%-80% RH conditions.  Hydrocyanic acid life: ≮50 minutes at 30L/min, 3mg/L.  Oil mist penetration coefficient: ≯0.005 at 30L/min.  Inhalation resistance: ≯ 200 pa at 30L/min.  Exhalation resistance: ≯ 100 pa at 30L/min.  Visual field: total ≮ 75%, binocular visual field ≮60%.  Weight: weight of a complete set of gas mask approx. 840g.  Storage life: 5 years. |  |  |
| 5 | Anti-Riot Helmet with shot-proof neck protection | Unit | 200 | Material: PC  The thickness of the visor: about 3 mm  Weight: about 1.7kg /piece  Neck protector: protect against shot and rubber bullet |  |  |
| 6 | Leg protection with shot-proof shin | Unit | 200 | Colour: Black.  Weight (a pair): min 1200 g.  Knee Protection:  Rigid Nylon armour plate; Leather exterior;  Terylene Oxford cloth interior; Inner padding.  Shin Protection: protect against shot and rubber bullet.  Foot Protection: Rigid Nylon armour plates on upper foot  and both sides; Leather exterior and interior; Inner padding |  |  |
|  | 7 | Third party pre-shipment/ Delivery inspection |  | - |  |  |  |
| **Additional FCA Costs** | | | | |  |  |  |
| **Total Final and All-Inclusive Price Quotation** | | | | |  |  |  |

**TABLE 2: Offer to Comply with Other Conditions and Related Requirements**

|  |  |  |  |
| --- | --- | --- | --- |
| **Other Information pertaining to our Quotation are as follows :** | **Your Responses** | | |
| ***Yes, we will comply*** | ***No, we cannot comply*** | ***If you cannot comply, pls. indicate counter proposal*** |
| Delivery Lead Time |  |  |  |
| Estimated weight/volume/dimension of the Consignment: | Please indicate: | | |
| Validity of Quotation |  |  |  |
| All Provisions of the UNDP General Terms and Conditions |  |  |  |
| Other requirements *[pls. specify]* |  |  |  |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.

*[Name and Signature of the Supplier’s Authorized Person]*

*[Designation]*

*[Date]*

1. *Official Letterhead/Stationery must indicate contact details – addresses, email, phone and fax numbers – for verification purposes*  [↑](#footnote-ref-1)