**CLARIFICATION ON ITB No. UNFPA/TUR/19/001**

MANUFACTURE AND/OR SUPPLY OF SIX (6) MINIBUS VEHICLES

|  |  |
| --- | --- |
| 1.2.10 | Portable or hydraulic wheelchair ramp |

As indicated in the technical specifications, ITEM 1.2.10 is revised as **portable wheelchair ramp** which can be folded or compacted to be carried easily. The length of the ramp should be incompliance with the entrance height of the vehicle, it should not be too steep. When the ramp is folded it should fit in the backside or an appropriate section of the vehicle. The material of the ramp should be anti-slip composite or aluminum.

The objective of having a ramp in the vehicle is to make sure that the beneficiary who uses a wheelchair to enter the vehicle without any additional support. The personnel of the vehicle will help the beneficiary to locate/sit in the vehicle without the wheelchair. After the beneficiary sits in the vehicle, the ramp and the wheelchair will be folded and put aside while the vehicle is moving.