**ANNEX 3**

**TECHNICAL AND COMMERCIAL BID FORM**

*Detailed address of the supplier:*

**The following tables should be completed by the Supplier:**

**Ref.: ITB N° 39-2010 – 3: Supply of Pedestrian Rollers for QUIEP Project in Sierra Leone**

**Date :** ……………………….

**Closing Date:**  20 Sept. 2010 (16:00 CET) **Reply Via: sealed mail**

**Ship-to country** : Sierra Leone **Mode of Transport: ………..**

**Delivery Term :** CIF Freetown **(INCOTERMS 2000)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Your Bid Reference** | **Date** | **Bid Validity Date** | **Currency** |
|  |  |  |  |
| **Total Amount**  **EXW** | **Place of Collection** | **Delivery Time**  **(In Calendar Days*)*** | **Total Weight, Kg &**  **Total Volume, M3** |
|  |  |  |  |
| **Total Amount**  **FCA (port of shipment)** | **Place of Collection** | **Delivery Time**  **(In Calendar Days*)*** | **Total Weight, Kg &**  **Total Volume, M3** |
|  |  |  |  |
| **Total Amount**  **CIF Freetown**  **(Sierra Leone)** | **Place of Collection** | **Delivery Time[[1]](#footnote-1)**  **(In Calendar Days*)*** | **Total Weight, Kg &**  **Total Volume, M3** |
|  |  |  |  |

The undersigned hereby certifies that the Bidder’s company (both parent company and/or any subsidiaries):

* is not identified on, or associated with any company or individual identified on, the list established pursuant to UN Security Council resolution 1267 (1999) (found at website [www.un.org/sc/committees/1267/consolist.shtml](http://www.un.org/sc/committees/1267/consolist.shtml));
* is not the subject of any form of sanction imposed by an organization or body within the United Nations System, including the World Bank.

**Responsible for sale: Signature:**

This Quotation has been prepared in accordance with

**“ILO Terms and Conditions for the Purchase of Goods”**

**ANNEX 3**

**TECHNICAL AND COMMERCIAL BID FORM**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **No** | **Item** | **UOM** | **QTY** | **Preferred**  **Delivery Date** | **Proposed**  **Delivery Time**  **(Calendar days)** | **Weight kg/**  **Volume m3** | Currency | Unit Price | **Total Price** |
| **1** | **Walk-behind Roller** | **Each** | **12** | End of 2010 |  |  |  |  |  |
| **2** | **Fast moving spares kits for one year** | **Each** | **12** | End of 2010 |  |  |  |  |  |
| ***Optional:*** | | | | | | | | | |
| **3** | **Training for operating**  **the equipment on-site** | **Amount** | **1** | End of 2010 |  |  |  |  |  |

Bidders are required to complete the following with “Yes”, “No” or specific information requested for the items being supplied. **Answers such as “see specifications attached” are unacceptable. Your bid may be considered non-compliant unless all questions are answered throughly. Bidders are NOT allowed to make any change in the “Our minimum requirements” columns of the comparative data tables below. Such changes might disqualify your bid.**

Bidders shall include with their bid any other pertinent information that the ILO should know in order to evaluate the bid properly.

**Requested Specifications for the Supply of Walk-behind Twin Drum Vibrating Rollers for QUIEP Project in Sierra Leone:**

| **Our minimum requirements** | **Your offer** *(please fill in)* | |
| --- | --- | --- |
| **Requested Specifications** | **Yes /No** | **Description of the proposed equipment** |
| **Engine:**   * Both drum driving, gravity sprinkler system mechanical drive; * Minimum vibrating power 30KN * Diesel, water or air cooled, automated & manual start, rated output minimum 5kw (ISO9249) continuous rating at manufacturer’s speed.   (*Please provide us with a copy of the ISO 9249 certification).* |  |  |
| **Weight and dimension:**   * Smooth drum, minimum working width 900mm, 2 scrapers fitted to each drum; * Minimum weight 1200kg. |  |  |
| **Exciter and brake system**   * Mechanical drive, with brakes capable of holding the machine safely on 30% grades. |  |  |
| **Fast moving spares for the requested numbers of rollers for one year**  (oil/fuel filters etc) |  |  |
| **Warranty period**   * Minimum 12 months. |  |  |
| **Spare parts availability**   * Minimum 5 (five) years |  |  |
| **Documentation: English Language**   * For each roller, one copy of: * Maintenance and Operation Manual, * Parts Book, * Workshop Book. |  |  |
| **OPTIONAL** |  |  |
| **Local representative for maintance and after-sales services**   * The supplier should have local representation in Sierra Leone or at least in West Africa and should provide after sales service (please provide detailed address and contact name). |  |  |
| **Training for operating the equipment on-site**   * Required language of the training: English; * Number of participants: 14 trainees; * Location of the training: Makeni, Bombali district (Sierra Leone); * Material to be provided during the training: Practical training + reference booklet/sheet. |  |  |

|  |
| --- |
| Please provide at least three references for similar size and type of equipment undertaken by the company (please provide Names **and E-mails of references**); |
|  |

1. Please note that the minimum warranty period required is 12 months. [↑](#footnote-ref-1)