**Section II: Schedule of Requirements**

**Technical specifications for Goods and Comparative Data Table:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item No** | **UNOPS minimum technical requirements** | **Quantity** | **Is quotation compliant?** Bidder to complete | **Details of goods offered.** Bidder to complete |
| 1 | **Blast Proof Film for Office of the Regional Director, Asia Region** | 143 sqm | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
|  | **Specification:** | **Please note that simply checking the “Yes” box does not satisfy the compliant requirement. Details should be included in the last column as well.** | | |
|  | Certificate testing: ASTM F1642, ANSI Z97.1, 16 CFR CPSC 1201, GSA TS01-2003, ISO 16933, EN 12600, or equivalent |  | ☐ Yes ☐ No | Insert details of goods offered |
|  | Film Thickness: minimum 0.15 mm |  | ☐ Yes ☐ No | Insert details of goods offered |
|  | Construction: micro layered |  | ☐ Yes ☐ No | Insert details of goods offered |
|  | Tear resistance: minimum 1,000 lbs% |  | ☐ Yes ☐ No | Insert details of goods offered |
|  | Tensile strength: 32,000 psi (220 MPa) |  | ☐ Yes ☐ No | Insert details of goods offered |
|  | Break Strength: minimum 210 lbs/in (934 N/22 mm) |  | ☐ Yes ☐ No | Insert details of goods offered |
|  | Peel strength > 8 lbs/in (36 N/25 mm) |  | ☐ Yes ☐ No | Insert details of goods offered |

**Detail window information (Detail Picture in Separate Attachments)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Reference** | **Type** | **Units(s)** | **Width (cm)** | **Height (cm)** |
| A | Black Metal Frame Windows | 6 | 166.5 | 146.8 |
| B1 | Grey Aluminum Frame Windows (upper part) | 40 | 113.2 | 190 |
| B2 | Grey Aluminum Frame Windows (lower part) | 40 | 113.2 | 56 |
| C1 | Grey Aluminum Frame Windows (upper part) | 2 | 58 | 190 |
| C2 | Grey Aluminum Frame Windows (lower part) | 2 | 58 | 56 |
| D1 | Grey Aluminum Frame Windows (upper part) | 2 | 58 | 190 |
| D2 | Grey Aluminum Frame Windows (lower part) | 2 | 58 | 56 |
| E1 | Grey Aluminum Frame Windows (upper part) | 1 | 95 | 190 |
| E2 | Grey Aluminum Frame Windows (lower part) | 1 | 95 | 56 |
| F1 | Grey Aluminum Frame Windows (upper part) | 1 | 37 | 190 |
| F2 | Grey Aluminum Frame Windows (lower part) | 1 | 37 | 56 |
| G1 | Grey Aluminum Frame Windows (upper part) | 4 | 73.5 | 190 |
| G2 | Grey Aluminum Frame Windows (lower part) | 4 | 73.5 | 56 |
| TOTAL | | **106** |  |  |

**Delivery requirements and Comparative Data Table:**

|  |  |  |  |
| --- | --- | --- | --- |
| **UNOPS Requirements** | | **Is quotation compliant?** Bidder to complete | **Details**  Bidder to complete |
| **Delivery time** | Bidder shall deliver the goods within 2 weeks or 31 December 2020, whichever comes first. | ☐ Yes ☐ No | Insert details |
| **Delivery place and Incoterms rules** | DAP Bangkok. | ☐ Yes ☐ No | Insert details |
| **Consignee details** | Will be shared after contract signature | ☐ Yes ☐ No | Insert details |
| **UNOPS Right to vary requirements** | At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- 20%, without any change in the unit prices or other terms and conditions of the RFQ. | ☐ Yes ☐ No | Insert details |