**Technical Proposal Form**

**ITB reference no: LITB 2021-9164590**

**Subject: Procurement of** **SMIS Server and Accessories for Data Centre**

**Annexure – B**

**Self-technical compliance to be filled by the Bidder.**

|  |  |  |  |
| --- | --- | --- | --- |
| **A** | **B** | **C** | **D** |
| **LITB.**  **No.** | **Item Description** | **Please indicate**  **Specifications offered conform to the requirement / do not conform (Yes/no)** | **Deviation in case 'No' in column ‘C’**  **(mention briefly)** |
| 10 | Next Generation Firewall - 2 Nos  Threat prevention subscription for devices in HA pair year 1 - 2 Nos  Wildfire subscription for devices in HA pair year 1 - 2 Nos  Global Protect subscription for devices in HA pair year 1 - 2 Nos  Partner enabled premium support year 1 - 2 Nos  Power cord for Continental Europe with IEC-60320 C13 and CEE 7/7 SCHUKO cord ends,10A, 250V max, 6ft - 2 Nos  Warranty/License: 1 Year |  |  |
| 20 | Load Balancer and Web Application Firewall - 1 No.  24x7 Standard Bundle Contract includes:  Firmware and General Upgrades, 24x7 Support, WAF Security Service, & IP Reputation Service  Application Delivery Controller - virtual appliance for all supported platforms. Supports up to 2x vCPU cores. - 1 No.  Three Years \_ Standard Bundle (24x7 IP Reputation and WAF Security Service) - 1 No.  Warranty/License: 3 Years |  |  |
| 30 | Physical Server: 2 Nos.  Chassis: 2.5 Chassis with up to 8 Hard Drives and 3PCle slots  CPU: Intel Xeon Silver 4210R 2.4G, 10C/20T, 9.6GT/s, 13.75 Cache, Turbo, HT (100W) DDR4-2400  2nd CPU: Intel Xeon Silver 4210R 2.4G, 10C/20T, 9.6GT/s, 13.75M  Cache, Turbo, HT (100W) DDR4-2400  Memory: 128GB (4×32GB RDIMM, 3200MT/s, Dual Rank)  Hard Disk: 2Nos × 240 GB SSD SATA Mix Use 6Gbps 512 2.5in  Raid: No RAID  Raid Ctrl: PERC H330 RAID Controller, Minicard  Network: Broadcom 57412 Dual Port 10GbE SFP+ & 5720 Dual Port 1GbE  BASE-T rNDC  Optical Drive: DVD +/-RW, SATA, Internal  Power Supply: Dual, Hot-plug, Redundant Power Supply (1+1), 750W  Rack Rail: ReadyRails Sliding Rails with Cable Management Arm  O/S: 4 x WinSvrSTDCore 2019 OLP 2Lic NL Gov CoreLic (License)    Trusted Platform Module 2.0  Warranty/License 3 Years |  |  |
| 40 | Storage Server: 1 No.  SYSTEM 10 x 2.4 TB HDD 10K SAS 512n 2.5in Hot-plug Hard Drive  CNC 8 Port Dual Controller for iSCSI SFP+ and/or FC  8 x SFP+ SR Optic 10GbE 850nm  2 x Jumper Cord - C13/C14, 4M, 250V, 10A (US, EU, TW, APCC countries except ANZ)  Warranty/License 3 Years |  |  |
| 50 | 10G Switch: 2 Nos  Switch 1U, PHY-less, 28 x 10GbE SFP+, 2 x QSFP28, IO to PSU, 2 PSU, OS10  QSFP+ to QSFP+, 40GbE Passive Copper Direct Attach Cable, 1 Meter  12 x Networking, Transceiver, SFP+,16Gbps Fibre Channel, SWL, 850nm, LC Duplex  2 x Jumper Cord - C13/C14, 2M, 250V, 10A (EU, TW, APCC countries except ANZ)  12 x Networking Cable, OM4 LC/LC Fiber Cable, (Optics required), 5 Meter  Warranty/License: 3 Years |  |  |
| 60 | Vmware Essentials Plus Kit  VMware vSphere 7 Essentials Plus Kit for 3 hosts  (Max 2 processors per host) - 1 No.  Production Support/Subscription VMware vSphere 7  Essentials Plus Kit for 3 year - 1 No.  Warranty/License: 3 Years |  |  |
| 70 | E-Mail Solution with 3 Year License (Warranty/License: 3 Year) |  |  |
| 80 | Cables and Other accessories required for fully functional unit.  (please mention list detail in Column C) |  |  |
| 90 | SFP Module (Compatible 1000BASE-LX/LH SFP 1310nm 10km) - 8 Nos. |  |  |
|  | Quality assurance and compliance certificate to be submitted with the offer. |  |  |
|  | Please mention address/details of Service Centers in Myanmar |  |  |
|  | # Bidders should provide detailed technical specifications and brochures of the offered model along with this bid for each item |  |  |
| **Note: Offers without technical and financial template i.e. Annexure B & C will not be considered.** | | | |

Signature **……………………………………………….**

Authorized official (name) **……………………………………………….**

Name of the Vendor **……………………………………………….**

Date **……………………………………………….**