**Section II: Schedule of Requirements**

**eSourcing reference:** **RFQ/2021/18687**

**Technical specifications for Goods and Comparative Data Table:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item No** | **UNOPS minimum technical requirements** | **Quantity** | **Is quotation compliant?** Bidder to complete | **Details of goods offered.** Bidder to complete |
| **LOT 1: HAZARD LABELING AND SEALING TOOLS** | | | | |
| 1 | Sealing Pliers Set Security Lead Seal for Lead Diameter 10mm | **5** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 2 | 4000 x 10mm security lead seals and seal wires for use by sealing pliers | **4,000** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 3 | White Paint Pens (for rock painting, waterproof/permanent) | **40** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 4 | Rolls (in a roll of 1,000) x Class 1 Explosive 1 Hazard Warning Diamond Label – Code J001 | **3** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 5 | Rolls (in a roll of 1,000) x Class 1 Explosive 1.1 Hazard Warning Diamond Label – Code J001/1.1 | **2** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 6 | Rolls (in a roll of 1,000) x Class 1 Explosive 1.4S Hazard Warning Diamond Label – Code J011 | **2** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 7 | Rolls (in a roll of 1,000) x Class 1 Explosive 1.4G Hazard Warning Diamond Label – Code J010 | **2** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| **LOT 2: HAZARDOUS LIQUID HANDLING SAFETY KITS** | | | | |
| 1 | **3 H1/Y rated 4 x 5 litre jerry can kits for shipping hazardous liquids**  Specifications:-   * Per unit includes 4 x 5 litre U.N. and IATA rated jerry cans for group II/III (Y/Z) liquids * Box is to be double walled with partition to safely store 4x 5 litre HDPE jerry cans * Box is to have orientation marking on min 2 sides   **5 litre jerry can specifications**   * 5 Litre HDPE jerry can with Tamper Evident Cap for hazardous liquids * 100% high density polyethylene (HDPE) * UN International and IATA rating tested and safe to transport hazardous materials and dangerous goods by land, air and sea. | **40** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 2 | **Rotary Drum Pump – Manual**   * FM approved for Class I and II flammable and combustible liquids * To fit 15-55 gallon container * Flow rate min 10 gal/min | **1** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 3 | **Full Face Organic Vapour Respirator (reusable)**  Silicone face piece and seal  Polycarbonate lense  Threaded cartridge connector  Size - 3 x Medium and 3 x Large | **6** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 4 | **Organic Vapour Filters**   * To fit Full face organic vapour * Reusable respirator | **18** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 5 | **Chemical Resistant Bib Apron**   * Tie at waist | **6** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |
| 6 | **Chemical Resistant latex gloves**   * Tear resistant * Anti-corrosive for use with chemicals * Flexible to wear * Sizes - 6 x medium / 6 x large / 6 x extra large | **20** | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable |

**Delivery requirements and Comparative Data Table:**

|  |  |  |  |
| --- | --- | --- | --- |
| **UNOPS Requirements** | | **Is quotation compliant?** Bidder to complete | **Details**  Bidder to complete |
| **Delivery time** | Bidder shall deliver the goods **within 4 weeks** after Contract signature. | ☐ Yes ☐ No | Insert details |
| **Delivery place and Incoterms rules** | CPT Entebbe (Incoterms 2010) | ☐ Yes ☐ No | Insert details |
| **Consignee details** | ESO Logistics. E-mail: ESOSupplychain@unops.org | ☐ Yes ☐ No | Insert details |
| **UNOPS Right to vary requirements** | At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- 20%, without any change in the unit prices or other terms and conditions of the RFQ. | ☐ Yes ☐ No | Insert details |

**00**

**: +45 45 33 75 0**