**Section II: Schedule of Requirements**

**eSourcing reference:** ITB/2021/21294

**1. Objective:** UNOPS is soliciting quotations for the establishment of a Long Term Agreement as defined in this tender. Quotations must be submitted by using the Requirement and Price List contained in the attachments ‘Section II: Schedule of Requirements’ and ‘Section III: Returnable Bidding Forms’. The overall objective of this solicitation is to establish a Long Term Agreement (LTA) to facilitate and expedite the process by which UNOPS will contract the supply of **Hook and Line Kits** once there are specific requirements in the 3 years following the signature of the LTA.

**2. Number of LTAs and non-exclusivity:** UNOPS will enter into an LTA agreement with one or multiple suppliers selected as a result of this procurement process as per evaluation methodology and criteria specified herein. The LTA shall be considered by UNOPS as non-exclusive and UNOPS will not be committed to purchase any minimum quantity.

**3. Call Off Order and prices:** Once the LTA is signed, if there is a specific requirement for **Hook and Line Kits,** the UNOPS appointed focal person shall issue a release Purchase Order (PO) to the supplier. The PO will include details on the type and number of items to be printed and other practical details. The pricing will be based on prices in the LTA contract as quoted in this ITB.

**4. Contract Management/Service Level Agreement:** The LTA supplier shall provide quarterly reports to the UNOPS focal point indicated in the LTA. UNOPS will regularly monitor the performance of the LTA supplier, based on the following Key Performance Indicators (KPIs):

* KPI 1: On-time delivery. Supplier shall deliver within maximum **30 working days** after receipt of the release of the PO.
* KPI 2: Completeness of the order, error free goods. Supplier shall deliver goods or services as per description/model included in the release order and at the right quantity.
* KPI 3: Price Compliance. Supplier shall supply goods as per unit prices identified in the LTA
* KPI 4: Accuracy of payment documentation. Supplier shall provide complete payment documentation including accurate invoices with correct quantities, unit price, order reference number, etc

If the supplier fails to meet UNOPS’ performance requirements detailed above, it will receive in the first instance a warning to improve their performance. Continued failure to meet performance requirements may result in termination of the LTA.

1. **Summary of Requirements**

UNOPS requirements are comprised of the following lots:

* Lot 1: Hook and line system – Large
* Lot 2: Hook and line system – lite
* Lot 3: Hook and line system – backpack
* Lot 4: Hook and line system – tactical kit
* Lot 5: Hook and line system – access kit
* Lot 6: Hook and line system – building kit
* Lot 7: Hook and line system – vehicle kit
* Lot 8: Hook and line system – tripod kit

1. **Technical specifications for Goods and Comparative Data Table**

**Technical specifications for Goods and Comparative Data Table for Lot 1:** **Hook and Line System – Large**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UNOPS minimum technical requirements** | | | **Is a Bid compliant? Bidder to complete** | **Details of goods offered. Bidder to complete** |
| **Lot** | **Contents minimum or equivalent to:** | **Minimum Qty** |
| 1 | **Description**  Large Hook & Line kit for IEDD and EOD tasks. Set stored in a heavy duty case. Corrosion-Resistant | | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable – **Important : Vendors shall provide relevant technical brochure to facilitate evaluation** |
| 1.1 | 3 Function Door Wedge | 2 | ☐ Yes ☐ No | Insert |
| 1.2 | Allen Grip (Heavy Duty Cantilever Jaw) | 2 | ☐ Yes ☐ No | Insert |
| 1.3 | Bar Clamp Anchor | 1 | ☐ Yes ☐ No | Insert |
| 1.4 | Bar Extension Anchor | 1 | ☐ Yes ☐ No | Insert |
| 1.5 | Belt Sling, 80mm (Width) | 1 | ☐ Yes ☐ No | Insert |
| 1.6 | Heavy Duty Telescopic Pole | 1 | ☐ Yes ☐ No | Insert |
| 1.7 | Hook Holder | 1 | ☐ Yes ☐ No | Insert |
| 1.8 | Hook Setter | 1 | ☐ Yes ☐ No | Insert |
| 1.9 | Hook, 25mm ID | 2 | ☐ Yes ☐ No | Insert |
| 1.10 | Hook, 50mm ID | 2 | ☐ Yes ☐ No | Insert |
| 1.11 | Hook, 50mm ID, 19mm GAP | 1 | ☐ Yes ☐ No | Insert |
| 1.12 | Hook, Double | 2 | ☐ Yes ☐ No | Insert |
| 1.13 | Hook, S | 1 | ☐ Yes ☐ No | Insert |
| 1.14 | Hook, SL 50mm ID | 1 | ☐ Yes ☐ No | Insert |
| 1.15 | Karabiner, Locking Gate (Large) | 4 | ☐ Yes ☐ No | Insert |
| 1.16 | Karabiner, Straight Gate (Small) | 4 | ☐ Yes ☐ No | Insert |
| 1.17 | Large Wedge | 2 | ☐ Yes ☐ No | Insert |
| 1.18 | Lightweight Spring Grip | 2 | ☐ Yes ☐ No | Insert |
| 1.19 | Line Branch with Clamp | 1 | ☐ Yes ☐ No | Insert |
| 1.20 | Line Puller | 2 | ☐ Yes ☐ No | Insert |
| 1.21 | Line, Black, minimum 100m | 1 | ☐ Yes ☐ No | Insert |
| 1.22 | Line, White, minimum 100m | 1 | ☐ Yes ☐ No | Insert |
| 1.23 | Modular Clamp, STD Tips | 1 | ☐ Yes ☐ No | Insert |
| 1.24 | Needle Nose Arm, Clamp | 2 | ☐ Yes ☐ No | Insert |
| 1.25 | Piton Anchor | 6 | ☐ Yes ☐ No | Insert |
| 1.26 | Pocket Search Mirror | 1 | ☐ Yes ☐ No | Insert |
| 1.27 | Reel Assembly | 2 | ☐ Yes ☐ No | Insert |
| 1.28 | Reel Bag | 2 | ☐ Yes ☐ No | Insert |
| 1.29 | Rope Loop, 450mm | 2 | ☐ Yes ☐ No | Insert |
| 1.30 | Rope Loop, 900mm | 2 | ☐ Yes ☐ No | Insert |
| 1.31 | Rope Sling, 3mm, 2m | 2 | ☐ Yes ☐ No | Insert |
| 1.32 | Rubber Door Wedge | 4 | ☐ Yes ☐ No | Insert |
| 1.33 | Screw Eye | 10 | ☐ Yes ☐ No | Insert |
| 1.34 | Seizers, (150mm minimum ) | 1 | ☐ Yes ☐ No | Insert |
| 1.35 | Seizers, Large (160mm minimum ) | 1 | ☐ Yes ☐ No | Insert |
| 1.36 | Self-Adhesive Anchor Pad | 10 | ☐ Yes ☐ No | Insert |
| 1.37 | Self-Opening Snatch Block/Pulley | 4 | ☐ Yes ☐ No | Insert |
| 1.38 | Serrated Arm, Clamp | 2 | ☐ Yes ☐ No | Insert |
| 1.39 | Shackle, D-Shaped | 1 | ☐ Yes ☐ No | Insert |
| 1.40 | Shock Cord, 10mm, 0.5m | 2 | ☐ Yes ☐ No | Insert |
| 1.41 | Shock Cord, 10mm, 1m | 2 | ☐ Yes ☐ No | Insert |
| 1.42 | Single Suction Anchor | 2 | ☐ Yes ☐ No | Insert |
| 1.43 | Sling Webbing, Long | 1 | ☐ Yes ☐ No | Insert |
| 1.44 | Sling Webbing, Short | 1 | ☐ Yes ☐ No | Insert |
| 1.45 | Snatch Block, One-Way Lock | 1 | ☐ Yes ☐ No | Insert |
| 1.46 | Heavy duty case with Foam | 1 | ☐ Yes ☐ No | Insert |
| 1.47 | Splitter Ball | 2 | ☐ Yes ☐ No | Insert |
| 1.48 | Suction Cup Bridge (Large) | 1 | ☐ Yes ☐ No | Insert |
| 1.49 | Suction Cup Bridge (Medium) | 1 | ☐ Yes ☐ No | Insert |
| 1.50 | Suction Cup Bridge (Small) | 1 | ☐ Yes ☐ No | Insert |
| 1.51 | Wide Pad, Clamp | 2 | ☐ Yes ☐ No | Insert |
| 1.52 | Wire Sling, 3mm, 0.9m | 1 | ☐ Yes ☐ No | Insert |
| 1.53 | Wire Sling, 3mm, 1.8m | 1 | ☐ Yes ☐ No | Insert |
| 1.54 | User Manual | 1 | ☐ Yes ☐ No | Insert |

**Technical specifications for Goods and Comparative Data Table for Lot 2:** **Hook and Line System – Lite**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UNOPS minimum technical requirements** | | | **Is a Bid compliant? Bidder to complete** | **Details of goods offered. Bidder to complete** |
| **Lot** | **Contents minimum or equivalent to:** | **Minimum Qty** |
| 2 | **Description**  Lite Hook & Line kit for IEDD and EOD tasks. Set stored in a heavy duty case. Corrosion-Resistant | | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable – **Important : Vendors shall provide relevant technical brochure to facilitate evaluation** |
| 2.1 | 3 Function Door Wedge | 1 | ☐ Yes ☐ No | Insert |
| 2.2 | Allen Grip (Heavy Duty Cantilever Jaw) | 1 | ☐ Yes ☐ No | Insert |
| 2.3 | Collapsible Pole with Pouch | 1 | ☐ Yes ☐ No | Insert |
| 2.4 | Hook Setter | 1 | ☐ Yes ☐ No | Insert |
| 2.5 | Hook, 25mm ID | 2 | ☐ Yes ☐ No | Insert |
| 2.6 | Hook, 50mm ID | 2 | ☐ Yes ☐ No | Insert |
| 2.7 | Hook, 50mm ID, 19mm GAP | 1 | ☐ Yes ☐ No | Insert |
| 2.8 | Hook, Double | 2 | ☐ Yes ☐ No | Insert |
| 2.9 | Hook, S | 1 | ☐ Yes ☐ No | Insert |
| 2.10 | Hook, SL 50mm ID | 1 | ☐ Yes ☐ No | Insert |
| 2.11 | Karabiner, Locking Gate (Large) | 2 | ☐ Yes ☐ No | Insert |
| 2.12 | Karabiner, Straight Gate (Small) | 2 | ☐ Yes ☐ No | Insert |
| 2.13 | Large Wedge | 1 | ☐ Yes ☐ No | Insert |
| 2.14 | Lightweight Spring Grip | 1 | ☐ Yes ☐ No | Insert |
| 2.15 | Line Puller | 1 | ☐ Yes ☐ No | Insert |
| 2.16 | Line, White, Minimum 100m | 1 | ☐ Yes ☐ No | Insert |
| 2.17 | Modular Clamp, STD Tips | 1 | ☐ Yes ☐ No | Insert |
| 2.18 | Needle Nose Arm, Clamp | 2 | ☐ Yes ☐ No | Insert |
| 2.19 | Piton Anchor | 6 | ☐ Yes ☐ No | Insert |
| 2.20 | Pocket Search Mirror | 1 | ☐ Yes ☐ No | Insert |
| 2.21 | Reel Assembly | 1 | ☐ Yes ☐ No | Insert |
| 2.22 | Reel Bag | 1 | ☐ Yes ☐ No | Insert |
| 2.23 | Rope Loop, 450mm | 2 | ☐ Yes ☐ No | Insert |
| 2.24 | Rope Loop, 900mm | 2 | ☐ Yes ☐ No | Insert |
| 2.25 | Rope Sling, 3mm, 2m | 2 | ☐ Yes ☐ No | Insert |
| 2.26 | Rubber Door Wedge | 2 | ☐ Yes ☐ No | Insert |
| 2.27 | Seizers, (150mm) | 1 | ☐ Yes ☐ No | Insert |
| 2.28 | Self-Adhesive Anchor Pad | 10 | ☐ Yes ☐ No | Insert |
| 2.29 | Self-Opening Snatch Block/Pulley | 2 | ☐ Yes ☐ No | Insert |
| 2.30 | Serrated Arm, Clamp | 2 | ☐ Yes ☐ No | Insert |
| 2.31 | Shock Cord, 10mm, 1m | 1 | ☐ Yes ☐ No | Insert |
| 2.32 | Single Suction Anchor | 2 | ☐ Yes ☐ No | Insert |
| 2.33 | Sling Webbing, Short | 1 | ☐ Yes ☐ No | Insert |
| 2.34 | Heavy duty case with Foam | 1 | ☐ Yes ☐ No | Insert |
| 2.35 | Splitter Ball | 2 | ☐ Yes ☐ No | Insert |
| 2.36 | Suction Cup Bridge (Medium) | 1 | ☐ Yes ☐ No | Insert |
| 2.37 | Wide Pad, Clamp | 2 | ☐ Yes ☐ No | Insert |
| 2.38 | Wire Sling, 3mm, 0.9m | 1 | ☐ Yes ☐ No | Insert |
| 2.39 | User Manual | 1 | ☐ Yes ☐ No | Insert |

**Technical specifications for Goods and Comparative Data Table for Lot 3: Hook and Line System – Backpack**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UNOPS minimum technical requirements** | | | **Is a Bid compliant? Bidder to complete** | **Details of goods offered. Bidder to complete** |
| **Lot** | **Contents minimum or equivalent to:** | **Minimum Qty** |
| 3 | **Description**  Hook & Line for IEDD and EOD tasks. Set stored in a heavy duty backpack. Corrosion-Resistant | | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable – **Important : Vendors shall provide relevant technical brochure to facilitate evaluation** |
| 3.1 | 3 Function Door Wedge | 2 | ☐ Yes ☐ No | Insert |
| 3.2 | Allen Grip (Heavy Duty Cantilever Jaw) | 1 | ☐ Yes ☐ No | Insert |
| 3.3 | Collapsible Pole with Pouch | 1 | ☐ Yes ☐ No | Insert |
| 3.4 | Multi-purpose Clamp | 1 | ☐ Yes ☐ No | Insert |
| 3.5 | Heavy duty Backpack | 1 | ☐ Yes ☐ No | Insert |
| 3.6 | Hook Setter | 1 | ☐ Yes ☐ No | Insert |
| 3.7 | Hook, 25mm ID | 2 | ☐ Yes ☐ No | Insert |
| 3.8 | Hook, 50mm ID | 2 | ☐ Yes ☐ No | Insert |
| 3.9 | Hook, Double | 2 | ☐ Yes ☐ No | Insert |
| 3.10 | Hook, SL 50mm ID | 1 | ☐ Yes ☐ No | Insert |
| 3.11 | Karabiner, Locking Gate (Large) | 3 | ☐ Yes ☐ No | Insert |
| 3.12 | Karabiner, Straight Gate (Small) | 3 | ☐ Yes ☐ No | Insert |
| 3.13 | Lightweight Spring Grip | 1 | ☐ Yes ☐ No | Insert |
| 3.14 | Line Branch with Clamp | 1 | ☐ Yes ☐ No | Insert |
| 3.15 | Line Puller | 1 | ☐ Yes ☐ No | Insert |
| 3.16 | Main Line | 1 | ☐ Yes ☐ No | Insert |
| 3.17 | Modular Clamp, STD Tips | 1 | ☐ Yes ☐ No | Insert |
| 3.18 | Needle Nose Arm, Clamp | 2 | ☐ Yes ☐ No | Insert |
| 3.19 | Piton Anchor | 4 | ☐ Yes ☐ No | Insert |
| 3.20 | Pocket Search Mirror | 1 | ☐ Yes ☐ No | Insert |
| 3.21 | Lightweight Reel | 1 | ☐ Yes ☐ No | Insert |
| 3.22 | Rope Loop, 450mm | 2 | ☐ Yes ☐ No | Insert |
| 3.23 | Rope Loop, 900mm | 2 | ☐ Yes ☐ No | Insert |
| 3.24 | Rope Sling, 3mm, 2m | 2 | ☐ Yes ☐ No | Insert |
| 3.25 | Rubber Door Wedge | 2 | ☐ Yes ☐ No | Insert |
| 3.26 | Screw Eye | 6 | ☐ Yes ☐ No | Insert |
| 3.27 | Secondary Line | 1 | ☐ Yes ☐ No | Insert |
| 3.28 | Seizers, Large (160mm) | 2 | ☐ Yes ☐ No | Insert |
| 3.29 | Self-Adhesive Anchor Pad | 10 | ☐ Yes ☐ No | Insert |
| 3.30 | Self-Opening Snatch Block/Pulley | 4 | ☐ Yes ☐ No | Insert |
| 3.31 | Serrated Arm, Clamp | 2 | ☐ Yes ☐ No | Insert |
| 3.32 | Shackle, D-Shaped | 1 | ☐ Yes ☐ No | Insert |
| 3.33 | Shock Cord, 10mm, 1m | 2 | ☐ Yes ☐ No | Insert |
| 3.34 | Single Suction Anchor | 2 | ☐ Yes ☐ No | Insert |
| 3.35 | Sling Webbing, Short | 1 | ☐ Yes ☐ No | Insert |
| 3.36 | Splitter Ball | 2 | ☐ Yes ☐ No | Insert |
| 3.37 | Suction Cup Bridge (Medium) | 1 | ☐ Yes ☐ No | Insert |
| 3.38 | Wall Stopper | 2 | ☐ Yes ☐ No | Insert |
| 3.39 | Wide Pad, Clamp | 2 | ☐ Yes ☐ No | Insert |
| 3.40 | Wire Sling, 3mm, 0.9m | 1 | ☐ Yes ☐ No | Insert |
| 3.41 | Wire Sling, 3mm, 1.8m | 1 | ☐ Yes ☐ No | Insert |
| 3.42 | User Manual | 1 | ☐ Yes ☐ No | Insert |

**Technical specifications for Goods and Comparative Data Table for Lot 4: Hook and Line System – Tactical Kit**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UNOPS minimum technical requirements** | | | **Is a Bid compliant? Bidder to complete** | **Details of goods offered. Bidder to complete** |
| **Lot** | **Contents minimum or equivalent to:** | **Minimum Qty** |
| 4 | **Description**  Lightweight Hook & Line for IEDD and EOD tactical tasks. Set stored in modular leg pouches. Corrosion-Resistant | | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable – **Important : Vendors shall provide relevant technical brochure to facilitate evaluation** |
| 4.1 | Line module | 1 | ☐ Yes ☐ No | Insert |
| 4.2 | Clamp module | 1 | ☐ Yes ☐ No | Insert |
| 4.3 | Anchor module | 1 | ☐ Yes ☐ No | Insert |
| 4.4 | Multi tool module | 1 | ☐ Yes ☐ No | Insert |
| 4.5 | Grappling hook module | 1 | ☐ Yes ☐ No | Insert |
| 4.6 | Heavy duty leg pouch | 1 | ☐ Yes ☐ No | Insert |
| 4.7 | User Manual | 1 | ☐ Yes ☐ No | Insert |

**Technical specifications for Goods and Comparative Data Table for Lot 5: Hook and Line System – Access Kit**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UNOPS minimum technical requirements** | | | **Is a Bid compliant? Bidder to complete** | **Details of goods offered. Bidder to complete** |
| **Lot** | **Contents minimum or equivalent to:** | **Minimum Qty** |
| 5 | **Description** Access Hook & Line for IEDD and EOD tasks. Set stored in a heavy duty case. Corrosion-Resistant | | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable – **Important : Vendors shall provide relevant technical brochure to facilitate evaluation** |
| 5.1 | Finger Pull Actuator | 1 | ☐ Yes ☐ No | Insert |
| 5..2 | 3 Function Door Wedge | 1 | ☐ Yes ☐ No | Insert |
| 5.3 | Handle/Grip Lifter | 1 | ☐ Yes ☐ No | Insert |
| 5.4 | Push Button Actuator | 1 | ☐ Yes ☐ No | Insert |
| 5.5 | Door Knob Turner | 1 | ☐ Yes ☐ No | Insert |
| 5.6 | Door Lever Lifter | 1 | ☐ Yes ☐ No | Insert |
| 5.7 | Spring Clamp, C1 | 1 | ☐ Yes ☐ No | Insert |
| 5.8 | Spring Clamp, C2 | 1 | ☐ Yes ☐ No | Insert |
| 5.9 | Spring Clamp, C3 | 1 | ☐ Yes ☐ No | Insert |
| 5.10 | Spring Clamp, C4 | 1 | ☐ Yes ☐ No | Insert |
| 5.11 | Spring Clamp, C5 | 1 | ☐ Yes ☐ No | Insert |
| 5.12 | Spring Clamp, C6 | 1 | ☐ Yes ☐ No | Insert |
| 5.13 | Spring Clamp, C7 | 1 | ☐ Yes ☐ No | Insert |
| 5.14 | Spring Clamp, C8 | 1 | ☐ Yes ☐ No | Insert |
| 5.15 | Spring Clamp, C9 | 1 | ☐ Yes ☐ No | Insert |
| 5.16 | Interior Hood Release | 1 | ☐ Yes ☐ No | Insert |
| 5.17 | Clamp Screw, Long | 6 | ☐ Yes ☐ No | Insert |
| 5.18 | Clamp Screw, Short | 2 | ☐ Yes ☐ No | Insert |
| 5.19 | Clamp Screw, Short | 1 | ☐ Yes ☐ No | Insert |
| 5.20 | Heavy duty case with Foam | 1 | ☐ Yes ☐ No | Insert |
| 5.21 | User Manual | 1 | ☐ Yes ☐ No | Insert |

**Technical specifications for Goods and Comparative Data Table for Lot 6: Hook and Line System – Building Kit**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UNOPS minimum technical requirements** | | | **Is a Bid compliant? Bidder to complete** | **Details of goods offered. Bidder to complete** |
| **Lot** | **Contents minimum or equivalent to:** | **Minimum Qty** |
| 6 | **Description**  Building Access Hook & Line for IEDD and EOD tasks. Set stored in a heavy duty case or heavy-duty backpack. Corrosion-Resistant | | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable – **Important : Vendors shall provide relevant technical brochure to facilitate evaluation** |
| 6.1 | Remote door opener | 1 | ☐ Yes ☐ No | Insert |
| 6.2 | Doorway anchor | 1 | ☐ Yes ☐ No | Insert |
| 6.3 | Multi-purpose anchor | 1 | ☐ Yes ☐ No | Insert |
| 6.4 | Door hinge anchor | 2 | ☐ Yes ☐ No | Insert |
| 6.5 | Key/handle clamp | 1 | ☐ Yes ☐ No | Insert |
| 6.6 | Heavy duty case with Foam or heavy-duty backpack | 1 | ☐ Yes ☐ No | Insert |
| 6.7 | User Manual | 1 | ☐ Yes ☐ No | Insert |

**Technical specifications for Goods and Comparative Data Table for Lot 7: Hook and Line System – Vehicle Kit**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UNOPS minimum technical requirements** | | | **Is a Bid compliant? Bidder to complete** | **Details of goods offered. Bidder to complete** |
| **Lot** | **Contents minimum or equivalent to:** | **Minimum Qty** |
| 7 | **Description**  Vehicle Access Hook & Line kit for IEDD and EOD tasks. Set stored in a heavy duty case or heavy-duty backpack. Corrosion-Resistant | | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable – **Important : Vendors shall provide relevant technical brochure to facilitate evaluation** |
| 7.1 | Engine compartment tool | 1 | ☐ Yes ☐ No | Insert |
| 7.2 | Window breaker | 1 | ☐ Yes ☐ No | Insert |
| 7.3 | hand break release | 1 | ☐ Yes ☐ No | Insert |
| 7.4 | Hood release hook set | 1 | ☐ Yes ☐ No | Insert |
| 7.5 | key turner | 1 | ☐ Yes ☐ No | Insert |
| 7.6 | Push button actuator | 1 | ☐ Yes ☐ No | Insert |
| 7.7 | Single suction Anchor Pad | 1 | ☐ Yes ☐ No | Insert |
| 7.8 | Self-Adhesive Anchor Pad | 1 | ☐ Yes ☐ No | Insert |
| 7.9 | Suction Cup bridge | 1 | ☐ Yes ☐ No | Insert |
| 7.10 | Spring clam C5 | 1 | ☐ Yes ☐ No | Insert |
| 7.11 | Spring clam C7 | 1 | ☐ Yes ☐ No | Insert |
| 7.12 | Heavy duty case with Foam or heavy-duty backpack | 1 | ☐ Yes ☐ No | Insert |
| 7.13 | Shock Cord, 10mm, 1m | 1 | ☐ Yes ☐ No | Insert |
| 7.14 | Rope sling, 3mm, 2 m | 1 | ☐ Yes ☐ No | Insert |
| 7.15 | Shock Cord, 10mm, 0.5 m | 1 | ☐ Yes ☐ No | Insert |
| 7.16 | User Manual | 1 | ☐ Yes ☐ No | Insert |

**Technical specifications for Goods and Comparative Data Table for Lot 8: Hook and Line System – Tripod Kit**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UNOPS minimum technical requirements** | | | **Is a Bid compliant? Bidder to complete** | **Details of goods offered. Bidder to complete** |
| **Lot** | **Contents minimum or equivalent to:** | **Minimum Qty** |
| 8 | **Description**  Lightweight tripod kit for IEDD and EOD tasks. Set stored in a heavy duty case or heavy-duty backpack. Corrosion-Resistant | | ☐ Yes ☐ No | Insert details of goods offered, including specifications and brand/model offered if applicable - **Important : Vendors shall provide relevant technical brochure to facilitate evaluation** |
| 8.1 | Lightweight tripod - able to lift a minimum of 80 kg | 1 | ☐ Yes ☐ No | Insert |
| 8.2 | Double snatch block pulley | 1 | ☐ Yes ☐ No | Insert |
| 8.3 | Auxiliary snatch block pulley | 1 | ☐ Yes ☐ No | Insert |
| 8.4 | Locking pins for tripod legs | 6 | ☐ Yes ☐ No | Insert |
| 8.5 | Bracing line | 3 | ☐ Yes ☐ No | Insert |
| 8.6 | Adjuster plate, bracing line | 3 | ☐ Yes ☐ No | Insert |
| 8.7 | Anchor peg, straight | 6 | ☐ Yes ☐ No | Insert |
| 8.8 | Anchor peg, serrated | 3 | ☐ Yes ☐ No | Insert |
| 8.9 | Heavy duty case with Foam or heavy-duty backpack | 1 | ☐ Yes ☐ No | Insert |
| 8.10 | User Manual | 1 | ☐ Yes ☐ No | Insert |

1. **Delivery requirements and Comparative Data Table:**

|  |  |  |  |
| --- | --- | --- | --- |
| **UNOPS Requirements** | | **Is bid compliant?** Bidder to complete | **Details**  Bidder to complete |
| **Delivery time** | Bidder shall deliver the goods 4-6 weeks after Contract signature. | ☐ Yes ☐ No | Insert details |
| **Delivery place and Incoterms rules** | Incoterms: FCA (Incoterm 2010) point(s) of delivery for offered products (Please enter the complete address) | ☐ Yes ☐ No | Insert details |
| **Consignee details** | Supplier is able to export Products to at least 20/28 locations. See below list: | ☐ Yes ☐ No | Insert details |
| **UNOPS Right to vary requirements** | At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- 20%, without any change in the unit prices or other terms and conditions of the ITB. | ☐ Yes ☐ No | Insert details |

**Delivery requirements and Comparative Data Table:**

UNOPS - Peace and Security Cluster is operating in the following countries. Bidders must be able to facilitate export to at least 20 out of 28 of the following locations.

1. Abyei 10. Iraq 19. Sudan, Darfur
2. Algeria 11. Lebanon 20. Sudan, Khartoum
3. Afghanistan 12. Libya 21. South Sudan
4. Burkina Faso 13. Mali 22. Syria
5. Cambodia 14. Myanmar 23. Tunisia
6. Central African Republic 15. Nepal 24. Turkey
7. Cyprus 16. Nigeria 25. Uganda
8. Colombia 17. Israel 26. Western Sahara
9. Democratic Republic of Congo (DRC) 18. Somalia 27. Yemen

28. USA – PSC New York Office