**Section II: Schedule of Requirements**

E-Sourcing reference: RFQ/2021/19995

1. **Summary of Requirements for Light and Sound Bars.**

**Supply and installation of Light and Sound Bars for Forensic laboratory vehicles of the National Police of Ukraine as further described in the Table B. Technical Specification for Goods and comparative data table**

1. **Technical specifications for Goods and Comparative Data Tables**

| **N** | **UNOPS minimum technical requirements** | **Is quotation compliant?** Bidder to complete | **Details of goods offered.**  Bidder to complete |
| --- | --- | --- | --- |
|  | **General technical requirements for Light and Sound Bars** |  |  |
| 1 | Control of light and sound signals on the microphone SGU (Signal loud-speaker setup (SGU), speakers) | ☐ Yes ☐ No | Insert details |
| 2 | SGU | ☐ Yes ☐ No | Insert details |
| 2.1 | SGU (Signal loud-speaker) is located inside the light bar | ☐ Yes ☐ No | Insert details |
| 2.2 | SGU power: 140-150 W output | ☐ Yes ☐ No | Insert details |
| 3 | 4 types of siren: WAIL, YELP, HI-LO, AIRHORN | ☐ Yes ☐ No | Insert details |
| 4 | 5 operating modes | ☐ Yes ☐ No | Insert details |
| 5 | Number of LEDs - 84 pcs. | ☐ Yes ☐ No | Insert details |
| 6 | Voltage: 12V or 24V | ☐ Yes ☐ No | Insert details |
| 7 | Light panel color: blue / blue | ☐ Yes ☐ No | Insert details |
| 8 | Dimensions: Length not less than 1180 mm and not more than 1200 mm | ☐ Yes ☐ No | Insert details |
| 9 | Width: not less than 240 mm and not more than 250 mm | ☐ Yes ☐ No | Insert details |
| 10 | Height: not less than 45 mm. and not more than 50 mm | ☐ Yes ☐ No | Insert details |
| 11 | Compatibility requirements: to be installed on the RENAULT TRAFIC L2H1 vehicle | ☐ Yes ☐ No | Insert details |
| 12 | Services on installation and connection of the equipment on RENAULT TRAFIC L2H1 vehicle at the End User’s site - Service Center of the National Police of Ukraine (27 Svyatoshynska Street, Kyiv, Ukraine). | ☐ Yes ☐ No | Insert details |
| 13 | **The period of validity of the Warranty.** The warranty shall remain valid for twelve (12) months after the Goods, or any portion thereof as the case may be, have been delivered to and accepted at the final destination. The Warranty should include corrective maintenance, replacement of defective parts/equipment, repair of equipment, labour for equipment repair and/or parts replacement. | ☐ Yes ☐ No | Insert details |
| 14 | **Warranty service.** Within the warranty period, the Supplier or its authorized service centre shall provide maintenance and/or repair services and/or replacement of the equipment not later than 30 (thirty) calendar days from the date of receipt of written or E-mail notification from an authorized party. The name of the company, address, telephone- and fax numbers, e-mail address must be mentioned in the bid. All costs connected with warranty maintenance are covered by the Supplier. | ☐ Yes ☐ No | Insert details |
| 15 | **Bid includes brand/model of the equipment and manufacturer's technical literature/catalogue, all confirming that the offered items comply with required specifications. A picture/photo of the equipment needs to be submitted as a separate file if not already included in the manufacturer's technical literature/catalogue.** | ☐ Yes ☐ No | Insert details |

**C. Delivery requirements and Comparative Data Table**

| **UNOPS Requirements** | | **Is bid compliant?** Bidder to complete | **Details**  Bidder to complete |
| --- | --- | --- | --- |
| **Delivery time** | Bidder shall deliver the goods within **two months** after Contract signature. | ☐ Yes ☐ No | Insert details |
| **Delivery place and Incoterms rules** | DAP Customs cleared, Kyiv, Ukraine +  offloading of goods at final destination | ☐ Yes ☐ No | Insert details |
| **Consignee details** | UNOPS,  Service Center of the National Police of Ukraine (27, Svyatoshynska Street, Kyiv, Ukraine) | ☐ Yes ☐ No | Insert details |
| **Acceptance** | Bidder shall remain liable for consistency of the items supplied for the period of shipment and acceptance for use. Any items found unacceptable shall be returned and changed at no costs to UNOPS. | ☐ Yes ☐ No | Insert details |
| **Packing standards** | Bidder shall ensure the best international packing standards of goods supplied, including use of eco-friendly packing materials. | ☐ Yes ☐ No | Insert details |

**D. Sustainability Considerations**

| **UNOPS Requirements** | | **Is bid compliant?** Bidder to complete | **Details**  Bidder to complete |
| --- | --- | --- | --- |
| **Sustainability Requirements - Sustainable Packaging** | In accordance with the UN’s efforts to eliminate single use plastics from its operations, bidders are required to avoid any unnecessary packaging and/or to consider more sustainable alternatives which include but are not limited to using biodegradable or recycled packaging, recyclable packaging, offering a packaging take-back option, packaging in bulk or other means | ☐ Yes ☐ No | Insert details |
| **Sustainability Requirements - Supplier commitment to gender equality** | The bidder shall provide a response that demonstrates its commitment to support gender equality and women’s empowerment through its operations. The bidder must provide a clear statement and supporting documentation that outlines how gender is mainstreamed internally. This should include for example the organization's current or future plans/activities with regards to:  - gender diversity in the recruitment process (such as outreach to potential diverse candidates and equitable, non-biased interview practices)  - ensuring equal pay between men and women for the same roles by providing pay gap analysis or pay stubs  - opportunities for females to be empowered and promoted internally (e.g. mentorship, leadership/ management skills training for both junior and senior employees),  - prevention of sexual exploitation and abuse or any form of discrimination at work (e.g. zero-tolerance policy in place),  - paid parental leave policies for men and women,  - provide professional safety training and access to equal protection facilities for all staffs without discrimination  - Undertaken and awarded an independent gender audit certificate or equivalent (e.g. Edge Certificate, WEPs GAP analysis). | ☐ Yes ☐ No | Insert details |

**E. Inspections and tests**

The following inspections and tests shall be performed:

(i) The Supplier shall perform all needed tests before the shipment to conform that the goods meet the Purchaser requirements. Documented confirmation of such tests has to be sent to the Purchaser before the shipment;

(ii) The Purchaser may undertake to perform a random check of goods for compliance with specifications, warranty term, etc., before the shipment.

UNOPS or its representative may inspect and/or test any or all items of the goods to confirm their conformity to the contract, prior to dispatch from the supplier’s premises. Such inspection and clearance will not prejudice the right of the consignee to inspect and test the goods on receipt at destination.

If the goods fail to meet the laid down specifications, the supplier shall take immediate steps to remedy the deficiency or replace the defective goods to the satisfaction of the purchaser.