**Section III: Returnable Bidding Forms**

**Note to Bidders:** **Instructions to complete each Form are highlighted in blue in each Form. Please complete the Returnable Bidding Forms as instructed** **and return them as part of your quotation.**

The following returnable forms are part of this RFQ and must be completed and returned by bidders as part of their Quotation.

**Form A: Quotation submission form**

Bidders are requested to complete this form, sign it and return it as part of their bid submission. The bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.

Date: [Insert submission date]

**Subject: Quotation for the supply of** [***Insert a brief description of goods/services*]****in**[***Name of country/city*],** RFQ Case No. [**RFQ/2021/25450**], dated **[insert date]**

We, the undersigned, declare that:

* 1. We offer to supply in conformity with the bidding documents, including the UNOPS General Conditions of Contract;
  2. Our quotation shall be valid for the period of time of [insert number of days which shall not be less than the specified in Section I: RFQ Particulars, Period of Validity of Quotations] from the date fixed for the submission deadline as set out in the RFQ, and it shall remain binding upon us and may be accepted at any time before the expiration of that period;
  3. We have no conflict of interest in any activity that would put it, if selected for this assignment, in a conflict of interest with UNOPS. [If you have any actual or potential conflict of interest as defined in Article 3 of Section II: Instructions to Bidders, please disclose it here];
  4. Our firm confirms that the offeror and sub-contractors have not been associated, or had been involved in any way, directly or indirectly, with the preparation of the design, terms of references and/or other documents used as a part of this solicitation;
  5. Our firm, its affiliates or subsidiaries—including any subcontractors or suppliers for any part of the Contract—has not been declared ineligible by UNOPS, nor is included in the suspended/ineligibility list of the UN/PD, other UN Agencies, the UN Security Council, and the World Bank, in accordance with Instructions to Bidders Article 3, Eligibility;
  6. We embrace the UN Supplier Code of Conduct and adhere to the principles of the UN Global Compact;
  7. We have not declared bankruptcy, are not involved in bankruptcy or receivership proceedings, and there is no judgment or pending legal action against them that could impair their operations in the foreseeable future;
  8. We have not offered and will not offer fees, gifts and/or favours of kind in exchange for this RFQ and will not engage in any such activity during the performance of any Contract awarded.

I, the undersigned, certify that I am duly authorized by [***insert full name of bidder***] to sign this quotation and bind [***insert full name of bidder***] should UNOPS accept this quotation:

Name: [complete]

Title: [complete]

Date: [complete]

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Provide the name and contact information for the primary contact from your company for this quotation:

Name: [complete]

Title: [complete]

Email address: [complete]

Telephone: [complete]

# Form B: Price Schedule Form

Bidders shall fill in this Price Schedule Form in accordance with the instructions indicated.

RFQ reference no: **RFQ/2021/25450**

| **Currency** | USD |
| --- | --- |

| **Lot No** | **Item No** | **Description** | **Qty** | **Unit price -** DDP - **(USD)** | **Total price -** DDP - **(USD)** |
| --- | --- | --- | --- | --- | --- |
|
| 01 | 1 | **Supply, Delivery and Installation of** Dual Channel AIS Receiver (USB and NMEA output) for Philippines | 02 |  |  |
| 2 | **Supply, Delivery and Installation of** Antenna for AIS Coastal Receiver for Philippines | 02 |  |  |
| SUB TOTAL - USD | | | |  |
| 02 | 1 | **Supply, Delivery and Installation of** Dual Channel AIS Receiver (USB and NMEA output) for Cambodia | 02 |  |  |
| 2 | **Supply, Delivery and Installation of** Antenna for AIS Coastal Receiver for Cambodia | 02 |  |  |
| SUB TOTAL - USD | | | |  |
| 03 | 1 | **Supply and Delivery of** Dual Channel AIS Receiver (USB and NMEA output) for Timor Leste | 01 |  |  |
| 2 | **Supply and Delivery of** Antenna for AIS Coastal Receiver for Timor Leste | 01 |  |  |
| SUB TOTAL - USD | | | |  |

**\*\*Note: When pricing for each lot, please consider the DDP delivery location given for each schedule in the delivery schedule**

Payment terms 30 days accepted: ☐ Yes

**Bidder’s discount for accelerated payment:** \_\_\_\_% of total firm price for each calendar day less than thirty (30) days

I, the undersigned, certify that I am duly authorized by [***insert full name of Bidder***] to sign this quotation and bind [***insert full name of Bidder***] should UNOPS accept this quotation:

Name : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Title : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Partial quotations shall not be allowed. Bidders must quote prices for the total goods and/or services for the total requirement requested. Evaluation will be done for the total requirement.*

# Form C: Technical Quotation Form

RFQ reference no: **RFQ/2021/25450**

Name of Bidder: [insert name of Bidder]

Bidders are required to complete the **Comparative Data Tables** included in Section III: Schedule of Requirements to demonstrate compliance with UNOPS requirements and insert them below. Bidders are NOT allowed to make any change in the “UNOPS requirements” columns of the Comparative Data Tables. Such changes might disqualify your quotation.

**Technical specifications for Goods and Comparative Data Table:**

**Lot 01 - Item 01: Supply, Delivery and Installation of Dual Channel AIS Receiver (USB and NMEA output) for Philippines**

| **Lot No.** | **Technical Specification** | **Bidder's Offer** | | **Remarks** |
| --- | --- | --- | --- | --- |
| **Yes.** | **No** |
| 1 | Make | Provide Details | |  |
| 2 | Model | Provide Details | |  |
| 3 | Country of Origin | Provide Details | |  |
| 4 | Dual Parallel AIS Receiver | ☐ Yes | ☐ No |  |
| 5 | Interface/modem to enable connection to PC/Display system | ☐ Yes | ☐ No |  |
| 6 | Power & channel LEDs are available | ☐ Yes | ☐ No |  |
| 7 | USB 2.0 compliant | ☐ Yes | ☐ No |  |
| 8 | Low power consumption | ☐ Yes | ☐ No |  |
| 9 | Compact design with Weight: Max 700g | ☐ Yes | ☐ No |  |
| 10 | USB or 12/24 volts dc powered | ☐ Yes | ☐ No |  |
| 11 | NMEA 0183 VDM output | ☐ Yes | ☐ No |  |
| 12 | Built in NMEA multiplexer | ☐ Yes | ☐ No |  |
| 13 | Should have a built-in AIS viewing programme to display the AIS targets on a screen | ☐ Yes | ☐ No |  |
| 14 | When connected to a PC, it should enable AIS data to be viewed directly or shared on a Local Network | ☐ Yes | ☐ No |  |
| 15 | Mounting: 4 mounting holes in end plates | ☐ Yes | ☐ No |  |
| 16 | Power Supply:12 V dc 3 W nominal (9-30 V dc) | ☐ Yes | ☐ No |  |
| 17 | Operating temp: -15°C to +55°C | ☐ Yes | ☐ No |  |
| 18 | AIS receiver needs to be in compliant with current regulations, IEC standards covering Class A and Class B CS and TDMA AIS and IMO Recommendation on performance standards and Resolutions for guidelines for use and the proof documents should be attached | ☐ Yes | ☐ No |  |
| 19 | The equipment should be covered with a comprehensive “Parts & Labor” warranty for the period of not less than 12 calendar months from the date of successful Installation & commissioning | ☐ Yes | ☐ No |  |
| 20 | User/Technical/Maintenance manuals to be supplied in English | ☐ Yes | ☐ No |  |
| 21 | Installation in Philippines will be handled by the Supplier/ Local agent | ☐ Yes | ☐ No |  |

**Lot 01 - Item 02: Supply, Delivery and Installation of Antenna for AIS Coastal Receiver for Philippines**

| **Lot No.** | **Technical Specification** | **Bidder's Offer** | | **Remarks** |
| --- | --- | --- | --- | --- |
| **Yes.** | **No** |
| 1 | Make | Provide Details | |  |
| 2 | Model | Provide Details | |  |
| 3 | Country of Origin | Provide Details | |  |
| 4 | Should be designed for VHF / AIS Land and Marine Service | ☐ Yes | ☐ No |  |
| 5 | Should facilitate monitoring of AIS sea traffic | ☐ Yes | ☐ No |  |
| 6 | Omnidirectional feature should be enabled | ☐ Yes | ☐ No |  |
| 7 | Material: non-corrosive aluminium | ☐ Yes | ☐ No |  |
| 8 | Should be Rugged and corrosion resistant | ☐ Yes | ☐ No |  |
| 9 | Pole mount bracket should be included | ☐ Yes | ☐ No |  |
| 10 | 10 m or better length cable should be included | ☐ Yes | ☐ No |  |
| 11 | Tunable frequency range of 135 -175 MHz | ☐ Yes | ☐ No |  |
| 12 | Weight: Max 600g | ☐ Yes | ☐ No |  |
| 13 | Should be supplied with centre element length L pre-adjusted for AIS frequencies | ☐ Yes | ☐ No |  |
| 14 | Should be supplied with J-mount antenna bracket for installation | ☐ Yes | ☐ No |  |
| 15 | Must be compatible with the AIS receiver; Covering Class A and Class B CS; | ☐ Yes | ☐ No |  |
| 16 | Comes with all necessary accessories such as power cable | ☐ Yes | ☐ No |  |
| 17 | The equipment should be covered with a comprehensive “Parts & Labor” warranty for the period of not less than 12 calendar months from the date of successful Installation & commissioning | ☐ Yes | ☐ No |  |
| 18 | User/Technical/Maintenance manuals to be supplied in English | ☐ Yes | ☐ No |  |
| 19 | Installation in Philippines will be handled by the Supplier/ Local agent | ☐ Yes | ☐ No |  |

**Lot 02 - Item 01: Supply, Delivery and Installation of Dual Channel AIS Receiver (USB and NMEA output) for Cambodia**

| **Lot No.** | **Technical Specification** | **Bidder's Offer** | | **Remarks** |
| --- | --- | --- | --- | --- |
| **Yes.** | **No** |
| 1 | Make | Provide Details | |  |
| 2 | Model | Provide Details | |  |
| 3 | Country of Origin | Provide Details | |  |
| 4 | Dual Parallel AIS Receiver | ☐ Yes | ☐ No |  |
| 5 | Interface/modem to enable connection to PC/Display system | ☐ Yes | ☐ No |  |
| 6 | Power & channel LEDs are available | ☐ Yes | ☐ No |  |
| 7 | USB 2.0 compliant | ☐ Yes | ☐ No |  |
| 8 | Low power consumption | ☐ Yes | ☐ No |  |
| 9 | Compact design with Weight: Max 700g | ☐ Yes | ☐ No |  |
| 10 | USB or 12/24 volts dc powered | ☐ Yes | ☐ No |  |
| 11 | NMEA 0183 VDM output | ☐ Yes | ☐ No |  |
| 12 | Built in NMEA multiplexer | ☐ Yes | ☐ No |  |
| 13 | Should have a built-in AIS viewing programme to display the AIS targets on a screen | ☐ Yes | ☐ No |  |
| 14 | When connected to a PC, it should enable AIS data to be viewed directly or shared on a Local Network | ☐ Yes | ☐ No |  |
| 15 | Mounting: 4 mounting holes in end plates | ☐ Yes | ☐ No |  |
| 16 | Power Supply:12 V dc 3 W nominal (9-30 V dc) | ☐ Yes | ☐ No |  |
| 17 | Operating temp: -15°C to +55°C | ☐ Yes | ☐ No |  |
| 18 | AIS receiver needs to be in compliant with current regulations, IEC standards covering Class A and Class B CS and TDMA AIS and IMO Recommendation on performance standards and Resolutions for guidelines for use and the proof documents should be attached | ☐ Yes | ☐ No |  |
| 19 | The equipment should be covered with a comprehensive “Parts & Labor” warranty for the period of not less than 12 calendar months from the date of successful Installation & commissioning | ☐ Yes | ☐ No |  |
| 20 | User/Technical/Maintenance manuals to be supplied in English | ☐ Yes | ☐ No |  |
| 21 | Installation in Cambodia will be handled by the Supplier/ Local agent | ☐ Yes | ☐ No |  |

**Lot 02 - Item 02: Supply, Delivery and Installation of Antenna for AIS Coastal Receiver for Cambodia**

| **Lot No.** | **Technical Specification** | **Bidder's Offer** | | **Remarks** |
| --- | --- | --- | --- | --- |
| **Yes.** | **No** |
| 1 | Make | Provide Details | |  |
| 2 | Model | Provide Details | |  |
| 3 | Country of Origin | Provide Details | |  |
| 4 | Should be designed for VHF / AIS Land and Marine Service | ☐ Yes | ☐ No |  |
| 5 | Should facilitate monitoring of AIS sea traffic | ☐ Yes | ☐ No |  |
| 6 | Omnidirectional feature should be enabled | ☐ Yes | ☐ No |  |
| 7 | Material: non-corrosive aluminium | ☐ Yes | ☐ No |  |
| 8 | Should be Rugged and corrosion resistant | ☐ Yes | ☐ No |  |
| 9 | Pole mount bracket should be included | ☐ Yes | ☐ No |  |
| 10 | 10 m or better length cable should be included | ☐ Yes | ☐ No |  |
| 11 | Tunable frequency range of 135 -175 MHz | ☐ Yes | ☐ No |  |
| 12 | Weight: Max 600g | ☐ Yes | ☐ No |  |
| 13 | Should be supplied with centre element length L pre-adjusted for AIS frequencies | ☐ Yes | ☐ No |  |
| 14 | Should be supplied with J-mount antenna bracket for installation | ☐ Yes | ☐ No |  |
| 15 | Must be compatible with the AIS receiver; Covering Class A and Class B CS; | ☐ Yes | ☐ No |  |
| 16 | Comes with all necessary accessories such as power cable | ☐ Yes | ☐ No |  |
| 17 | The equipment should be covered with a comprehensive “Parts & Labor” warranty for the period of not less than 12 calendar months from the date of successful Installation & commissioning | ☐ Yes | ☐ No |  |
| 18 | User/Technical/Maintenance manuals to be supplied in English | ☐ Yes | ☐ No |  |
| 19 | Installation in Cambodia will be handled by the Supplier/ Local agent | ☐ Yes | ☐ No |  |

**Lot 03 - Item 01: Supply, Delivery and Installation of Dual Channel AIS Receiver (USB and NMEA output) for Timor Leste**

| **Lot No.** | **Technical Specification** | **Bidder's Offer** | | **Remarks** |
| --- | --- | --- | --- | --- |
| **Yes.** | **No** |
| 1 | Make | Provide Details | |  |
| 2 | Model | Provide Details | |  |
| 3 | Country of Origin | Provide Details | |  |
| 4 | Dual Parallel AIS Receiver | ☐ Yes | ☐ No |  |
| 5 | Interface/modem to enable connection to PC/Display system | ☐ Yes | ☐ No |  |
| 6 | Power & channel LEDs are available | ☐ Yes | ☐ No |  |
| 7 | USB 2.0 compliant | ☐ Yes | ☐ No |  |
| 8 | Low power consumption | ☐ Yes | ☐ No |  |
| 9 | Compact design with Weight: Max 700g | ☐ Yes | ☐ No |  |
| 10 | USB or 12/24 volts dc powered | ☐ Yes | ☐ No |  |
| 11 | NMEA 0183 VDM output | ☐ Yes | ☐ No |  |
| 12 | Built in NMEA multiplexer | ☐ Yes | ☐ No |  |
| 13 | Should have a built-in AIS viewing programme to display the AIS targets on a screen | ☐ Yes | ☐ No |  |
| 14 | When connected to a PC, it should enable AIS data to be viewed directly or shared on a Local Network | ☐ Yes | ☐ No |  |
| 15 | Mounting: 4 mounting holes in end plates | ☐ Yes | ☐ No |  |
| 16 | Power Supply:12 V dc 3 W nominal (9-30 V dc) | ☐ Yes | ☐ No |  |
| 17 | Operating temp: -15°C to +55°C | ☐ Yes | ☐ No |  |
| 18 | AIS receiver needs to be in compliant with current regulations, IEC standards covering Class A and Class B CS and TDMA AIS and IMO Recommendation on performance standards and Resolutions for guidelines for use and the proof documents should be attached | ☐ Yes | ☐ No |  |
| 19 | The equipment should be covered with a comprehensive “Parts & Labor” warranty for the period of not less than 12 calendar months from the date of successful Installation & commissioning | ☐ Yes | ☐ No |  |
| 20 | User/Technical/Maintenance manuals to be supplied in English | ☐ Yes | ☐ No |  |

**Lot 03 - Item 02: Supply, Delivery and Installation of Antenna for AIS Coastal Receiver for Timor Leste**

| **Lot No.** | **Technical Specification** | **Bidder's Offer** | | **Remarks** |
| --- | --- | --- | --- | --- |
| **Yes.** | **No** |
| 1 | Make | Provide Details | |  |
| 2 | Model | Provide Details | |  |
| 3 | Country of Origin | Provide Details | |  |
| 4 | Should be designed for VHF / AIS Land and Marine Service | ☐ Yes | ☐ No |  |
| 5 | Should facilitate monitoring of AIS sea traffic | ☐ Yes | ☐ No |  |
| 6 | Omnidirectional feature should be enabled | ☐ Yes | ☐ No |  |
| 7 | Material: non-corrosive aluminium | ☐ Yes | ☐ No |  |
| 8 | Should be Rugged and corrosion resistant | ☐ Yes | ☐ No |  |
| 9 | Pole mount bracket should be included | ☐ Yes | ☐ No |  |
| 10 | 10 m or better length cable should be included | ☐ Yes | ☐ No |  |
| 11 | Tunable frequency range of 135 -175 MHz | ☐ Yes | ☐ No |  |
| 12 | Weight: Max 600g | ☐ Yes | ☐ No |  |
| 13 | Should be supplied with centre element length L pre-adjusted for AIS frequencies | ☐ Yes | ☐ No |  |
| 14 | Should be supplied with J-mount antenna bracket for installation | ☐ Yes | ☐ No |  |
| 15 | Must be compatible with the AIS receiver; Covering Class A and Class B CS; | ☐ Yes | ☐ No |  |
| 16 | Comes with all necessary accessories such as power cable | ☐ Yes | ☐ No |  |
| 17 | The equipment should be covered with a comprehensive “Parts & Labor” warranty for the period of not less than 12 calendar months from the date of successful Installation & commissioning | ☐ Yes | ☐ No |  |
| 18 | User/Technical/Maintenance manuals to be supplied in English | ☐ Yes | ☐ No |  |

**Delivery requirements and Comparative Data Table:**

| **UNOPS Requirements** | | **Is quotation compliant?** Bidder to complete | **Details**  Bidder to complete |
| --- | --- | --- | --- |
| **Delivery time** | **Lot No 01 - Item No 01:** Dual Channel AIS Receiver (USB and NMEA output) for Philippines - Bidder shall deliver the goods as soon as possible but not later than **45** calendar days after the Contract signature for DDP | ☐ Yes ☐ No | Insert details |
| **Lot No 01 - Item No 02:** Antenna for AIS Coastal Receiver for Philippines - Bidder shall deliver the goods as soon as possible but not later than **45** calendar days after the Contract signature for DDP | ☐ Yes ☐ No | Insert details |
| **Lot No 02 - Item No 01:** Dual Channel AIS Receiver (USB and NMEA output) for Cambodia - Bidder shall deliver the goods as soon as possible but not later than **45** calendar days after the Contract signature for DDP | ☐ Yes ☐ No | Insert details |
| **Lot No 02 - Item No 02:** Antenna for AIS Coastal Receiver for Cambodia - Bidder shall deliver the goods as soon as possible but not later than **45** calendar days after the Contract signature for DDP | ☐ Yes ☐ No | Insert details |
| **Lot No 03 - Item No 01:** Dual Channel AIS Receiver (USB and NMEA output) for Timor Leste - Bidder shall deliver the goods as soon as possible but not later than **45** calendar days after the Contract signature for DDP | ☐ Yes ☐ No | Insert details |
| **Lot No 03 - Item No 02:** Antenna for AIS Coastal Receiver for Timor Leste - Bidder shall deliver the goods as soon as possible but not later than **45** calendar days after the Contract signature for DDP | ☐ Yes ☐ No | Insert details |
| **Delivery place and Incoterms rules** | **Lot 01 - Item 01 & 02 :** DDP, National Coast Watch Center, 139 25th Street, South Harbor, 1018 Manila, Philippines  Incoterms: DDP (Bidders shall offer their bid prices, including all taxes, duties, customs clearance cost, and VAT payable by the Contractor shall be included in the price.) | ☐ Yes ☐ No | Insert details |
| **Lot 02 -**  **01 No of Dual Channel AIS Receiver plus 01 No of Antenna for AIS Coastal Receiver:** Preap Island, Group 11, Village #3, Sangkat #1, Sihanouk City, Sihanouk Province, Postal Code: 18201, Cambodia  Incoterms: DDP (Bidders shall offer their bid prices, including all taxes, duties, customs clearance cost, and VAT payable by the Contractor shall be included in the price.) | ☐ Yes ☐ No | Insert details |
| **Lot 02 -**  **01 No of Dual Channel AIS Receiver plus 01 No of Antenna for AIS Coastal Receiver:** Street Tomnub Koh Preab, -Village 3, Sangkat 1, Preah Sihanouk town, Preah Sihanouk Province, Cambodia  Incoterms: DDP (Bidders shall offer their bid prices, including all taxes, duties, customs clearance cost, and VAT payable by the Contractor shall be included in the price.) | ☐ Yes ☐ No | Insert details |
| **Lot 03 - Item 01 & 02 :** DDP, Timor Leste Maritime Police (UPM) Operations Centre, Quarter UPM, Rua Largo Lecider, Dili, Timor Leste  Incoterms: DDP (Bidders shall offer their bid prices, including all taxes, duties, customs clearance cost, and VAT payable by the Contractor shall be included in the price.) | ☐ Yes ☐ No | Insert details |
| **Consignee details** | **Lot 01:** National Coast Watch Center, 139 25th Street, South Harbor, 1018 Manila, Philippines | ☐ Yes ☐ No | Insert details |
| **Lot No 02:**  **01 No of Dual Channel AIS Receiver plus 01 No of Antenna for AIS Coastal Receiver:** National Committee for Maritime Security, Cambodia (NCMS) | ☐ Yes ☐ No | Insert details |
| **Lot No 02:**  **01 No of Dual Channel AIS Receiver plus 01 No of Antenna for AIS Coastal Receiver:** Cambodian National Police (CNP) | ☐ Yes ☐ No | Insert details |
| **Lot 03:** Timor Leste Maritime Police (UPM) Operations Centre, Quarter UPM, Rua Largo Lecider, Dili, Timor Leste | ☐ Yes ☐ No | Insert details |

**Delivery requirements and Comparative Data Table:**

# Form D: Previous experience form

RFQ reference no: **RFQ/2021/25450**

Name of Bidder: [insert name of Bidder]

| **Description of services/goods** | **Country** | **Total amount of Contract** | **Contract Identification and Title and**  **Contact details of Client**  **(Name, Address, telephone, email, fax)** | **Year project was undertaken** |
| --- | --- | --- | --- | --- |
| Insert the details here | Insert the details here | Insert the details here | Insert the details here | Insert the details here |
| Insert the details here | Insert the details here | Insert the details here | Insert the details here | Insert the details here |
| Insert the details here | Insert the details here | Insert the details here | Insert the details here | Insert the details here |

**NOTE: Please list minimum 1 of completed order details during the last 12 months(UN/ Government / Non Government/ Private Sector, etc).**

Name : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Title : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**75 00ax: +45 45 33 75 01**