## **ANNEX 3: TECHNICAL AND FINANCIAL OFFER - GOODS**

*Bidders are requested to complete this form, sign it and return it as part of their bid along with Annex 2: Quotation Submission Form. The Bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.*

|  |  |  |
| --- | --- | --- |
| Name of Bidder: | Click or tap here to enter text. | |
| RFQ reference: | RFQMUS2022-001 | Date: Click or tap to enter a date. |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Currency of the Quotation:** Click or tap here to enter text.  **INCOTERMS:** Click or tap here to enter text. | | | | | | |
| **Item No** | **Description** | **UOM** | **Qty for 1 set** | **Projected Quantities of FADs\*** | **Unit price (USD)** | **Total price (USD)** |
| **LOT 1 – Supply of Materials for mooring line (Long Term Agreement)** | | | | | | |
| 1.1 | Chain - Galvanised and interlinked, diameter 12mm |  | 20 m | **15 Sets\*** |  |  |
| 1.2 | Rope polyamide - Diameter 18mm, 3 strands twist right hand lay |  | 1 coil of 200 m |  |  |
| 1.3 | Rope polypropylene - diameter 20mm, 3 strands twist right hand lay |  | 10 coils of 200 m each |  |  |
| 1.4 | Shackles - Galvanized, diameter 12mm |  | 4 |  |  |
| 1.5 | Shackles - Galvanized, diameter 16mm |  | 6 |  |  |
| 1.6 | Thimble - Galvanized, diameter 18mm |  | 4 |  |  |
| 1.7 | Thimble - Galvanized, diameter 12mm |  | 4 |  |  |
| 1.8 | Swivel - Galvanized, diameter 18mm |  | 5 |  |  |
| 1.9 | Self-adhesive retro reflective tape - Width 50mm, Class B with honeycomb structure.  Colors: Red, Silver or Fluo |  | Roll of 3 m |  |  |
| 1.10 | Strap bands Brown/black/dark blue colour |  | 1 coil of 25 m |  |  |
| 1.11 | Mixed-wire rope (nylon-type intertwined with steel) diameter 14mm |  | 100 m |  |  |
| 1.12 | Zinc anode 1 to 1.5kg |  | 3 |  |  |
| **Subtotal for LOT 1** | | | | |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Currency of the Quotation:** Click or tap here to enter text.  **INCOTERMS:** Click or tap here to enter text. | | | | | | |
| **Item No** | **Description** | **UOM** | **Qty for 1 set** | **Projected Quantities of FADs\*** | **Unit price (USD)** | **Total price (USD)** |
| **LOT 2 – Supply of Satellite buoy tracking/ biomass sensor and associated satellite tracking software (Long Term Agreement)** | | | | | | |
| **2.1** | **Satellite buoy tracking / biomass sensor as per following specifications** |  | **1** | **15 sets\*** |  |  |
| The satellite buoy tracking/ biomass sensor should be:   * Capable of producing pings on a regular basis * Able to detect the aggregation of biomass down to a depth of at least 300m beneath the FAD * Able to capture and transmit data such as GPS position, temperature, sea surface temperature and diurnal migration of biomass * Compatible with cartography of Eastern Africa * Impact and abrasion resistant * Fitted with an echo sounder for accurate biomass determination * Able to distinguish big from small fish (eco filtering, species/size discrimination) * Able to estimate biomass volume * Capable of detecting fish shoal behaviour |
| **2.2** | **Relevant downloading and processing software compatible with the above Satellite buoy tracking / biomass sensor** |  | **1 (One-off Item)** | |  |  |
| **2.3** | **Relevant training to at least five (5) Officers from the MoBEMRFS and the Rodrigues Regional Assembly about downloading and processing software compatible with satellite buoy tracking/ biomass sensor** |  | **At least 5 (One-off Item)** | |  |  |
|  | **Subtotal for LOT 2** | | | | |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Currency of the Quotation:** Click or tap here to enter text.  **INCOTERMS:** Click or tap here to enter text. | | | | | | | | | | | | | |
| **Item No** | | **Description** | | **UOM** | | **Qty for 1 set** | **Projected Quantities of FADs\*** | | **Unit price (USD)** | | **Total price (USD)** | | |
| **LOT 3 – Supply of Reinforced Fibreglass Buoy (Long Term Agreement)** | | | | | | | | | | | | | |
| **3.1** | | **Reinforced Fibreglass Buoy as per following specifications:** | |  | | 1 | **15 Sets\*** | |  | |  | | |
| * + - * The buoy should be a large, fiberglass reinforced plastic buoy of a volume of 800 to 900 litres, diameter1200 to 1300 mm and height of 1000mm measured from base to top of the buoy and ballasted with concrete to act as counterweight to provide stability.       * The thickness of the fibreglass buoy should be at least 10mm       * A stainless-steel rod of diameter 16 mm with both extremities secured within the concrete ballast and twisted into a ring of diameter 100mm should be provided under the buoy for anchoring the buoy       * The buoy should bear a stainless-steel mast of 60mm diameter and 1450mm in height reinforced with fiberglass.       * At least three stainless steel lifting legs should be provided on the top side of the buoy and 2 stainless U-bolt on the sides for rigging purposes.       * The buoy should be filled with polystyrene foam and fitted on the outside throughout the maximum horizontal circumference with a rubber fender of minimum thickness 60mm.       * Fitted with a solar-powered flashing beacon light and a tube type radar reflector on a stainless-steel mast.       * The buoy should be coloured yellow and bear the ‘X’-stop mark indication as provided in the International Navigation and Maritime Guidelines.       * The buoy should bear the **relevant logos to be provided by the project team** and markings of at least 150mm in height and in black colour as follows: **FAD, DCP, FISHERIES, MAURITIUS, Tel: +2302347207, Email: fitec@govmu.org**       * Resistant to adverse weather condition and designed to buffer the impact of collision with sea going vessels | |
| **Subtotal for LOT 3** | | | | | | | | | | |  | | |
| **TOTAL (LOT 1 + LOT 2 + LOT 3)** | | | | | | | | | | |  | | |
| **Currency of the Quotation:** Click or tap here to enter text.  **INCOTERMS:** Click or tap here to enter text. | | | | | | | | | | | | |
|  | | **Description** | | **Projected Quantities of FADs\*** | | | **Unit Price (USD)** | | **Total Price (USD)** | |
| **LOT 4: Mounting, installation, and deployment of Fish Aggregating Devices (FADs) including provision of necessary materials – (Long Term Agreement)** | | | | | | | | | | |
| **A** | | Mounting, installation, and deployment of Fish Aggregating Devices (FADs) including provision of necessary materials *(Including assembly, transportation of the FADs and deployment at sea)* | | **15\*** | | |  | |  | |
| **B** | | Relevant downloading and processing software compatible with the above Satellite buoy tracking / biomass sensor **(One-Off item for Lot 4)** | | 1 | | |  | |  | |
| **C** | | Relevant training to at least five (5) Officers from the Ministry of Blue Economy, Marine Resources, Fisheries and Shipping and the Rodrigues Regional Assembly about downloading and processing software compatible with satellite buoy tracking/ biomass sensor **(One-Off item for Lot 4)** | | At least 5 | | |  | |  | |
| **TOTAL FOR LOT 4** | | | | | | | | |  | |

***\*The projected total quantity to be ordered by UNDP over the lifetime of the Long-Term Agreement however, UNDP makes no financial commitment for purchase of any quantity.***

**Compliance with Requirements**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **You Responses** | | |
| **Yes, we will comply** | **No, we cannot comply** | **If you cannot comply, pls. indicate counter - offer** |
| Minimum Technical Specifications |  |  | Click or tap here to enter text. |
| Delivery Term (INCOTERMS) |  |  | Click or tap here to enter text. |
| Delivery Lead Time |  |  | Click or tap here to enter text. |
| Warranty and After-Sales Requirements |  |  | Click or tap here to enter text. |
| Validity of Quotation |  |  | Click or tap here to enter text. |
| Payment terms |  |  | Click or tap here to enter text. |
| Other requirements *[pls. specify]* |  |  | Click or tap here to enter text. |

**Other Information:**

|  |  |
| --- | --- |
| Estimated weight/volume/dimension of the Consignment: | Click or tap here to enter text. |
| Country/ies of Origin:  (*if export licence required this must be submitted if awarded the contract*) | Click or tap here to enter text. |

|  |  |
| --- | --- |
| I, the undersigned, certify that I am duly authorized to sign this quotation and bind the company below in event that the quotation is accepted. | |
| *Exact name and address of company*  Company NameClick or tap here to enter text.  Address: Click or tap here to enter text.  Click or tap here to enter text.  Phone No.: Click or tap here to enter text.  Email Address: Click or tap here to enter text. | Authorized Signature:  Date: Click or tap here to enter text.  Name: Click or tap here to enter text.  Functional Title of Authorised  Signatory: Click or tap here to enter text.  Email Address: Click or tap here to enter text. |

## 