**ADDENDUM - Annex A – CRIS TECHNICAL SPECIFICATONS – ITB-SC-NIGMA-2022-02 – Supply and Delivery of CRIs**

**Annual Requirements**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | | |  |  | |  |  |
| **Company Qualification:** | | |  |  | | |  | | |
| **Please state year founded, all office locations, number** | | |  |  | | |  | | |
| **Please state the main (core) business of your company** | | |  |  | | |  | | |
| **Please list here contact details of at least 2 current or former clients (excluding UNHCR) for reference checks** | | |  |  | | | **Client Org.: Contact Person: Email/Tel.:** | | |
|  |  | | | **Client Org.: Contact Person: Email/Tel.:** | | |
| **Please state the total number of current clients** | | |  |  | | |  | | |
| **Firm experience: List 2 similar projects currently underway or successfully completed projects in the past 2-3 years; (supported by proofing documentation, such as copy of PO or Contract or work order)** | | |  |  | | | **Service/Goods: Client: Location: Value:** | | |
|  |  | | | **Service/Goods: Client: Location: Value:** | | |
| **Item No** | **Item** | **Technical Specifications - CRIs** | | | **UOM** | **Annual Requirements** | | **Please specify Quantity ready to dispatch on Emergency basis** | **Pleae indicate Delivery Time upon receipt of PO – (5-10 days)** |
| 1 | Blankets | **Make:** Woven, 50% wool fibres ±5%, 50% other textile fibres, recycled fibres accepted.  **Colour:** Grey, brown or other dark colours preferably not died.  **Size:** 150cm x 200cm +3%/-1%.  **Weight:** 2kg, edges must be stitched with cloth. To be taken on flat stabilized sample, without folds.  **Packing:** 60 pieces. Compressed and strapped with 5 straps (2 lengthwise, 3 crosswise).  **Logo**: Blue UNHCR Logo approx. 0.5m x 0.5m at center. | | | **Piece** | **90,000** | |  |  |
| 2 | Sleeping Mats | **Make:** Synthetic, Tear proof, Plastic, Water impervious.  **Size:** 1.8 X 0.9m minimum **+3%/-1%**  **Weight:** 500g/m² minimum  **Colour:** Assorted, neutral design. **Weave:** Floor mats made in a tightly woven twill weave fabric (2/1, 3/1, 2/2, 3/2) of clean and net appearance.  **Weft**: Recycled polypropylene (PP) hollow tubes not containing any filler.  **Packing:** Bales of 25 pieces, compressed. Package to be wrapped in a protective outer PP woven canvas, with 4 straps. No individual.  **Logo**: Blue UNHCR Logo approx**. 0.5m x 0.5m**, in the center | | | **Piece** | **100,000** | |  |  |
| 3 | Jerry Can | **Make:** Polyamide 38 micron made of Polyethylene 280micron UV stabilized with non-toxic coating. A built-in carrying handle. Zipper closed top opening, 140mm.  **Volume:** 10L. minimum  **Weight:** 250g minimum  **Colour:** Yellow jerry can with red caps. UV treated for long -term outdoor use. Allows users to see the fill-level of jerry cans without opening the lid.  **Packing:** The packing must guaranty that the jerrycans will not be damaged while delivery and without intended designed bended plastic surfaces.  **Logo**: UNHCR logo situated in the centre of the 2 largest opposite sides on each jerry can - **approx. 0.5m x 0.5m** | | | **Piece** | **60,000** | |  |  |
| 4 | Jerry Can | **Make:** Polyamide 38 micron made of Polyethylene 280micron UV stabilized with non-toxic coating. A built-in carrying handle. Zipper closed top opening, 140mm.  **Volume:** 20L. minimum  **Weight:** 300g minimum  **Colour:** Yellow jerry can with red caps. UV treated for long -term outdoor use. Allows users to see the fill-level of jerry cans without opening the lid.  **Packing:** The packing must guaranty that the jerrycans will not be damaged while delivery and without intended designed bended plastic surfaces.  **Logo**: UNHCR logo situated in the centre of the 2 largest opposite sides on each jerry can - **approx. 0.5m x 0.5m** | | | **Piece** | **30,000** | |  |  |
| 5 | Laundry powder Detergent | **Make:** Powder or soap for hand washing clothes, not harmful to skin, product must be fit for human utilization, without any disagreeable odours and flavours, to the skin, from vegetable or animal fat, no containing pork fat.  **Colour**: Homogeneous colour  **Weight:** 200g  **Packing:** **24 packs of 200g per carton.** | | | **Piece** | **210,000** | |  |  |
| 6 | Bath Soap | **Make**: Bar of 225gr-250gr for bathing, not harmful to skin, from animal or vegetable fat not containing pork fat, must be fit for human utilization, without any disagreeable odours and flavours  **Type: Foaming hand wash**  **Content: Fatty acid: min.70%. NaOH content: maximum 0.3%**  **Colour:** Homogeneous colour  **Size:** minimum 5.5x10x3cm  **Weight:**  **225gr -250gr**  **Packing:** 24 bars of **225gr -**250g per carton. Bars individually packed in nylon bag film sealed and enclosed on all edges. | | | **Piece** | **230,000** | |  |  |
| 7 | Treated Mosquito Nets | **Make:** Manufactured from 100% high density polyethylene OR polyester. Mosquito nets Long Lasting Insecticidal Nets (LLIN's). Treated with 80 mg/m² Deltamethrin.  **Mesh size:** Minimum 130 holes per inch². Minimum 320 Kpa.  **Height:** 150-160cm,  **Length:** 180cm,  **Width:** 190cm.  **Packing:** Individual packaged, then bale. | | | **Piece** | **60,000** | |  |  |
| 8 | Reusable Sanitary Pads. | **Make: Top: A**bsorbent layer of Micro fleece 100% Polyester or 100% cotton (towel type). **Inside:** The absorbance part consists of at least two additional layers of 100% cotton (towel type) or 2 absorbent layers of Micro fleece, 80% polyester and 20% polyamide. **Bottom:** Waterproof layer of Polyurethane Laminate (PUL).  **Absorption:** The pad must have an absorption capacity of at least 40ml.  (absorbent) OR 60ml (super absorbent).  **Width:** Width 20cm. **Length**: 28cm, Tolerance: +/- 5%  **Colour:** Dr. Brown type or similar, no pink colour.  **Packing:** Good quality transparent sealed polythene bag made of virgin polythene including 6 to 8 sanitary pads and waterproof bag. | | | **Piece** | **70,000** | |  |  |
| 9 | Basins | **Make:** Heavy-duty plastic, Polyethylene.  **Manufacturing:** Injection moulded.  **Design**: Curved join inside base to wall for easy cleaning.  **Dimensions**: Height: 18cm, top diameter: 33cm, base diameter: 23cm, +/-5%  **Colour:** Blue colour.  **Weight:** 200g  **Capacity**: 10 Litres minimum.  **Packing:**  In strong boxes of 40 basins. | | | **Piece** | **30,000** | |  |  |
| 10 | Plastic Kettle | **Make:** polyethylene with lid.  **Volume**: minimum 2L.  **Finish:** Handle and spout with no sharp edges | | | **Piece** | **60,000** | |  |  |
| 11 | Solar Lamps | **Make:** Rechargeable lamp by built-in solar cell and 110V- 250V direct power outlet. Includes USB cell phone charger and USB cable.  **Casing:** made of unbreakable plastic.  **Batteries/power**: 3x1000mAH, AA size, Dry Battery.  **LEDs**: 15 pieces high-brightness SMD with 1-piece lampshade.  **Solar Run Time:** (duration on a day's solar charge): Minimum 4 hrs.  **Solar panel:** Mono crystalline, working current 70-120MA  **Weight**: 250g | | | **Piece** | **40,000** | |  |  |
| 12 | Foldable Mattress | **Description: Double Sided Folded Mattress**  **Type of foam**: Medium: Polyurethane foam, 25kg/m³; thickness: 10cm, minimum, in 1 piece not glued.  **Cover:** Woven polyester 75g/m² minimum OR non-woven polypropylene of 100g/m² minimum, with strong plastic zip.  **Size**: 2m x 0.7m. Thickness: 0.06m.  **Weight:** 2kg  **Packing:** Wrapped in a water-tight micro perforated plastic film and covered with a polypropylene or jute woven bag.  **Logo:** Blue UNHCR Logo approx. 0.5m x 0.5m at centre. | | | **Piece** | **80,000** | |  |  |
| 13 | Bucket | **Make:** Heavy-duty plastic bucket, with metallic handle  **Volume/Capacity:**  10L, minimum.  **Material:** Virgin HDPE high density polyethylene, and virgin LDPE low density polyethylene  **Manufacturing:** Injection moulded.  **Design:** Reinforced bottom ridge to prevent scraping of the base. Reinforced top to prevent bucket distorting to an oval shape bucket together curved join inside base to wall for easy cleaning.  Colour: Blue Colour.  **Weight:** 100g  **Dimension:** +/-5% Height: 26.5cm, top diameter: 29cm, base diameter: 21cm. Cover with outlet of 50mm +/- 10% and clip cap.  **Packing:** In strong boxes of 20 buckets.  **Logo**: UNHCR logo situated in the centre/midpoint on outside (white Logo). | | | **Piece** | **75,000** | |  |  |
| 14 | Cooking Pots  **Set of two (2) pieces** | **Make:** Locally made aluminium. Chemical composition of semi products used for the fabrication of articles for use in contact with food.  **Capacity:** 7 Litres, 2mm thick  **Design:** with lid. Bowl shaped parameter from the bottom side upwards connected to an inward circular bent and an outward circular extended diameter at the top.  **Material:** Locally made aluminium. Chemical composition of semi products used for the fabrication of articles for use in contact with food.  **Lid:** 1mm minimum thickness with strong durable handle. Handle must resist 2kg minimum load  **Finish:** No sharp edges, food grade surface finish | | | **Set of two (2) pieces** | **30,000** | |  |  |
| 15 | Stainless Trays | **Capacity:** 1.5 -2 litres minimum  **Material:** 200 series stainless steels of appropriate grades.  **Thickness:** min 0.5mm in the centre of the bottom?  **Diameter:** Minimum 40-45cm diameter.  **Weight:** 200-250g  **Finish:** No sharp edges, food grade surface finish Packing Carton | | | **Piece** | **60,000** | |  |  |
| 16 | Stainless Cups | **Volume:** 0.3 litres minimum  **Material:** Stainless steel  **Handles:** Secure weld. Handle to resist to 1kg load  **Finish:** No sharp edges, food grade surface finish  **Packaging**: In a carton of 80 pcs. | | | **Piece** | **180,000** | |  |  |
| 17 | Kitchen Knife | **Material:** One-piece solid stainless steel attached to a wooden or plastic handle  **Length** 29cm  **Weight**  100g  **Packing:** 240 knifes per carton with protective cover on each knife. | | | **Piece** | **30,000** | |  |  |
| 18 | Serving Spoon | **Volume:** 35ml minimum  **Material:** One-piece solid Aluminium local made  **Length:** 35cm-40cm  **Thickness:** 1mm minimum in the centre of the scoop  **Finish:** No sharp edges, food grade surface finish  **Packing:** 50 pcs per packet. | | | **Piece** | **60,000** | |  |  |
| 19 | Polyester Packaging bags - Large | **Make:** The bags should be in “box like” shape (like “GHANA MUST GO” or equivalent to BAGCO bags having two handles on both sides with strong zip on top and the colour should be plain either grey or harsh or white.  It should be 100% POLYESTER and strong enough to carry almost 15 to 30 KG weight.  **Sizes**: Large  Dimension: L= 0.65m, B = 0.35m and H = 0.65m. Volume is 0.15m3  **Logo**: Branded with UNHCR Logo (dark blue color) and name as screen printing on all sides of bags. | | | **Piece** | **30,000** | |  |  |
| 20 | Polyester Packaging bags - **Medium** | **Make:** The bags should be in “box like” shape (like “GHANA MUST GO” or equivalent to BAGCO bags having two handles on both sides with strong zip on top and the colour should be plain either grey or harsh or white.  It should be 100% POLYESTER and strong enough to carry almost 15 to 20 KG weight.  **Sizes**: **Medium**.  Dimension is L = 0.5, B = 0.25 and H = 0.5 Volume: 0.06m3  **Logo**: Branded with UNHCR Logo (dark blue color) and name as screen printing on all sides of bags. | | | **Piece** | **10,000** | |  |  |
| 21 | Disposable Sanitary Pads (Single use) | "Always",Dr Brown or virony brand.  Absorbent layer: Top (60-100mm) Polyester 100% or 100% cotton. Middle absorbent layer of cellulosic material and outer layer of plastic. Protective Barrier: Should have an identifying mark or colour indicating clearly the side of the barrier. Odour:The sanitary pad should not have unpleasant odour either in dry state. Packages of 8 to 10 pieces of white color. Texture: The sanitary pad should be smooth and soft when felt by hand. | | | **piece** | **60,000** | |  |  |
| 22 | **Fuel Efficient Stoves** | **Material:**  Mixture of Clay and sawdust, which is molded, baked, and finished with a metal cladding (mild steel of thickness greater than or equal to 0.5mm with heat resistant paint).  **Weight:**  14-15kg  **Height:**  24-26cm  **Top Diameter:**  33-36cm  **Bottom Diameter:**  25-27cm  **Firewood Opening:**  8x8cm -15x15cm  **Further Description:** There should be a removeable charcoal grate. Handles must be present for safety during cooking and there must be three (3) solid stove legs to ensure sufficient stability during cooking. While eight (8) to nine (9) symmetrical air holes are provided on the bottom of the combustion chamber. Bottom of the stove should have a cylindrical shape and the top of the stove should have the shape of a cone. The stoves should be able to accommodate the predominant shape of cooking pots in Maiduguri. | | | **Piece** | **44,300** | |  |  |

Company’s Name:

Signature and Stamp:

Date: