**Annex 7 - NETWORK PRINTER TECHNICAL SPECIFICATIONS**

1. **Network Printer (Black & White) - 44**

**Main Specifications** MX-M5051

* Type Monochrome multi-function digital document system
* Display 10.1" (diagonal) color dot matrix high-resolution touch panel tilting display. 1,024 x 600 dots (W-SVGA)
* Functions Copy, print, network print, network scan, document filing and fax1
* Copy System Dry electrostatic transfer/Dual component developer/Magnetic brush development/OPC drums/Belt fusing/white LED exposure
* Originals Sheets and bound documents
* Max. Original Size 11" x 17"
* Output Size Min. 5½" x 8½", Max. 12" x 18"
* Copy Speed 50/60 ppm (8½" x 11")
* Multiple Copy Max. 9,999 copies
* Magnification 25% to 400% in 1% increments (with RSPF 25%-200%)
* Original Feed 100-sheet RSPF with original size detection
* Scan Speed Copy: Up to 80 ipm (Mono)Scan: Up to 80 ipm (Mono/Color)
* Original Sizes 5½" x 8½", 8½" x 11", 8½" x 11" R, 8½" x 14", 11" x 17"
* Paper Capacity Standard: 650 Sheets, Maximum: 6,300 Sheets
* Paper Feed Standard: (1) paper drawer 550 sheets (letter/legal/ledger/ stmt. System size) or up to 50 envelopes (max. height: 25 mm), 100-sheet (or 20 envelope) bypass tray.
* Paper Weights Paper drawers: 18 lb. bond to 110 lb. cover. and Types Drawer 1: 20-24 lb. bond or Monarch/Com-9 envelopes. Split Tandem Drawers: 18 lb. bond to 28 lb. bond or plain, pre-printed, recycled, pre-punched, letterhead and color paper. Bypass tray: 16-28 lb. bond (plain paper), 13-16 lb. bond (thin paper), 28 lb. bond-110 lb. cover (heavy paper), tab paper (letter) and Monarch/Com-10 envelopes. Also label, gloss, preprinted, recycled, pre-punched, letterhead and color paper or OHP film.
* Duplexing Standard automatic duplex copying and printing
* CPU Up to 1.4 GHz multi-processor design
* Interface 10/100/1000 Base-T Ethernet, USB 2.0: 2 host ports (front & rear), **include wireless 802.11 b/g/n**
* Memory Standard 5 GB copy/print (shared)
* Hard Disk Drive 500 GB
* Copy Resolution Scan: Up to 600 x 600 dpiOutput: Up to 600 x 600 dpi
* Copy Modes Monochrome/Grayscale

1. **Network Printer (Color) - 37**

**Main Specifications:** MX- 3551

* Type Color multi-function digital document system
* Display 10.1" (diagonally measured) color dot matrix high-resolution touch panel tilting display. 1,024 x 600 dots (W-SVGA)
* Functions Copy, print, network print, network scan, document filing and fax1
* Copy System Dry electrostatic transfer/Dual component developer/Magnetic brush development/OPC drums/Belt fusing/white LED exposure
* Originals Sheets and bound documents
* Max. Original Size 11" x 17"
* Output Size Min. 5½" x 8½", Max. 12" x 18"
* Copy Speed 35 ppm Mono/Color (8½" x 11")
* Multiple Copy Max. 9,999 copies
* First Copy Time Platen Glass: Mono 4.7, Color 6.7 (In Seconds)2 RSPF: Mono 7.6, Color 9.7
* Warm Up Time 33 seconds (from main power switch on), 20 seconds (from [Power] button on)
* Magnification 25% to 400% in 1% increments (with RSPF 25%-200%)
* Original Feed 100-sheet RSPF with original size detection.
* Scan Speed Copy: Up to 80 ipm (Mono)/53 ipm (Color)Scan: Up to 80 ipm (Mono/Color)
* Original Sizes 5½" x 8½", 8½" x 11", 8½" x 11" R, 8½" x 14", 11" x 17"
* Paper Capacity Standard: 650 Sheets/Maximum: 6,300 Sheets
* Paper Feed Standard: (1) paper drawer 550 sheets (letter/legal/ledger/ stmt. System size) or up to 50 envelopes (max. height: 25 mm), 100-sheet (or 20 envelope) bypass tray.
* Paper Weights Paper drawers: 18 lb. bond to 110 lb. cover. and Types Drawer 1: 20-24 lb. bond or Monarch/Com-9 envelopes. Split Tandem Drawers: 18 lb. bond to 28 lb. bond or plain, pre-printed, recycled, pre-punched, letterhead and color paper. Bypass tray: 16-28 lb. bond (plain paper), 13-16 lb. bond (thin paper), 28 lb. bond-110 lb. cover (heavy paper), tab paper (letter) and Monarch/Com-10 envelopes. Also label, gloss, preprinted, recycled, pre-punched, letterhead and color paper or OHP film.
* Duplexing Standard automatic duplex copying and printing
* CPU Up to 1.4 GHz multi-processor design
* Interface 10/100/1000 Base-T Ethernet, USB 2.0: 2 host ports (front & rear), 1 available device port (rear), **Include wireless 802.11 b/g/n**
* Memory Standard 5 GB copy/print (shared)
* Hard Disk Drive 500 GB
* Copy Resolution Scan: 600 x 600 dpi (Mono/Color)Output: Up to 600 x 600 dpi
* Color Modes Auto Color Selection (ACS), Full Color Mode, Monochrome (B/W)