**Refrigerator:**

* Installation method: standing separately
* Width, cm: 47.5-48.5
* Height, cm: 82-85
* Depth, cm: 50-53
* Number of doors: 1
* Construction: single chamber
* Management: mechanical
* Backlight: LED
* Energy consumption class: A+ and higher
* Climate class: SN, N, ST, T
* Noise level, dB: 35-45
* Color: white
* Total volume, l: 85-95
* The useful volume of the refrigerating chamber, l:  80-85
* Freezing: none
* Defrosting of the refrigerating chamber: automatic (drip)
* Compressor type: piston
* Number of compressors: 1
* Number of separately cooled circuits: 1
* Number of main shelves in the refrigerating chamber: 3-4
* Shelves material: glass (strained preferable)
* Voltage: 220-230 V
* Frequency: 50 Hz