United Nations Population Fund

Address: 131, 31 August 1989 Street

Chisinau, Republic of Moldova

Tel: (+373) 22 214002

**Date:** 21/06/2023

**Request for Quotation No. UNFPA/MD/RFQ/21/2023**

Dear Sir/Madam,

We hereby solicit your quotation for Gynaecological Mobile Clinic and supplies, named below to Str. Industriala 5, Chisinau, Moldova, Incoterm: CPT

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| # | Item | Description | Quantity | Unit of Measure |
| 1 | Gynaecological Mobile Clinic and supplies | Gynaecological Mobile clinic based on truck should be counted as an autonomous medical unit and has a capacity to provide range of health services.  A picture containing wheel, transport, vehicle, land vehicle  Description automatically generated  Gynaecological Mobile clinic should meet following.  Dimensions:  Outside: Ca 6.5x2.2x3 (LxWxH)  Inside Medical unit: Ca 4.3x2.0x2.0(LxWxH)  **Vehicle Details:**   * Single Cabin; Left Hand Drive; 1+2 seat * Turbo & Euro – 3/5 * Power lock & Power Window * Front & Rear Disc Brake * Front Under-Run Protection * Factory Fitted driver cab AC * Payload – 4.2 Tons approx. * Engine- EURO-3/5, 4000cc. or above 4 cylinder * Manual Gear Box * Engine Power: 136hp or higher * Transmission: 5 forward and 1 reverse speed * 6-stud disc wheel, including spare tires * Ground clearance – 185mm * USB Charging Port * Tool Kit and battery charging cable   **1. Equipment for an independent operation and furniture:**   * Two desks with drawers and cabinets for both, doctor and nurse * Closet with shelves. * Cabinet for medicine and instrument storage with drawers. * Washing basin with automatic electrical water tap and water tanks for fresh & wastewater 50 liters each. * Floor in clinic’s cabinet: wooden floor, covered with PVC sheet anti-slippery and antistatic and anti-bacterial, and washable. * High and low temp insulation of the roof and side walls. * Medical cabinet designed and executed to store and mount the stated equipment and tools: * Drops to the drugs, one for sharp materials (needles…etc), the other for trash. * Footsteps at the clinic cabinet entrances at the rear doors. * Storage compartments, with sliding transparent doors. * Stationary heater. * Air conditioning for the patient’s cabin. (central & AC unit) * Windows foil: windows in patient’s compartment covered in a fogy or frosted foil. * Two rotating seats for doctor and nurse. * Rear door open 270o. * Right side door for rear clinic compartment. * All equipment compartments must be washable. * High quality finishing without any sharp edges. * Lettering & signs (as per our requirements). * Control panel inside patient cabinet to ease access to the operating switches for lighting, air-conditioning & heating and exhaust fans. * Two inverters 220v – 12v and 12v – 220v with electric outlets sockets 220 qty: 4v and 12v qty 2, the inverter must supply power of 2000w and having enough capacity to operate all medical facilities simultaneously. * LED internal lightening covers all ceiling for night and day operations. * Spot light above patient examination bed. * Digital watch. * Extra battery for medical equipment’s. * Battery charger (220v – 12v) (350w) * 25 meters x for external connection of 220v including electrical socket located outside of the rear compartment. * Intercom between clinic cabinet and driver cabinet refrigerator for the medical compartment. * Light bar (red led lights), mounted over driver cab. * 100w capacity of public address system with different tone siren. * Qty (2) rear working spotlight mounted at the rear and both sides R&L of the vehicle. * 6.5 KVA electrical generator (Diesel engine). * Rolling electrical umbrella, on one side (L: 3m), can be operated by a remote control. * Central oxygen therapy: (2 bottles oxygen cylinders connected to pressure regulator flow meter humidifier).  1. **Medical equipment:** 2. Gynaecological Examination Couch.  * Gynecology Examination bed, manual and multipurpose type. * Structure in steel tube and epoxy paint; foam bed lined with nappa leather; * 5 Drawers and built-in step; * 3 Sections which the head section is articulated by rack and section of the legs is extensible; * Footer stainless steel that includes tray * waste in stainless steel, 2 adjustable support for and paper rollers bracket. * Dimensions: 1700 x 590 x 850mm  1. Fully digital portable B/141 ultrasound system including following probe:  * Convex Probe. FUT-CS602-5AX 3.0/3.5/4.0 MHz, 60R. * Transvaginal Probe: FUT-TVD114-7L 4.0/5.0/6.0 MHz, 12R * Features: * Fully digital portable ultrasound system. * Continuous dynamic focusing. * One touch image optimization. * Digital data management. * Tissue harmonic imaging. * Color scaling image function. * Dual probe connection. * 2 way backlight key panel. * Ergonomically designed for ease of use. * UDB flash – memory image filling. * Technical specifications: * Scanning methods * Electronic convex array. * Electronic liner array. * Electronic micro convex array. * Monitor display * 12” active matrix (TFT) LCD flat monitor. * 800 x 600 pixels (SVGA) * Imaging Modes: * B mode (2D) Tissue harmonic imaging. M mode. * Combined Modes * B dual (28) B quad (48) B + M * Multiple gynaecologic examination sets  1. Cardiotocograph machine (CTG) (Fetal monitor  * Features: * FHR (Fetal heart rate), UC (Uterine Contraction) and FM (Fetal movement). * Automatic fetal movement detect inn. * LED display of FHR and UC. * Alarm on abnormal FHR. * Easy to read A4 size chart paper. * Use inexpensive fax paper.  1. Pulse Oximeter 2. Wall mounted sphygmomanometer/ & stethoscope sphygmomanometer blood pressure with cuff inflate. 3. Diagnostic set (eye, ear and mouth) 4. Laryngoscope kit. 5. Resuscitation bag (adult, children, infant). 6. Foldable field stretcher. 7. Eye level physician scale with high rod. 8. Adult/infant scale | 1 | L/S |

Partial bids are not allowed under this RFQ.

Payment Terms: **100% after satisfactory delivery of goods.**

Warranty: Minimum 2-year warranty for medical items/Furniture and 3 years warranty or 100,000KM for vehicle.

The unit including medical equipment’s, are to be delivered maximum in 90 days to the UNFPA warehouse with the address below upon issuing of PO. The quotation shall be valid at least for 120days after the closing date.

Vitra

Str. Industriala 5

Chisinau

Moldova

<https://goo.gl/maps/nVN19BpARyve8Myy6>

Note: **The transportation cost should be included in the price of the quotation**.

If you are interested in submitting a quotation for these items, kindly fill in the attached Quotation Form along with all the supporting documents and send by email to the address indicated below:

Email: [tender.mda@unfpa.org](mailto:tender.mda@unfpa.org)

**Please submit your quotation with catalogue for each item quoted, including images.**

For any further queries please contact [rajasekhar@unfpa.org](mailto:rajasekhar@unfpa.org) (only to submit queries)

Please submit your quotation in USD currency. Conversion of currency into the UNFPA preferred currency, if the offer is quoted differently from what is required, shall be based only on UN Operational Exchange Rate prevailing at the time of competition deadline.

The **local suppliers from Moldova** should submit their offers in local currency. UNFPA is exempted from VAT and quotation should be submitted without VAT.

Your earliest submission to this Request for Quotation would be highly appreciated, with a deadline no later than **28 June 2023, 22:00 hours, Moldova time**.

Note: Current UNFPA supplier policies apply to this solicitation and can be found at: <http://www.unfpa.org/suppliers>.

Best regards,

Rajeev Rajasekhar

Email: [rajasekhar@unfpa.org](mailto:rajasekhar@unfpa.org)

**Quotation Form**

**Name of Bidder:**

**Date of Bid:**

**Request for Quotation No:**

**Currency of Bid price:**

**Delivery time** *(weeks from receipt of order till dispatch):*

**Expiration of Validity of Quotation** *(The quotation shall be*

*valid for a period of at least 120 days after the Closing date.):*

**Price Schedule:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Item No. | Item Name | Quantity | Unit Price | Transportation cost | Total CPT | Delivery Schedule |
| Chisinau |
| 1 | Vehicle with chassis  Dimensions:  Outside: Ca 6.5x2.2x3 (LxWxH)  Inside Medical unit: Ca 4.3x2.0x2.0(LxWxH) | 1 | L/S |  |  |  |
| 2 | Equipment for an independent operation and furniture: | 1 | L/S |  |  |  |
|  | Two desks with drawers and cabinets for both, doctor and nurse |  |  |  |  |  |
|  | Closet with shelves. |  |  |  |  |  |
|  | Cabinet for medicine and instrument storage with drawers. |  |  |  |  |  |
|  | Washing basin with automatic electrical water tap and water tanks for fresh & wastewater 50 liters each. |  |  |  |  |  |
|  | Floor in clinic’s cabinet: wooden floor, covered with PVC sheet anti-slippery and antistatic and anti-bacterial, and washable. |  |  |  |  |  |
|  | High and low temp insulation of the roof and side walls. |  |  |  |  |  |
|  | Medical cabinet designed and executed to store and mount the stated equipment and tools: |  |  |  |  |  |
|  | Drops to the drugs, one for sharp materials (needles…etc), the other for trash. |  |  |  |  |  |
|  | Footsteps at the clinic cabinet entrances at the rear doors. |  |  |  |  |  |
|  | Storage compartments, with sliding transparent doors. |  |  |  |  |  |
|  | Stationary heater. |  |  |  |  |  |
|  | Air conditioning for the patient’s cabin. (central & AC unit) |  |  |  |  |  |
|  | Windows foil: windows in patient’s compartment covered in a fogy or frosted foil. |  |  |  |  |  |
|  | Two rotating seats for doctor and nurse. |  |  |  |  |  |
|  | Rear door open 270o. |  |  |  |  |  |
|  | Right side door for rear clinic compartment. |  |  |  |  |  |
|  | All equipment compartments must be washable. |  |  |  |  |  |
|  | High quality finishing without any sharp edges. |  |  |  |  |  |
|  | Lettering & signs (as per our requirements). |  |  |  |  |  |
|  | Control panel inside patient cabinet to ease access to the operating switches for lighting, air-conditioning & heating and exhaust fans. |  |  |  |  |  |
|  | Two inverters 220v – 12v and 12v – 220v with electric outlets sockets 220 qty: 4v and 12v qty 2, the inverter must supply power of 2000w and having enough capacity to operate all medical facilities simultaneously. |  |  |  |  |  |
|  | LED internal lightening covers all ceiling for night and day operations. |  |  |  |  |  |
|  | Spot light above patient examination bed. |  |  |  |  |  |
|  | Digital watch. |  |  |  |  |  |
|  | Extra battery for medical equipment’s. |  |  |  |  |  |
|  | Battery charger (220v – 12v) (350w) |  |  |  |  |  |
|  | 25 meters x for external connection of 220v including electrical socket located outside of the rear compartment. |  |  |  |  |  |
|  | Intercom between clinic cabinet and driver cabinet refrigerator for the medical compartment. |  |  |  |  |  |
|  | Light bar (red led lights), mounted over driver cab. |  |  |  |  |  |
|  | 100w capacity of public address system with different tone siren. |  |  |  |  |  |
|  | Qty (2) rear working spotlight mounted at the rear and both sides R&L of the vehicle. |  |  |  |  |  |
|  | 6.5 KVA electrical generator (Diesel engine). |  |  |  |  |  |
|  | Rolling electrical umbrella, on one side (L: 3m), can be operated by a remote control. |  |  |  |  |  |
|  | Central oxygen therapy: (2 bottles oxygen cylinders connected to pressure regulator flow meter humidifier). |  |  |  |  |  |
| 3 | Medical equipment: | 1 | EA |  |  |  |
|  | Gynaecological Examination Couch. |  |  |  |  |  |
|  | Fully digital portable B/141 ultrasound system including following probe: |  |  |  |  |  |
|  | Convex Probe. FUT-CS602-5AX 3.0/3.5/4.0 MHz, 60R. |  |  |  |  |  |
|  | Transvaginal Probe: FUT-TVD114-7L 4.0/5.0/6.0 MHz, 12R |  |  |  |  |  |
|  | Cardiotocograph machine (CTG) (Fetal monitor |  |  |  |  |  |
|  | Pulse Oximeter |  |  |  |  |  |
|  | Wall mounted sphygmomanometer/ & stethoscope sphygmomanometer blood pressure with cuff inflate. |  |  |  |  |  |
|  | Diagnostic set (eye, ear and mouth) |  |  |  |  |  |
|  | Laryngoscope kit. |  |  |  |  |  |
|  | Resuscitation bag (adult, children, infant). |  |  |  |  |  |
|  | Foldable field stretcher. |  |  |  |  |  |
|  | Eye level physician scale with high rod. |  |  |  |  |  |
|  | Adult/infant scale |  |  |  |  |  |

**In your offer, please include:**

1. Detailed technical specifications of each products offered
2. Catalogue and images of the equipment’s
3. Completed Fast Track Procurement Questionnaire for Medical Devices
4. Quality standard of the products, ISO, EC. Confirmation of CE markings.
5. Company registration document
6. Previous experience with UNFPA and UN organization
7. Written Self-Declaration of not being included in the UN Security Council 1267/1989 list, UN Procurement Division List or other UN Ineligibility List
8. Warranty information
9. Price should exclude VAT – UNFPA is exempted from VAT

*Vendor’s Comments:*

**I hereby certify that this company, which I am duly authorized to sign for, accepts the terms and conditions of UNFPA (**<http://www.unfpa.org/resources/unfpa-general-conditions-contract> **) and we will abide by this quotation until it expires.**

**Name and title Date and Place**