**Section II: Schedule of Requirements\_revision 1**

| E-Sourcing reference no: RFQ/2024/51411\_revision 1 |
| --- |

1. **Summary of Requirements for provision of modular vests, helmets, plate carriers.**

**UNOPS requirements are comprised of the following 3 (three) lots:**

**Lot 1 - Tactical modular vest with ballistic level IV plates**

**Lot 2 - Ballistic modular helmet**

**Lot 3 - Plate carriers**

1. **Requirements and technical specifications.**

**Lot 1 - Tactical modular vest with ballistic level IV plates**

| **N** | **UNOPS minimum technical requirements**  **Мінімальні технічні вимоги UNOPS** | **Is Bid Compliant? Bidder to complete** | **Details of the offered goods. Bidder to complete** |
| --- | --- | --- | --- |
| **1** | **Tactical modular vest with ballistic protection level NIJ level IV (0101.06) or higher** | ☐ Yes ☐ No |  |
| 1.1 | Light-weight and flexible | ☐ Yes ☐ No |  |
| 1.2 | Capable of taking hard armor plates for protection against high-velocity bullets | ☐ Yes ☐ No |  |
| 1.3 | Have low back face deformation | ☐ Yes ☐ No |  |
| 1.4 | Plates that can be fitted to the front and back of the jacket | ☐ Yes ☐ No |  |
| 1.5 | Lightweight plates: Depending on the size and cut, the weights range from 4 pounds (1.8 kg) to 8.8 pounds (4 kg) | ☐ Yes ☐ No |  |
| 1.6 | To provide a certificate that confirms protection level NIJ level IV (0101.06) or higher | ☐ Yes ☐ No |  |
| 1.7 | At least 4 adjustment points for maximizing comfort | ☐ Yes ☐ No |  |
| 1.8 | Main plate should provide a level of protection NIJ IV or higher. | ☐ Yes ☐ No |  |
| 1.9 | Mesh retaining panels are fitted to the front and rear to aid comfort | ☐ Yes ☐ No |  |
| 1.10 | Low profile | ☐ Yes ☐ No |  |
| 1.11 | Color: grey/blue(preferable)/black | ☐ Yes ☐ No |  |
| 1.12 | Modular  - collar for neck protection, detachable;  - protection of the lower abdomen, detachable.  Any level of protection. | ☐ Yes ☐ No |  |
| 1.13 | Ballistic plates are classified as a stand-alone plate | ☐ Yes ☐ No |  |
| 1.14 | Ballistic plates classified as Level 4 NIJ standard | ☐ Yes ☐ No |  |
| 1.15 | Size: S, M, L, XL | ☐ Yes ☐ No |  |
| **2** | **General requirements** |  |  |
| 2.1 | All the mentioned equipment should be new. | ☐ Yes ☐ No |  |
| 2.2 | Bid includes brand/model of the goods and manufacturer's technical literature/catalogue, all confirming that the offered items comply with required specifications | ☐ Yes ☐ No |  |
| 2.3 | **Warranty:** at least soft plates are 5 years and for steel 10 years | ☐ Yes ☐ No |  |
| 2.4 | Technical documentation for maintenance and repair of the supplied goods. The minimum set of technical documents to be provided with each piece of equipment delivered is the following: • User Manual and Operating Instructions (in Ukrainian or English) • Technical Certificate/maintenance guidelines (in Ukrainian or English) The Bidder is required to confirm the list and contents of documentation to be provided together with the Goods at the delivery. All tags/labels on the equipment shall be in English or Ukrainian language. | ☐ Yes ☐ No |  |
| 2.5 | Bid includes the Country of origin of the goods. | ☐ Yes ☐ No |  |

**C. 1. Delivery requirements for Lot 1**

| **UNOPS Requirements** | |
| --- | --- |
| **Delivery time** | Bidder shall deliver the goods as soon as possible **but not later than 30 days after PO issuance. Please indicate the delivery time in your Quotation**. |
| **Delivery place and Incoterms rules** | DAP Customs cleared Incoterms 2020 (delivered at place) Kyiv, Ukraine, net of any direct taxes, customs duties, or indirect taxes. |
| **Consignee details** | 3rd floor, 15, Yaroslaviv Val str., Kyiv, Ukraine. |
| **Acceptance** | Bidder shall remain liable for the packing and consistency of the items supplied for the period of shipment and acceptance for use. Any items found unacceptable shall be returned and changed at no cost to UNOPS. |
| **Packing standards** | Bidder shall ensure the best international packing standards of goods supplied, including the use of eco-friendly packing materials. |

**Lot 2 - Ballistic modular helmet**

| **N** | **UNOPS minimum technical requirements**  **Мінімальні технічні вимоги UNOPS** | **Is Bid Compliant? Bidder to complete** | **Details of the offered goods. Bidder to complete** |
| --- | --- | --- | --- |
| **1** | **Ballistic modular helmet with protection Level: NIJ Standard 0106.01 for ballistic helmet. Type II (Higher Velocity 357 Magnum 9 mm)** | ☐ Yes ☐ No |  |
| 1.1 | Helmet with Kevlar | ☐ Yes ☐ No |  |
| 1.2 | Protect against bullets, shrapnel & fragments | ☐ Yes ☐ No |  |
| 1.3 | Coverage: Low cut | ☐ Yes ☐ No |  |
| 1.4 | Have structural stability | ☐ Yes ☐ No |  |
| 1.5 | Have long term stability | ☐ Yes ☐ No |  |
| 1.6 | Low сut design | ☐ Yes ☐ No |  |
| 1.7 | Designed for comfort | ☐ Yes ☐ No |  |
| 1.8 | Compatibility with Chem/Bio Masks and communication devices | ☐ Yes ☐ No |  |
| 1.9 | Offers unsurpassed impact protection and ballistic-rated hardware | ☐ Yes ☐ No |  |
| 1.10 | To provide certificates that confirm protection level NIJ level IIIa (0108.01/0101.06) or higher. | ☐ Yes ☐ No |  |
| 1.11 | 4 Point Suspension System | ☐ Yes ☐ No |  |
| 1.12 | Allows free use of common equipment | ☐ Yes ☐ No |  |
| 1.13 | Flexible Harness System | ☐ Yes ☐ No |  |
| 1.14 | Enhanced Stability and Resist Roll-offs | ☐ Yes ☐ No |  |
| 1.15 | Color: black/blue(preferable) | ☐ Yes ☐ No |  |
| 1.16 | Modular.  Availability of velcro patches, compatibility with night-vision goggles and gas masks (any type). | ☐ Yes ☐ No |  |
| 1.17 | Increased padding for comfort | ☐ Yes ☐ No |  |
| 1.18 | Accommodating variety of sizes or Size: S, M, L, XL | ☐ Yes ☐ No |  |
| **2** | **General requirements** |  |  |
| 2.1 | All the mentioned equipment should be new. | ☐ Yes ☐ No |  |
| 2.2 | Bid includes brand/model of the goods and manufacturer's technical literature/catalogue, all confirming that the offered items comply with required specifications | ☐ Yes ☐ No |  |
| 2.3 | **Warranty:** at least 5 years (ballistic warranty), 1 year (parts warranty) | ☐ Yes ☐ No |  |
| 2.4 | Technical documentation for maintenance and repair of the supplied goods. The minimum set of technical documents to be provided with each piece of equipment delivered is the following: • User Manual and Operating Instructions (in Ukrainian or English) • Technical Certificate/maintenance guidelines (in Ukrainian or English) The Bidder is required to confirm the list and contents of documentation to be provided together with the Goods at the delivery. All tags/labels on the equipment shall be in English or Ukrainian language. | ☐ Yes ☐ No |  |
| 2.5 | Bid includes the Country of origin of the goods. | ☐ Yes ☐ No |  |

**C. 2. Delivery requirements for Lot 2**

| **UNOPS Requirements** | |
| --- | --- |
| **Delivery time** | Bidder shall deliver the goods as soon as possible **but not later than 30 days after PO issuance. Please indicate the delivery time in your Quotation**. |
| **Delivery place and Incoterms rules** | DAP Customs cleared Incoterms 2020 (delivered at place) Kyiv, Ukraine, net of any direct taxes, customs duties, or indirect taxes. |
| **Consignee details** | 3rd floor, 15, Yaroslaviv Val str., Kyiv, Ukraine. |
| **Acceptance** | Bidder shall remain liable for the packing and consistency of the items supplied for the period of shipment and acceptance for use. Any items found unacceptable shall be returned and changed at no cost to UNOPS. |
| **Packing standards** | Bidder shall ensure the best international packing standards of goods supplied, including the use of eco-friendly packing materials. |

**Lot 3 - Plate carriers**

| **N** | **UNOPS minimum technical requirements**  **Мінімальні технічні вимоги UNOPS** | **Is Bid Compliant? Bidder to complete** | **Details of the offered goods. Bidder to complete** |
| --- | --- | --- | --- |
| **1** | **Plate carriers standard with flame resistance standard BS 6941:2003 or higher** | ☐ Yes ☐ No |  |
| 1.1 | compatibility with plate inserts that comply with standard NIJ - 0101.06 (threat level 4 (IV)) | ☐ Yes ☐ No |  |
| 1.2 | to provide certificate flame resistance standard BS 6941:2003 or higher | ☐ Yes ☐ No |  |
| 1.3 | compatibility with plate inserts that have size 250x300mm | ☐ Yes ☐ No |  |
| 1.4 | availability of an evacuation strap on the back | ☐ Yes ☐ No |  |
| 1.5 | MOLLE and VELCRO panels on the front side | ☐ Yes ☐ No |  |
| 1.6 | color: blue (preferable)/black or grey | ☐ Yes ☐ No |  |
| 1.7 | availability of a quick-release solution | ☐ Yes ☐ No |  |
| 1.8 | availability of cummerbunds | ☐ Yes ☐ No |  |
| 1.9 | color Blue (preferable)/black or grey | ☐ Yes ☐ No |  |
| 1.10 | modular (protection for neck, and shoulders, detachable. Any level) The plate carrier of the vest has the feature of connecting a collar for a detachable neck protection module and a detachable module for protection of the lower abdomen. | ☐ Yes ☐ No |  |
| 1.11 | Size: adjustable or S, M, L, XL | ☐ Yes ☐ No |  |
| **2** | **General requirements** |  |  |
| 2.1 | All the mentioned equipment should be new. | ☐ Yes ☐ No |  |
| 2.2 | Bid includes brand/model of the goods and manufacturer's technical literature/catalogue, all confirming that the offered items comply with required specifications | ☐ Yes ☐ No |  |
| 2.3 | **Warranty:** at least 1 year | ☐ Yes ☐ No |  |
| 2.4 | Technical documentation for maintenance and repair of the supplied goods. The minimum set of technical documents to be provided with each piece of equipment delivered is the following: • User Manual and Operating Instructions (in Ukrainian or English) • Technical Certificate/maintenance guidelines (in Ukrainian or English) The Bidder is required to confirm the list and contents of documentation to be provided together with the Goods at the delivery. All tags/labels on the equipment shall be in English or Ukrainian language. | ☐ Yes ☐ No |  |
| 2.5 | Bid includes the Country of origin of the goods. | ☐ Yes ☐ No |  |

**C. 3. Delivery requirements for Lot 3**

| **UNOPS Requirements** | |
| --- | --- |
| **Delivery time** | Bidder shall deliver the goods as soon as possible **but not later than 30 days after PO issuance. Please indicate the delivery time in your Quotation**. |
| **Delivery place and Incoterms rules** | DAP Customs cleared Incoterms 2020 (delivered at place) Kyiv, Ukraine, net of any direct taxes, customs duties, or indirect taxes. |
| **Consignee details** | 3rd floor, 15, Yaroslaviv Val str., Kyiv, Ukraine. |
| **Acceptance** | Bidder shall remain liable for the packing and consistency of the items supplied for the period of shipment and acceptance for use. Any items found unacceptable shall be returned and changed at no cost to UNOPS. |
| **Packing standards** | Bidder shall ensure the best international packing standards of goods supplied, including the use of eco-friendly packing materials. |

**D. Inspections and tests**

Any delivered item may on or after delivery be inspected and will be rejected if found not compliant with the requirements of the contract. Such rejected items shall be held at the cost and risk of the supplier who shall, when called upon, remove them immediately at his own cost and forthwith substitute them with items that do comply with the requirements of the contract within 15 (fifteen) working days. Failing such removal, the rejected supplies shall be returned at the supplier's cost.