**Section III: Returnable Bidding Forms**

**eSourcing reference**: ITB/2024/51800

Note to Bidders: The following returnable forms are part of this ITB and must be completed and returned by bidders as part of their quotation. Instructions to complete each Form are highlighted in blue in each Form. Please complete the Returnable Bidding Forms as instructed and return them as part of your quotation by uploading them against their specific Document Checklist in the UNOPS eSourcing system.

**Form A: Joint Venture Partner Information Form**

The Bidder shall fill in this Form in accordance with the instructions indicated below.

ITB reference no: ITB/2024/51800

Name of Bidder: [insert name of bidder]

Date: [insert submission date]

To be completed and returned with your Bid if the Bid is submitted as a Joint Venture/Consortium/Association.

| **JV / Consortium/ Association Information** | |
| --- | --- |
| **Name** | [complete] |
| **Names of each partner and contact information**  (address, telephone numbers, fax numbers, e-mail address) | [complete] |
| **Name of leading** partner (with authority to bind the JV, Consortium, Association during the Bidding process and, in the event a Contract is awarded, during contract execution) | [complete] |
| **Proposed proportion of responsibilities between partners (in %) with indication of the type of the goods/services to be delivered by each** | [complete] |

**Signatures of all partners of the JV:**

We hereby confirm that if the contract is awarded, all parties of the Joint Venture/Consortium/Association shall be jointly and severally liable to UNOPS for the fulfillment of the provisions of the Contract.

Name of partner: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Name of partner: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name of partner: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Name of partner: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Form B: Bid Submission Form**

Bidders are requested to complete this form, sign it and return it as part of their bid submission. The bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.

Date: [Insert submission date]

**Subject: Bid for the Supply and Delivery of Police Boat (10m Inshore Patrol Craft-Catamaran type) with Trailer to the Maritime Police in Kiribati, Nauru, Tuvalu and Vanuatu islands ITB Case No. ITB/2024/51800,**

dated **14 June 2024.**

We, the undersigned, declare that:

* 1. We have examined and have no reservations to the bidding documents, including amendments No.: [Insert the number and issuing date of each amendment];
  2. We offer to supply in conformity with the bidding documents, including the UNOPS General Conditions of Contract, and in accordance with the delivery schedules specified in the Schedule of Requirements
  3. The total price of our bid, excluding any discounts offered in item (d) below, is: [Insert the total bid price in words and figures, indicating the various amounts and the respective currencies];
  4. The discounts offered and the methodology for their application are:
* **Discounts**: If our bid is accepted, the following discounts shall apply. [Specify in detail each discount offered and the specific item of the Schedule of Requirements to which it applies, including if applicable discounts for accelerated payment.]
* **Methodology of application of the discounts**: The discounts shall be applied using the following method: [Specify in detail the method that shall be used to apply the discounts];
  1. Our bid shall be valid for the period of time of [insert number of days which shall not be less than the specified in Section I: ITB Particulars, Period of Validity of Bids] from the date fixed for the bid submission deadline as set out in the ITB, and it shall remain binding upon us and may be accepted at any time before the expiration of that period;
  2. If our bid is accepted, and if so requested in Section I: ITB Particulars, we commit to obtain a performance security in accordance with Instructions to Bidders, Article 34 and the General Conditions of Contract;
  3. We have no conflict of interest in any activity that would put it, if selected for this assignment, in a conflict of interest with UNOPS;
  4. We have not declared bankruptcy, are not involved in bankruptcy or receivership proceedings, and there is no judgment or pending legal action against them that could impair their operations in the foreseeable future;
  5. Our firm confirms that the Bidder and sub-contractors have not been associated, or had been involved in any way, directly or indirectly, with the preparation of the design, terms of references and/or other documents used as a part of this solicitation;
  6. We embrace the principles of the United Nations Supplier Code of Conduct and adhere to the principles of the United Nations Global Compact;
  7. Our firm, its affiliates or subsidiaries—including any subcontractors or suppliers for any part of the contract—has not been declared ineligible by UNOPS, nor is included in the suspended/ineligibility list of the UN/PD, other UN Agencies, the UN Security Council, and the World Bank, in accordance with Instructions to Bidders Article 4, Eligibility;
  8. We have not offered and will not offer fees, gifts and/or favours of kind in exchange for this ITB and will not engage in any such activity during the performance of any contract awarded;
  9. We understand that you are not bound to accept the lowest evaluated bid or any other bid that you may receive.

I, the undersigned, certify that I am duly authorized by [***insert full name of bidder***] to sign this bid and bind [***insert full name of bidder***] should UNOPS accept this bid:

Name : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Title : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

[*Stamp form of bid with official stamp of the bidder*]

# **Form C: Price Schedule Form**

Bidders shall fill in this Price Schedule Form in accordance with the instructions indicated.

ITB reference no: ITB/2024/51800

| **Currency** | USD |
| --- | --- |

| **Item No.** | **Description** | **Qty** | **Currency: USD** | |
| --- | --- | --- | --- | --- |
| **Unit Price**  **DAP, to the specified Island** | **Total Price DAP, to the specified Island** |
| 01 | Supply and Delivery of Police Boat (10m Inshore Patrol Craft-Catamaran type) with Trailer to the Maritime Police in **Kiribati island** | **01** |  |  |
| 02 | Supply and Delivery of Police Boat (10m Inshore Patrol Craft-Catamaran type) with Trailer to the Maritime Police in **Nauru island** | **01** |  |  |
| 03 | Supply and Delivery of Police Boat (10m Inshore Patrol Craft-Catamaran type) with Trailer to the Maritime Police in **Tuvalu island** | **01** |  |  |
| 04 | Supply and Delivery of Police Boat (10m Inshore Patrol Craft-Catamaran type) with Trailer to the Maritime Police in **Vanuatu island** | **01** |  |  |
|  | **Total Cost in USD** | | |  |

Payment terms 15 days accepted: ☐ Yes

**Bidder’s discount for accelerated payment:** \_\_\_\_% of total firm price for each calendar day less than fifteen (15) days

**List of subcontractors or suppliers**

Bidders must identify the names of all subcontractors/suppliers who will be providing goods/services under this Contract and the type of work being subcontracted, if applicable.

1. \_[Full legal name and address of subcontractors]\_\_\_\_\_\_\_\_\_\_\_
2. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

I, the undersigned, certify that I am duly authorized by [***insert full name of Bidder***] to sign this quotation and bind [***insert full name of Bidder***] should UNOPS accept this quotation:

Name : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Title : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Form D: Technical Bid Form**

ITB reference no: ITB/2024/51800

Name of Bidder: [insert name of Bidder]

Bidders are required to complete the **Comparative Data Tables** included in Section II: Schedule of Requirements to demonstrate compliance with UNOPS requirements and insert them below. Bidders are NOT allowed to make any change in the “UNOPS requirements” columns of the Comparative Data Tables. Such changes might disqualify your quotation.

**Supply and Delivery of Police Boat (10m Inshore Patrol Craft-Catamaran type) with Trailer to the Maritime Police in Kiribati, Nauru, Tuvalu and Vanuatu islands**

| **No** | **Minimum Requirements** | **Bidder’s Offer** | | **Remarks** |
| --- | --- | --- | --- | --- |
| **Yes** | **No** |
|  | Make |  |  |  |
|  | Model |  |  |  |
|  | Country of Origin |  |  |  |
| **1** | **General specification - The vessel design must incorporate the following features:** |  |  |  |
| 1.1 | Boat Hull Overall length: 10m | ☐ Yes | ☐ No |  |
| 1.2 | Beam overall: 4m | ☐ Yes | ☐ No |  |
| 1.3 | Draft: 1m | ☐ Yes | ☐ No |  |
| 1.4 | Material: Marine grade Aluminum | ☐ Yes | ☐ No |  |
| 1.5 | Performance Criteria:  Speed (Maximum) > 30.0 kts (at 100% MCR, calm sea, Full Load Displacement)  Range (Minimum) > 150 nm (at 20 knots,in calm sea with 10% fuel reserve (residual fuel based on total tank volume), and with auxiliary engine running) | ☐ Yes | ☐ No |  |
| 1.6 | Bottom sides: 6mm | ☐ Yes | ☐ No |  |
| 1.7 | Topsides: 5mm | ☐ Yes | ☐ No |  |
| 1.8 | Transom: 6mm | ☐ Yes | ☐ No |  |
| 1.9 | Number of people(Basic) : 8 | ☐ Yes | ☐ No |  |
| 1.10 | Vessel must be powered by two 300HP 4-stroke outboard engines (YAMAHA or Equivalent) | ☐ Yes | ☐ No |  |
| 1.11 | Transom Shaft Length: 25'' | ☐ Yes | ☐ No |  |
| 1.12 | The vessel must have a Sillitoe Tartan strip running around the boat beneath the sponson from Port quarter to bow to Starboard quarter. The Sillitoe Tartan to be yellow and blue in color | ☐ Yes | ☐ No |  |
| 1.13 | A Police crest to be positioned on both Port and Starboard sides of the superstructure in consultation with the Principal. | ☐ Yes | ☐ No |  |
| **2** | **Hull** |  |  |  |
| 2.1 | Marine aluminum sheets/profiles (5083 H116) | ☐ Yes | ☐ No |  |
| 2.2 | Welding wire (5183) | ☐ Yes | ☐ No |  |
| 2.3 | Helium/Argon (100%) | ☐ Yes | ☐ No |  |
| 2.4 | Painting (Including primer, intermediate paint, topcoat etc) and the hull and superstructure to be white in color | ☐ Yes | ☐ No |  |
| 2.5 | The word ‘POLICE’ to be in Bold lettering on each side of the hull below the gunwales, black in color.  The name of the vessel to be in Bold lettering on each side of the hull below the gunwales, black in color. | ☐ Yes | ☐ No |  |
| **3** | **Outfitting** |  |  |  |
| 3.1 | Driver seat (Integrated shock-absorbing seat) - 2 sets | ☐ Yes | ☐ No |  |
| 3.2 | Crew seats (Normal Marine grade seats) - 6 pcs | ☐ Yes | ☐ No |  |
| 3.3 | Fender - 1set | ☐ Yes | ☐ No |  |
| 3.4 | Fairlead bollard (Aluminium) - 6pcs | ☐ Yes | ☐ No |  |
| 3.5 | Stern aft engine protection frame (Aluminium) - 1set | ☐ Yes | ☐ No |  |
| 3.6 | Full ship railing (φ25×3) - 1set | ☐ Yes | ☐ No |  |
| 3.7 | Full ship glass (Frame glass) - 1set | ☐ Yes | ☐ No |  |
| 3.8 | Mooring cleat (Aluminum) - 1set | ☐ Yes | ☐ No |  |
| 3.9 | Toilet Room (TMC brand toilet) - 1pcs | ☐ Yes | ☐ No |  |
| 3.10 | Shower - 1pcs | ☐ Yes | ☐ No |  |
| 3.11 | Kitchen area (Stove and sink) - 1set | ☐ Yes | ☐ No |  |
| 3.12 | Refrigerator (Domestic brand 80L ) - 1pcs | ☐ Yes | ☐ No |  |
| 3.13 | Gas Detector - 1 Pcs | ☐ Yes | ☐ No |  |
| 3.14 | Deck (Aluminum Checker plate) - 1set | ☐ Yes | ☐ No |  |
| 3.15 | Fresh water tank (150L Aluminum) - 1set | ☐ Yes | ☐ No |  |
| 3.16 | Black/Grey water (100L Aluminum) - 1set | ☐ Yes | ☐ No |  |
| 3.17 | Sticker | ☐ Yes | ☐ No |  |
| 3.18 | Navigation Mast (Aluminum ) - 1set | ☐ Yes | ☐ No |  |
| **4** | **Propulsion and Steering** |  |  |  |
| 4.1 | Main Engine, 300HP 4-stroke outboard engines (YAMAHA or Equivalent) - 2set | ☐ Yes | ☐ No |  |
| 4.2 | Control System (Electrical Control) - 1set | ☐ Yes | ☐ No |  |
| 4.3 | Fuel tank(cabinet) (2\*800L) - 1 pcs | ☐ Yes | ☐ No |  |
| 4.4 | Electronic liquid level gauge (12V) - 1pcs | ☐ Yes | ☐ No |  |
| 4.5 | Fuel Pipeline (φ16) - 1 batch | ☐ Yes | ☐ No |  |
| 4.6 | Oil filler - (φ50) - 1pcs | ☐ Yes | ☐ No |  |
| 4.7 | vent port (φ50) - 1pcs | ☐ Yes | ☐ No |  |
| 4.8 | Electric bilge pump (12V) - 4set | ☐ Yes | ☐ No |  |
| 4.9 | Hydraulic steering (Seastar Brand) - 1pcs | ☐ Yes | ☐ No |  |
| **5** | **Deck Equipment and Machinery** |  |  |  |
| 5.1 | Anchor (15-20 kgs stainless steel) - 1pcs | ☐ Yes | ☐ No |  |
| 5.2 | Anchor Chain & rope (10m anchor chain 50m anchor rope) - 1set | ☐ Yes | ☐ No |  |
| 5.3 | Electric Winch (1200W ) - 1 pcs | ☐ Yes | ☐ No |  |
| 5.4 | Electric Bilge Pumps (12V) - 5 set | ☐ Yes | ☐ No |  |
| **6** | **Lighting** |  |  |  |
| 6.1 | Navigation Lights - 2pcs  (Navigation lights placement to comply with International Regulations for preventing collisions at sea – COLREGS) | ☐ Yes | ☐ No |  |
| 6.2 | Internal Cabin Lighting - 6pcs  (Cabin lighting must have option for red or white light for night time operation) | ☐ Yes | ☐ No |  |
| 6.3 | Curtesy Light in the cockpit - 1 set  (Curtesy lighting must have option for red or white light for night time operation) | ☐ Yes | ☐ No |  |
| 6.4 | Flood lights - 2pcs  (Mounted on the top aft of the cabin, positioned to provide lighting overboard or to another vessel alongside) | ☐ Yes | ☐ No |  |
| 6.5 | Blue Strobe Flashing Police lights - 2pcs  (Mounted on the mast, and visible all round) | ☐ Yes | ☐ No |  |
| 6.6 | 12/24V LED Search light - 1pcs  (fixed mounted, with remote electric control located in the wheelhouse) | ☐ Yes | ☐ No |  |
| 6.7 | Anchor light - 1pcs | ☐ Yes | ☐ No |  |
| **7** | **Electrical** |  |  |  |
| 7.1 | All electronics must be integrated systems through NMEA or N2K standardization | ☐ Yes | ☐ No |  |
| 7.2 | 16''Multifunction display (MFD) with GPS (Garmin or equivalent ) - 1 set | ☐ Yes | ☐ No |  |
| 7.3 | GPS Antenna - 1set | ☐ Yes | ☐ No |  |
| 7.4 | Radar(24'' Radome 4kw) (Garmin or equivalent) - 1 set | ☐ Yes | ☐ No |  |
| 7.5 | 1kw through hull transducer (SS164 Lawrance or equivalent) - 1set | ☐ Yes | ☐ No |  |
| 7.6 | CMAP Charter for Pacific- 1set | ☐ Yes | ☐ No |  |
| 7.7 | 12'' MFD mounted at the navigation console (Garmin or equivalent) - 1 set | ☐ Yes | ☐ No |  |
| 7.8 | AIS Class A Tx Transponder (Furuno FA-170 or equivalent) - 1set | ☐ Yes | ☐ No |  |
| 7.9 | VHF Radio (GX1400 or equivalent) - 1set | ☐ Yes | ☐ No |  |
| 7.10 | VHF Antenna (GX1400 or equivalent) - 1set | ☐ Yes | ☐ No |  |
| 7.11 | Compass - 1pcs | ☐ Yes | ☐ No |  |
| 7.12 | 12V or 24V DC electrical system - 1set | ☐ Yes | ☐ No |  |
| 7.13 | Shore Power - 1set | ☐ Yes | ☐ No |  |
| 7.14 | Marine Air Conditions (11000 BTU 24W ) - 1set | ☐ Yes | ☐ No |  |
| 7.15 | Thermal Imaging system (FLIR M232or equivalent) - 1set | ☐ Yes | ☐ No |  |
| 7.16 | AM/FM Radio - 1set | ☐ Yes | ☐ No |  |
| 7.17 | 120W Marine speakers - 2pcs | ☐ Yes | ☐ No |  |
| **8** | **Safety Equipment** |  |  |  |
| 8.1 | EPIRB - 1set  (emergency procedure resource kit- Capsize bottle complete) | ☐ Yes | ☐ No |  |
| 8.2 | Life jacket - 8 pcs | ☐ Yes | ☐ No |  |
| 8.3 | Life Buoy - 1pcs | ☐ Yes | ☐ No |  |
| 8.4 | First Aid Kit - 1set | ☐ Yes | ☐ No |  |
| 8.5 | Distress flares - 6pcs | ☐ Yes | ☐ No |  |
| 8.6 | Waterproof Floating Torch - 2pcs | ☐ Yes | ☐ No |  |
| **9** | **Spare Parts** |  |  |  |
| 9.1 | Engine service kits - 12pcs | ☐ Yes | ☐ No |  |
| 9.2 | stainless steel propellers - 2 sets | ☐ Yes | ☐ No |  |
| 9.3 | Hull repair kits - 2 sets | ☐ Yes | ☐ No |  |
| 9.4 | 1 spare engine battery - 1pcs | ☐ Yes | ☐ No |  |
| **10** | **Boat tow Trailer** |  |  |  |
| 10.1 | Trailer Construction: The trailer should be constructed from high-strength, corrosion-resistant materials (e.g., galvanized steel or marine-grade aluminum) to withstand harsh marine environments. | ☐ Yes | ☐ No |  |
| 10.2 | The frame should be reinforced to ensure durability and safety during transport. | ☐ Yes | ☐ No |  |
| 10.3 | The trailer must include a customized cradle specifically designed to fit the Boat. | ☐ Yes | ☐ No |  |
| 10.4 | The cradle should provide secure support for the hull, minimizing movement during transport and preventing damage | ☐ Yes | ☐ No |  |
| 10.5 | The trailer should be equipped with a robust braking system, including hydraulic or electric brakes for enhanced safety | ☐ Yes | ☐ No |  |
| 10.6 | A breakaway system should be installed to automatically engage the brakes if the trailer becomes detached from the towing vehicle | ☐ Yes | ☐ No |  |
| 10.7 | The trailer must feature a compatible towing hitch and coupling system designed to attach securely to the towing vehicle | ☐ Yes | ☐ No |  |
| 10.8 | The hitch should be rated for the trailer's maximum weight capacity and include a safety lock mechanism | ☐ Yes | ☐ No |  |
| 10.9 | The trailer should have multiple axles with appropriate suspension systems to ensure smooth and stable transportation of the Boat | ☐ Yes | ☐ No |  |
| 10.10 | Heavy-duty tires suitable for various terrains should be installed. | ☐ Yes | ☐ No |  |
| 10.11 | Multiple tie-down points should be provided on the trailer to securely fasten the Boat during transp | ☐ Yes | ☐ No |  |
| 10.12 | High-strength tie-down straps or ratchets should be included to ensure the Boat remains secure | ☐ Yes | ☐ No |  |
| **11** | **Others** |  |  |  |
| 11.1 | Lloyd drawing certificate/ National Standard for Commercial Vessels (NSCA) or equivalent certificate | ☐ Yes | ☐ No |  |
| 11.2 | Lloyd Boat Certificate or equivalent certificate | ☐ Yes | ☐ No |  |

**Delivery Requirements and Comparative Data Table:**

| **UNOPS Requirements** | | **Is quotation compliant?** Bidder to complete | **Details**  Bidder to complete |
| --- | --- | --- | --- |
| **Delivery time** | Bidder shall deliver the goods within Eight (08) months after Contract signature. | ☐ Yes ☐ No | Insert details |
| **Incoterm applicable** | **DAP Incoterms**  Maritime Police in Kiribati, Nauru, Tuvalu and Vanuatu islands | ☐ Yes ☐ No | Insert details |
| **Consignee details** | Will be confirmed at the time of the Contract issuance stage. | ☐ Yes ☐ No | Insert details |
| **UNOPS Right to vary requirements** | At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- 20%, without any change in the unit prices or other terms and conditions of the ITB. | ☐ Yes ☐ No | Insert details |

**Inspections and tests**

The following inspections and tests shall be performed,

The manufacturer should provide the Lloyd drawing certificate and Lloyd Boat Certificate or equivalent certificates.

The offered goods and related services (if applicable) are in accordance with the required specifications and requirements specified in **Section II: Schedule of Requirements**.

☐ Yes ☐ No

ANY DEVIATION MUST BE LISTED BELOW:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Title : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# **Form E: Previous Experience Form**

ITB reference no: ITB/2024/51800

Name of Bidder: [insert name of Bidder]

| **Order placed by (Full address of purchaser)** | **Order no & date** | **Description & quantity of ordered items** | **Value of Order** | **Date of completion of Delivery as per Contract** | **Remarks indicating reasons of late delivery, if any** |
| --- | --- | --- | --- | --- | --- |
|
|  |  |  |  |  | Name:  eMail :  Phone: |
|  |  |  |  |  | Name:  eMail :  Phone: |
|  |  |  |  |  | Name:  eMail :  Phone: |
|  |  |  |  |  | Name:  eMail :  Phone: |

**NOTE: Please list minimum 3 completed contract details in supplying the same products (Inshore patrol boat) or similar products during the last 3 Years. It can be for the UN / Government / Non Government/ Private Sector, etc.**

Name : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Title : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Form F- Manufacturer’s Authorization Form**

A letter issued by the manufacturer authorizing the applicant to participate in this particular RFQ must be submitted with the bid in the format provided in this Form.

To be eligible for delivery of goods, the bidder must be either the manufacturer of the offered goods or a sole representative of the manufacturer to the United Nations. Should offers for a particular make and model be received from more than one appointed representative, UNOPS reserves the right to select only one.

ITB reference no: ITB/2024/51800

Name of Bidder: [insert name of bidder]

Date: [insert submission date]

To: UNOPS

**WHEREAS**

We ***[insert complete name of manufacturer***], who are official manufacturers of [***insert type of goods manufactured],*** having factories at ***[insert full address of manufacturer’s factories***], do hereby authorize ***[insert complete name of bidder]*** to submit a quotation for the purpose of which is to provide the following goods, manufactured by us ***[insert name and or brief description of the goods]***, and to subsequently negotiate and sign the contract.

We hereby extend our full guarantee and warranty in accordance with Clause 4.5 of the General Conditions of Contract for the provision of Goods, with respect to the goods offered by the above firm.

Signed: [***insert signature(s) of authorized representative(s) of the manufacturer]***

Name***: [insert complete name(s) of authorized representative(s) of the manufacturer]***

Title: ***[insert title]***

Dated on \_\_\_\_\_\_\_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_\_\_\_\_\_ ***[insert date of signing]***