OTS-24 - Stethoscope

**Description**

*Device to listen to adult patient heart and lungs sound*

**Reference Picture**

*Note: The images below are intended solely as a guiding support and should be considered as purely indicative and not restrictive of the expected item characteristics*



| Brand / Marque | |  | |
| --- | --- | --- | --- |
| Model / Modèle | |  | |
| Model code as per manufacturer classification / Numéro de référence du produit fournisseur | |  | |
| Manufacturer name / Nom du Fabricant | |  | |
| Manufacturing site / Site du Fabricant | |  | |
| Country of manufacturing / Pays de fabrication | |  | |
| Country of origin / Pays d'origine | |  | |

|  | **UNOPS Minimum technical requirements // Exigences techniques minimales de l'UNOPS** | **Complies (Yes/No) // Conforme (Oui/Non)** | **Comments/ Technical data //**  **Commentaires/Données techniques** |
| --- | --- | --- | --- |
| **A** | **Functionality and Performance / Fonctionnalité et performances** |  |  |
| 1 | For the auscultation of high and low frequency tones. |  |  |
| 2 | Combined double chest piece: combined bell and diaphragm |  |  |
| 3 | Stainless steel chestpiece. |  |  |
| 4 | Arms with a flexible spring: stainless steel, anodized aluminum, chrome-plated or similar material corrosion resistant. |  |  |
| 5 | Diaphragm diameter: at least 40 mm. |  |  |
| 6 | PVC or similar material stethoscope tubing, double lumen. |  |  |
| 7 | Length at least 540 mm. |  |  |
| 8 | Removable silicone (or similar material) earpieces. |  |  |
| 9 | All materials latex-free. |  |  |
| 10 | All materials are corrosion resistant and cleanable with hospital grade disinfectants. |  |  |
|  | **Accessories included in the offered price** |  |  |
| 1 | One (1) Storage case. |  |  |
| 2 | One (1) spare adult diaphragm, additional to that included in the device. |  |  |
| 3 | Ten (10) sets spare earpieces, additional to those included in the device. |  |  |
| **B** | **Certifications and post sales included in the offered price** |  |  |
| 1 | The Supplier, included in the offered price, will provide the post sales services described in the document “OT-PS Type I post sales requirements for Medical Devices”. |  |  |
| C | **Supplied with** |  |  |
| 1 | Detailed step-by-step instructions for assembly, use and cleaning in pictograms. |  |  |
| **D** | **ANY DEVIATIONS OR SUPERIOR CHARACTERISTICS MUST BE INDICATED BELOW // TOUTE DÉVIATION OU CARACTÉRISTIQUE SUPÉRIEURE DOIT ÊTRE INDIQUÉE CI-DESSOUS\* :** | | |
|  | | |