OTI-06 - Cesarean section box

**Description**

*Complete set of surgery instruments for cesarean section*

**Reference Pictures at the end of this document as part of Annex 1**.

| Brand / Marque | |  | |
| --- | --- | --- | --- |
| Model / Modèle | |  | |
| Model code as per manufacturer classification / Numéro de référence du produit fournisseur | |  | |
| Manufacturer name / Nom du Fabricant | |  | |
| Manufacturing site / Site du Fabricant | |  | |
| Country of manufacturing / Pays de fabrication | |  | |
| Country of origin / Pays d'origine | |  | |

|  | **UNOPS Minimum technical requirements // Exigences techniques minimales de l'UNOPS** | **Complies (Yes/No) // Conforme (Oui/Non)** | **Comments/ Technical data //**  **Commentaires/Données techniques** |
| --- | --- | --- | --- |
| **A** | **Functionality and Performance / Fonctionnalité et performances** |  |  |
| 1 | Made of high grade medical Stainless Steel AISI 316 grade, clearly identifying the grade of steel used in the manufacture of the instruments, in accordance with ISO 7153-1: 2016, DIN 58298, ASTM F899 or an equivalent standard. |  |  |
| 2 | Non-sterile, reusable instruments. |  |  |
| 3 | Can be autoclaved at 134ºC |  |  |
| 4 | Please note that the ranges and dimensions shown below are approximate. They may vary from brand to brand. |  |  |
| 5 | Complete set of surgery instruments for cesarean section contains all the items contained in the Annex 1 (Description must be included in column “Comments/ Technical data // Commentaires/Données techniques” for each item) |  |  |
| **B** | **Certifications and post sales included in the offered price** |  |  |
| 1 | The Supplier, included in the offered price, will provide the post sales services described in the document “OT-PS Type I post sales requirements for Medical Devices”. |  |  |
| C | **Supplied with** |  |  |
| 1 | Detailed step-by-step instructions for cleaning and disinfection, preferably using pictograms and Lubricating agents where necessary for maintenance.. |  |  |
| **D** | **ANY DEVIATIONS OR SUPERIOR CHARACTERISTICS MUST BE INDICATED BELOW // TOUTE DÉVIATION OU CARACTÉRISTIQUE SUPÉRIEURE DOIT ÊTRE INDIQUÉE CI-DESSOUS\* :** | | |
|  | | |

**Annex 1 - Box composition**


1. **Sterilization container**: for sterilization of surgical instruments, with perforated lid, perforated button and clip lock. Reference dimension (Length x width x height): 300X274X247 mm. Size 1/2.
2. **Surgery Instrumentation:**

| **Item** | **Description** | **Detail** | **Reference Dimensions** | **Nr of units** | **Complies (Yes/No) // Conforme (Oui/Non)** | **Comments/ Technical data //**  **Commentaires/Données techniques** |
| --- | --- | --- | --- | --- | --- | --- |
| 6.1 | Bengolea forceps | AG | 18cm | 3 |  |  |
| 6.2 | Bengolea curved forceps | SG | 16cm | 3 |  |  |
| 6.3 | O’Shaugnessy dissecting forceps |  | 23cm | 1 |  |  |
| 6.4 | Kelly forceps | Straight | 16cm | 3 |  |  |
| 6.5 | Kelly forceps | Curved | 16cm | 3 |  |  |
| 6.6 | Dissecting forceps | SG | 18cm | 1 |  |  |
| 6.7 | Dissecting forceps | AG | 18cm | 1 |  |  |
| 6.8 | Dissecting forceps | SG | 25cm | 1 |  |  |
| 6.9 | Dissecting forceps | AG | 25cm | 1 |  |  |
| 6.10 | Mayo scissors | Straight | 18cm | 1 |  |  |
| 6.11 | Mayo scissors | Curved | 18cm | 1 |  |  |
| 6.12 | Metzenbaum scissors | Curved | 26cm | 1 |  |  |
| 6.13 | Mayo-Hegar needle holder |  | 20cm | 1 |  |  |
| 6.14 | Koche forceps | AG | 14cm | 6 |  |  |
| 6.15 | Kelly valve |  | 19 x 3,8cm | 1 |  |  |
| 6.16 | Backhaus forceps |  | 14cm | 6 |  |  |
| 6.17 | Dartigues hysterolabe |  |  | 1 |  |  |
| 6.18 | Gosset GM retractor | 3 valves |  | 1 |  |  |
| 6.19 | Farabeuf retractor (pair) |  | 15cm | 1 |  |  |
| 6.20 | Allis forceps |  | 19cm | 2 |  |  |
| 6.21 | Scalpel handle | N°4 |  | 1 |  |  |
| 6.22 | Scalpel handle | N°3 |  | 1 |  |  |
| 6.23 | Instrument pins |  | 18cm | 2 |  |  |
| 6.24 | Bowl |  | 80ml | 1 |  |  |
| 6.25 | Bowl |  | 500ml | 1 |  |  |
| 6.26 | Cotte self-static retractor |  |  | 1 |  |  |
| 6.27 | Rezzano clamp |  |  | 1 |  |  |
| 6.28 | JL Faures clamps |  |  | 2 |  |  |

**Reference Picture:**

*Note: The images below are intended solely as a guiding support and should be considered as purely indicative and not restrictive of the expected item characteristics*


*Item 5:*

**

*Item 6.1:*

**

*Item 6.2:*

**

*Item 6.3:*

  
]

*Item 6.4*



*Item 6.5*

**

*Item 6.6*

**

*Item 6.7*

**

*Item 6.8*

**

*Item 6.9*



*Item 6.10*

**

*Item 6.11*

**

*Item 6.12*

**


*Item 6.13*

**

*Item 6.14*

**


*Item 6.15*

**

*Item 6.16*

**

*Item 6.17*

**

*Item 6.18*

**

*Item 6.19*

**

*Item 6.20*

**

*Item 6.21*

**

*Item 6.22*

**

*Item 6.23*

**

*Item 6.24*

**

*Item 6.25*

**

*Item 6.26*

**

*Item 6.27*



*Item 6.28*

**