OTI-11 - Small surgery box

**Description**

*Complete set of instruments for complete minor surgery*

**Reference Pictures at the end of this document as part of Annex 1**.

| Brand / Marque | |  | |
| --- | --- | --- | --- |
| Model / Modèle | |  | |
| Model code as per manufacturer classification / Numéro de référence du produit fournisseur | |  | |
| Manufacturer name / Nom du Fabricant | |  | |
| Manufacturing site / Site du Fabricant | |  | |
| Country of manufacturing / Pays de fabrication | |  | |
| Country of origin / Pays d'origine | |  | |

|  | **UNOPS Minimum technical requirements // Exigences techniques minimales de l'UNOPS** | **Complies (Yes/No) // Conforme (Oui/Non)** | **Comments/ Technical data //**  **Commentaires/Données techniques** |
| --- | --- | --- | --- |
| **A** | **Functionality and Performance / Fonctionnalité et performances** |  |  |
| 1 | Made of high grade medical Stainless Steel AISI 316 grade, clearly identifying the grade of steel used in the manufacture of the instruments, in accordance with ISO 7153-1: 2016, DIN 58298, ASTM F899 or an equivalent standard. |  |  |
| 2 | Non-sterile, reusable instruments. |  |  |
| 3 | Can be autoclaved at 134ºC |  |  |
| 4 | Please note that the ranges and dimensions shown below are approximate. They may vary from brand to brand. |  |  |
| 5 | Complete set of surgery instruments for cesarean section contains all the items contained in the Annex 1 (Description must be included in column “Comments/ Technical data // Commentaires/Données techniques” for each item) |  |  |
| **B** | **Certifications and post sales included in the offered price** |  |  |
| 1 | The Supplier, included in the offered price, will provide the post sales services described in the document “OT-PS Type I post sales requirements for Medical Devices”. |  |  |
| C | **Supplied with** |  |  |
| 1 | Detailed step-by-step instructions for cleaning and disinfection, preferably using pictograms and Lubricating agents where necessary for maintenance.. |  |  |
| **D** | **ANY DEVIATIONS OR SUPERIOR CHARACTERISTICS MUST BE INDICATED BELOW // TOUTE DÉVIATION OU CARACTÉRISTIQUE SUPÉRIEURE DOIT ÊTRE INDIQUÉE CI-DESSOUS\* :** | | |
|  | | |

**Annex 1 - Box composition**

1. **Sterilization container:** for sterilization of surgical instruments, with lid, perforated. Reference dimension (Length x width x height): 250X100X50 mm.
2. **Surgery Instrumentation:**

| **Item** | **Description** | **Detail** | **Reference Dimensions** | **Nr of units** | **Complies (Yes/No) // Conforme (Oui/Non)** | **Comments/ Technical data //**  **Commentaires/Données techniques** |
| --- | --- | --- | --- | --- | --- | --- |
| 6.1 | Dissecting forceps. | SG | 14cm | 1 |  |  |
| 6.2 | Dissecting forceps. | AG | 14cm | 1 |  |  |
| 6.3 | Péan forceps. |  | 14cm | 1 |  |  |
| 6.4 | Scissors | Straight | 14cm | 1 |  |  |
| 6.5 | Scalpel handle. |  | N°3 | 1 |  |  |
| 6.6 | Scalpel handle. |  | N°4 | 1 |  |  |
| 6.7 | Halstead haemostatic forceps. | SG curved / straight | 12,5cm | 2 |  |  |
| 6.8 | Scissors. | Straight with pointed tips | 14cm | 1 |  |  |
| 6.9 | Kocher forceps. | Straight, AG | 18cm | 1 |  |  |
| 6.10 | Kocher forceps. | Straight, SG | 18cm | 1 |  |  |
| 6.11 | Mayo Hégar needle holder. |  | 14cm | 1 |  |  |
| 6.12 | Grooved probe |  |  | 1 |  |  |
| 6.13 | Metzebaum scissors 2 |  | 20,3cm | 1 |  |  |

**Reference Picture:**

*Note: The images below are intended solely as a guiding support and should be considered as purely indicative and not restrictive of the expected item characteristics*

*Item 5:*

**

*Item 6.1:*

**

*Item 6.2:*

**

*Item 6.3:*

**

*Item 6.4:*

**

*Item 6.5:*

**

*Item 6.6:*

**

*Item 6.7:*

**

*Item 6.8:*

**

*Item 6.9:*

**

*Item 6.10:*

**

*Item 6.11:*

**

*Item 6.12:*

**

*Item 6.13:*

**

**Supplied with:**

Detailed step-by-step instructions for cleaning and disinfection, preferably using pictograms and Lubricating agents where necessary for maintenance.

**Post sales services requirement**

The Supplier, included in the offered price, will provide the post sales services described in the document “*OT-PS Type I post sales requirements for Medical Devices*”.