OTI-08 - Hysterectomy box

**Description**

*Complete set of instruments for hysterectomy*

**Reference Pictures at the end of this document as part of Annex 1**.

| Brand / Marque | |  | |
| --- | --- | --- | --- |
| Model / Modèle | |  | |
| Model code as per manufacturer classification / Numéro de référence du produit fournisseur | |  | |
| Manufacturer name / Nom du Fabricant | |  | |
| Manufacturing site / Site du Fabricant | |  | |
| Country of manufacturing / Pays de fabrication | |  | |
| Country of origin / Pays d'origine | |  | |

|  | **UNOPS Minimum technical requirements // Exigences techniques minimales de l'UNOPS** | **Complies (Yes/No) // Conforme (Oui/Non)** | **Comments/ Technical data //**  **Commentaires/Données techniques** |
| --- | --- | --- | --- |
| **A** | **Functionality and Performance / Fonctionnalité et performances** |  |  |
| 1 | Made of high grade medical Stainless Steel AISI 316 grade, clearly identifying the grade of steel used in the manufacture of the instruments, in accordance with ISO 7153-1: 2016, DIN 58298, ASTM F899 or an equivalent standard. |  |  |
| 2 | Non-sterile, reusable instruments. |  |  |
| 3 | Can be autoclaved at 134ºC |  |  |
| 4 | Please note that the ranges and dimensions shown below are approximate. They may vary from brand to brand. |  |  |
| 5 | Complete set of surgery instruments for cesarean section contains all the items contained in the Annex 1 (Description must be included in column “Comments/ Technical data // Commentaires/Données techniques” for each item) |  |  |
| **B** | **Certifications and post sales included in the offered price** |  |  |
| 1 | The Supplier, included in the offered price, will provide the post sales services described in the document “OT-PS Type I post sales requirements for Medical Devices”. |  |  |
| C | **Supplied with** |  |  |
| 1 | Detailed step-by-step instructions for cleaning and disinfection, preferably using pictograms and Lubricating agents where necessary for maintenance.. |  |  |
| **D** | **ANY DEVIATIONS OR SUPERIOR CHARACTERISTICS MUST BE INDICATED BELOW // TOUTE DÉVIATION OU CARACTÉRISTIQUE SUPÉRIEURE DOIT ÊTRE INDIQUÉE CI-DESSOUS\* :** | | |
|  | | |

**Annex 1 - Box composition**


1. **Sterilization container:** for sterilization of surgical instruments, with perforated lid, perforated button and clip lock. Reference dimension (Length x width x height): 500X200X120 mm.
2. **Surgery Instrumentation:**

| **Item** | **Description** | **Detail** | **Reference Dimensions** | **Nr of units** | **Complies (Yes/No) // Conforme (Oui/Non)** | **Comments/ Technical data //**  **Commentaires/Données techniques** |
| --- | --- | --- | --- | --- | --- | --- |
| 6.1 | Mayo-Harrington Dissecting Scissors | Straight | 22,5 cm | 1 |  |  |
| 6.2 | Nelson- Metzenbaum Dissecting Scissors | Curved | 25 cm | 1 |  |  |
| 6.3 | Wertheim Scissors | Curved | 22,5 cm | 1 |  |  |
| 6.4 | Yankauer Suction Cannula |  | 27 cm | 1 |  |  |
| 6.5 | Heywood-Smith Polyp Forceps |  | 20 cm | 1 |  |  |
| 6.6 | Dartigues Elevating Forceps |  | 25,5 cm | 1 |  |  |
| 6.7 | Kocher-Ochsner Forceps | 1x2 Teeth Curved | 16 cm | 4 |  |  |
| 6.8 | Kocher-Ochsner Forceps | 1x2 Teeth Straight | 16 cm | 4 |  |  |
| 6.9 | Backhaus Towel Clamp |  | 15 cm | 4 |  |  |
| 6.10 | Doyen Intestinal Forceps | Straight | 23 cm | 2 |  |  |
| 6.11 | Museux Tenaculum Forceps | 6mm | 24 cm | 1 |  |  |
| 6.12 | Dissecting Forceps | straight, toothless | 20 cm | 1 |  |  |
| 6.13 | Dissecting Forceps | 1X2 teeth | 20 cm | 1 |  |  |
| 6.14 | Guyon Clamp | Curved | 23 cm | 1 |  |  |
| 6.15 | Doyen Vaginal Speculum | Blade 75x45 mm |  | 1 |  |  |
| 6.16 | Doyen Vaginal Speculum | Blade 90x45 mm |  | 1 |  |  |
| 6.17 | Doyen Vaginal Speculum | Blade 110x45 mm |  | 1 |  |  |
| 6.18 | Kelly Retractor | Blade 190x38 mm |  | 1 |  |  |
| 6.19 | Kelly Retractor | Blade 190x57 mm |  | 1 |  |  |
| 6.20 | Gosset Abdominal Retractor | Set Complete |  | 1 |  |  |

**Reference Picture:**

*Note: The images below are intended solely as a guiding support and should be considered as purely indicative and not restrictive of the expected item characteristics*


*Item 5:*

**


*Item 6.1:*

**

*Item 6.2:*




*Item 6.3:*

**


*Item 6.4:*

**


*Item 6.5:*




*Item 6.6:*

**

*Item 6.7:*

**


*Item 6.8:*

**


*Item 6.9:*

**

*Item 6.10:*

**

*Item 6.11:*

**


*Item 6.12:*




*Item 6.13:*



*Item 6.14:*

**


*Item 6.15, 6.16 & 6.17*

**

*Item 6.18 & 6.19*

**

*Item 6.20:*

**