**Section II: Schedule of Requirements**

| UNOPS E-Sourcing RFQ/2024/53619 |
| --- |

1. **Summary of Requirements for provision of modular vests, helmets, and plate carriers.**

**UNOPS requirements are comprised of the following 3 (three) lots:**

**Lot 1 - Tactical armor carriers with main ballistic panels (removable), side protection, and detachable protection for groin**

**Lot 2 - Low-cut ballistic helmet**

**Lot 3 - Tactical armor carriers (without removable main ballistic panels), with side protection and detachable protection for groin**

1. **Requirements and technical specifications.**

**Lot 1 - Tactical armor carriers with main ballistic panels (removable), side protection, and detachable protection for groin**

| **N** | **UNOPS minimum technical requirements** |
| --- | --- |
| **1** | **Tactical armor carriers with removable ballistic panels, side protection, and detachable protection for groin** |
| 1.1 | Main ballistic panels are classified as hard armor panels |
| 1.2 | **Provide certificate that main ballistic panels have a rated level of protection “Type IV” in accordance with NIJ Standard 0101.06 or level of protection “6” in accordance with DSTU 8782:2018** |
| 1.3 | Main ballistic panels are classified as stand-alone panels |
| 1.4 | Main ballistic panels have curved shape |
| 1.5 | Main ballistic panels are lightweight (weight ranges from 4 pounds (1.8 kg) to 11.5 pounds (5 kg) depending on size) |
| 1.6 | Tactical armor carriers should be designed for use with removable main ballistic panels |
| 1.7 | Tactical armor carriers are compatible with main ballistic panels that have rated level of protection “Type IV” in accordance with NIJ Standard 0101.06 or level of protection “6” in accordance with DSTU 8782:2018 |
| 1.8 | Tactical armor carriers are compatible with main ballistic panels that have size 250x300mm |
| 1.9 | Tactical armor carriers have evacuation straps (emergency drag handles) on the rear side |
| 1.10 | Tactical armor carriers have VELCRO panels on the front and rear sides |
| 1.11 | Tactical armor carriers have MOLLE panels on the front and rear sides |
| 1.12 | Tactical armor carriers have a quick-release solution |
| 1.13 | Tactical armor carriers have at least 4 adjustment points (one on each shoulder and one on each side in the lower part of a plate carrier) |
| 1.14 | Tactical armor carriers have internal mesh lining to improve ventilation |
| 1.15 | Tactical armor carriers (without main ballistic panels, side, groin, and neck protection) are lightweight (not more than 2 kg). |
| 1.16 | Tactical armor carriers are made in one of the following colors: blue (preferable), black, or grey |
| 1.17 | Tactical armor carriers are made in the following sizes: S, M, L, and XL |
| 1.18 | Tactical armor carriers have side protection |
| 1.19 | Side protection has a rated level of protection “Type IIIa” in accordance with NIJ Standard 0101.06or level of protection “2” in accordance with DSTU 8782:2018 |
| 1.20 | Tactical armor carriers have detachable groin protection |
| 1.21 | Detachable groin protection has a rated level of protection “Type IIIa” in accordance with NIJ Standard 0101.06or level of protection “2” in accordance with DSTU 8782:2018 |
| 1.22 | Tactical armor carriers have flame resistance - any (preferable according to standard BS 6941:2003) |
| **2** | **General requirements** |
| 2.1 | All the mentioned equipment should be new. |
| 2.2 | Bid includes the brand/model of the goods and the manufacturer's technical literature/catalog, all confirming that the offered items comply with the required specifications |
| 2.3 | **Warranty:** at least soft armor 5 years and for hard armor 10 years, carrier at least 1 year |
| 2.4 | Technical documentation for maintenance and repair of the supplied goods. The minimum set of technical documents to be provided with each piece of equipment delivered is the following: • User Manual and Operating Instructions (in Ukrainian or English) • Technical Certificate/maintenance guidelines (in Ukrainian or English) The Bidder is required to confirm the list and contents of documentation to be provided together with the Goods at the delivery. All tags/labels on the equipment shall be in English or Ukrainian language. |
| 2.5 | Bid includes the Country of origin of the goods. |

**C. 1. Delivery requirements for Lot 1**

| **UNOPS Requirements** | |
| --- | --- |
| **Delivery time** | Bidder shall deliver the goods as soon as possible **but not later than 30 days after PO issuance. Please indicate the delivery time in your Quotation**. |
| **Delivery place and Incoterms rules** | DAP Customs cleared Incoterms 2020 (delivered at place) Kyiv, Ukraine, net of any direct taxes, customs duties, or indirect taxes. |
| **Consignee details** | 2nd floor, 9B, Mykhaila Hrushevskoho str., BC SUMMIT, Kyiv, Ukraine. |
| **Acceptance** | Bidder shall remain liable for the packing and consistency of the items supplied for the period of shipment and acceptance for use. Any items found unacceptable shall be returned and changed at no cost to UNOPS. |
| **Packing standards** | Bidder shall ensure the best international packing standards of goods supplied, including the use of eco-friendly packing materials. |

**Lot 2 - Low-cut ballistic helmet**

| **N** | **UNOPS minimum technical requirements** |
| --- | --- |
| **1** | **Low-cut ballistic helmet with rated level of protection “Type IIIa” (in accordance with NIJ Standard 0106.01) or level of protection “1” (or higher) in accordance with DSTU 8835:2019** |
| 1.1 | Ballistic helmet is made from Kevlar (preferable), aramid or ultrahigh molecular weight polyethylene |
| 1.2 | **Provide a certificate that the ballistic helmet has a rated level of protection “Type IIIa” in accordance with NIJ Standard 0106.01 (modified) or level of protection “1” (or higher) in accordance with DSTU 8835:2019** |
| 1.3 | Ballistic helmet has one of the following designs: PASGT, MICH, ACH, or ECH |
| 1.4 | Ballistic helmet provides coverage “low cut” |
| 1.5 | Ballistic helmet has at least 4 points suspension system |
| 1.6 | Harness system of the ballistic helmet has a quick-release buckle |
| 1.7 | Ballistic helmet is compatible with gas masks and communication devices (any type) |
| 1.8 | Ballistic helmet is made in one of the following colors: blue (preferable) or black |
| 1.9 | Ballistic helmet has VELCRO panels |
| 1.10 | Preferable: ballistic helmet has two side accessory rails, one per side |
| 1.11 | Ballistic helmet has internal padding for comfort |
| 1.12 | Ballistic helmets are offered in the following sizes: S, M, L, XL |
| 1.13 | The weight of the ballistic helmet is 1.45 - 1.75 kg, depending on the size. |
| **2** | **General requirements** |
| 2.1 | All the mentioned equipment should be new. |
| 2.2 | Bid includes the brand/model of the goods and the manufacturer's technical literature/catalog, all confirming that the offered items comply with the required specifications |
| 2.3 | **Warranty:** at least 5 years (ballistic warranty), 1 year (parts warranty) |
| 2.4 | Technical documentation for maintenance and repair of the supplied goods. The minimum set of technical documents to be provided with each piece of equipment delivered is the following: • User Manual and Operating Instructions (in Ukrainian or English) • Technical Certificate/maintenance guidelines (in Ukrainian or English) The Bidder is required to confirm the list and contents of documentation to be provided together with the Goods at the delivery. All tags/labels on the equipment shall be in English or Ukrainian language. |
| 2.5 | Bid includes the Country of origin of the goods. |

**C. 2. Delivery requirements for Lot 2**

| **UNOPS Requirements** | |
| --- | --- |
| **Delivery time** | Bidder shall deliver the goods as soon as possible **but not later than 30 days after PO issuance. Please indicate the delivery time in your Quotation**. |
| **Delivery place and Incoterms rules** | DAP Customs cleared Incoterms 2020 (delivered at place) Kyiv, Ukraine, net of any direct taxes, customs duties, or indirect taxes. |
| **Consignee details** | 2nd floor, 9B, Mykhaila Hrushevskoho str., BC SUMMIT, Kyiv, Ukraine. |
| **Acceptance** | Bidder shall remain liable for the packing and consistency of the items supplied for the period of shipment and acceptance for use. Any items found unacceptable shall be returned and changed at no cost to UNOPS. |
| **Packing standards** | Bidder shall ensure the best international packing standards of goods supplied, including the use of eco-friendly packing materials. |

**Lot 3 - Tactical armor carriers (without removable main ballistic panels), with side protection and detachable protection for groin**

| **N** | **UNOPS minimum technical requirements** |
| --- | --- |
| **1** | **Tactical armor carriers (without removable main ballistic panels), with side protection and detachable protection for groin** |
| 1.1 | Tactical armor carriers should be designed for use with removable main ballistic panels |
| 1.2 | Tactical armor carriers are compatible with main ballistic panels that have rated level of protection “Type IV” in accordance with NIJ Standard 0101.06 or level of protection “6” in accordance with DSTU 8782:2018 |
| 1.3 | Tactical armor carriers are compatible with main ballistic panels that have size 250x300mm |
| 1.4 | Tactical armor carriers have evacuation straps (emergency drag handles) on the rear side |
| 1.5 | Tactical armor carriers have VELCRO panels on the front and rear sides |
| 1.6 | Tactical armor carriers have MOLLE panels on the front and rear sides |
| 1.7 | Tactical armor carriers have a quick-release solution |
| 1.8 | Tactical armor carriers have at least 4 adjustment points (one on each shoulder and one on each side in the lower part of a plate carrier) |
| 1.9 | Tactical armor carriers have internal mesh lining to improve ventilation |
| 1.10 | Tactical armor carriers (without main ballistic panels, side, groin, and neck protection) are lightweight (not more than 2 kg). |
| 1.11 | Tactical armor carriers are made in one of the following colors: blue (preferable), black, or grey |
| 1.12 | Tactical armor carriers are made in the following sizes: S, M, L, and XL |
| 1.13 | Tactical armor carriers have side protection |
| 1.14 | Side protection has a rated level of protection “Type IIIa” in accordance with NIJ Standard 0101.06or level of protection “2” in accordance with DSTU 8782:2018 |
| 1.15 | Tactical armor carriers have detachable groin protection |
| 1.16 | Detachable groin protection has a rated level of protection “Type IIIa” in accordance with NIJ Standard 0101.06or level of protection “2” in accordance with DSTU 8782:2018 |
| 1.17 | Tactical armor carriers have flame resistance - any (preferable according to standard BS 6941:2003) |
| **2** | **General requirements** |
| 2.1 | All the mentioned equipment should be new. |
| 2.2 | Bid includes the brand/model of the goods and the manufacturer's technical literature/catalog, all confirming that the offered items comply with the required specifications |
| 2.3 | **Warranty:** at least 1 year |
| 2.4 | Technical documentation for maintenance and repair of the supplied goods. The minimum set of technical documents to be provided with each piece of equipment delivered is the following: • User Manual and Operating Instructions (in Ukrainian or English) • Technical Certificate/maintenance guidelines (in Ukrainian or English) The Bidder is required to confirm the list and contents of documentation to be provided together with the Goods at the delivery. All tags/labels on the equipment shall be in English or Ukrainian language. |
| 2.5 | Bid includes the Country of origin of the goods. |

**C. 3. Delivery requirements for Lot 3**

| **UNOPS Requirements** | |
| --- | --- |
| **Delivery time** | Bidder shall deliver the goods as soon as possible **but not later than 30 days after PO issuance. Please indicate the delivery time in your Quotation**. |
| **Delivery place and Incoterms rules** | DAP Customs cleared Incoterms 2020 (delivered at place) Kyiv, Ukraine, net of any direct taxes, customs duties, or indirect taxes. |
| **Consignee details** | 2nd floor, 9B, Mykhaila Hrushevskoho str., BC SUMMIT, Kyiv, Ukraine. |
| **Acceptance** | Bidder shall remain liable for the packing and consistency of the items supplied for the period of shipment and acceptance for use. Any items found unacceptable shall be returned and changed at no cost to UNOPS. |
| **Packing standards** | Bidder shall ensure the best international packing standards of goods supplied, including the use of eco-friendly packing materials. |

**D. Inspections and tests**

Any delivered item may on or after delivery be inspected and will be rejected if found not compliant with the requirements of the contract. Such rejected items shall be held at the cost and risk of the supplier who shall, when called upon, remove them immediately at his own cost and forthwith substitute them with items that do comply with the requirements of the contract within 15 (fifteen) working days. Failing such removal, the rejected supplies shall be returned at the supplier's cost.