**Section II: Schedule of Requirements**

**eSourcing reference:**

1. **Technical specifications for Goods and Comparative Data Table**

| **Item No** | **UNOPS minimum technical requirements** | **Quantity** |
| --- | --- | --- |
| **01** | **FLAK Jackets - XXX-Large - UK//EU/US standard size**   * Protection Level NIJ 0101.04 IIIA or NIJ 0101.06 III+ * Adjustable from 38" To 48" Chest Size * Outer cover manufactured from tough, lightweight, nylon fabric, * Durable Emergency Drag Handle * Anti-slip Shoulder Padding With Velcro * Side Release Buckles On The Internal Waist Strap * Padded Mesh Separators For The Interior Of The Carrier For Breathability * Fits front and back Cut Plates * Horizontal VELCRO strip on the upper chest and back 10cmx 25cm * 1000 Denier/500D * Bottom Loading * Colour:Blue | 23 |
| **Hard Armour Upgrade Plates**   * Meet protection level NIJ 0101.04 IIIA or NIJ 0101.06 III+ combined with above. soft armour * back plates material should be Polyethylene (PE) * Set consisting of:   1. 1X multi-curved front chest plate   2. 1 x back plate |
| **Supplied with:**   * Carrying Case * Rear Evacuation Handle * Maintenance, fitting and adjustment guide |
| **02** | **FLAK Jackets - XX-Large - UK//EU/US standard size**   * Protection Level NIJ 0101.04 IIIA or NIJ 0101.06 III+ * Adjustable from 38" To 48" Chest Size * Outer cover manufactured from tough, lightweight, nylon fabric, * Durable Emergency Drag Handle * Anti-slip Shoulder Padding With Velcro * Side Release Buckles On The Internal Waist Strap * Padded Mesh Separators For The Interior Of The Carrier For Breathability * Fits front and back Cut Plates * Horizontal VELCRO strip on the upper chest and back 10cmx 25cm * 1000 Denier/500D * Bottom Loading * Colour: Blue | 72 |
| **Hard Armour Upgrade Plates**   * Meet protection level NIJ 0101.04 IIIA or NIJ 0101.06 III+ combined with above. soft armour * Set consisting of:   1. 1X multi-curved front chest plate   2. 1 x back plate |
| **Supplied with:**   * Carrying Case * Rear Evacuation Handle * Maintenance, fitting and adjustment guide |
| **03** | **FLAK Jackets - X-Large - UK//EU/US standard size**   * Protection Level NIJ 0101.04 IIIA or NIJ 0101.06 III+ * Adjustable from 38" To 48" Chest Size * Outer cover manufactured from tough, lightweight, nylon fabric, * Durable Emergency Drag Handle * Anti-slip Shoulder Padding With Velcro * Side Release Buckles On The Internal Waist Strap * Padded Mesh Separators For The Interior Of The Carrier For Breathability * Fits front and back Cut Plates * Horizontal VELCRO strip on the upper chest and back 10cmx 25cm * 1000 Denier/500D * Bottom Loading * Colour: Blue | 61 |
| **Hard Armour Upgrade Plates**   * Meet protection level NIJ 0101.04 IIIA or NIJ 0101.06 III+ combined with above. soft armour * Set consisting of:   1. 1X multi-curved front chest plate   2. 1 x back plate |
| **Supplied with:**   * Carrying Case * Rear Evacuation Handle * Maintenance, fitting and adjustment guide |
| **04** | **FLAK Jackets - Large - UK//EU/US standard size**   * Protection Level NIJ 0101.04 IIIA or NIJ 0101.06 III+ * Adjustable from 38" To 48" Chest Size * Outer cover manufactured from tough, lightweight, nylon fabric, * Durable Emergency Drag Handle * Anti-slip Shoulder Padding With Velcro * Side Release Buckles On The Internal Waist Strap * Padded Mesh Separators For The Interior Of The Carrier For Breathability * Fits front and back Cut Plates * Horizontal VELCRO strip on the upper chest and back 10cmx 25cm * 1000 Denier/500D * Bottom Loading * Colour: Blue | 44 |
| **Hard Armour Upgrade Plates**   * Meet protection level NIJ 0101.04 IIIA or NIJ 0101.06 III+ combined with above. soft armour * Set consisting of:   1. 1X multi-curved front chest plate   2. 1 x back plate |
| **Supplied with:**   * Carrying Case * Rear Evacuation Handle * Maintenance, fitting and adjustment guide |
| **05** | **FLAK Jackets - Medium - UK//EU/US standard size**   * Protection Level NIJ 0101.04 IIIA or NIJ 0101.06 III+ * Adjustable from 38" To 48" Chest Size * Outer cover manufactured from tough, lightweight, nylon fabric, * Durable Emergency Drag Handle * Anti-slip Shoulder Padding With Velcro * Side Release Buckles On The Internal Waist Strap * Padded Mesh Separators For The Interior Of The Carrier For Breathability * Fits front and back Cut Plates * Horizontal VELCRO strip on the upper chest and back 10cmx 25cm * 1000 Denier/500D * Bottom Loading * Colour: Blue | 27 |
| **Hard Armour Upgrade Plates**   * Meet protection level NIJ 0101.04 IIIA or NIJ 0101.06 III+ combined with above. soft armour * Set consisting of:   1. 1X multi-curved front chest plate   2. 1 x back plate |
| **Supplied with:**   * Carrying Case * Rear Evacuation Handle * Maintenance, fitting and adjustment guide |
| **06** | **FLAK Jackets - Small - UK//EU/US standard size**   * Protection Level NIJ 0101.04 IIIA or NIJ 0101.06 III+ * Adjustable from 38" To 48" Chest Size * Outer cover manufactured from tough, lightweight, nylon fabric, * Durable Emergency Drag Handle * Anti-slip Shoulder Padding With Velcro * Side Release Buckles On The Internal Waist Strap * Padded Mesh Separators For The Interior Of The Carrier For Breathability * Fits front and back Cut Plates * Horizontal VELCRO strip on the upper chest and back 10cmx 25cm * 1000 Denier/500D * Bottom Loading * Colour: Blue | 2 |
| **Hard Armour Upgrade Plates**   * Meet protection level NIJ 0101.04 IIIA or NIJ 0101.06 III+ combined with above. soft armour * Set consisting of:   1. 1X multi-curved front chest plate   2. 1 x back plate |
| **Supplied with:**   * Carrying Case * Rear Evacuation Handle * Maintenance, fitting and adjustment guide |
| **07** | **Ballistic helmets/HIGH CUT BALLISTIC HELMET - X-Large - UK//EU/US standard size**   * NIJ Standard-0106.01 * Resistant level IIIA * Protection level NIJ IIIA * The helmet material shall be PE * Water, oil and vibration resistant * Temperature, altitude and pressure stable * Improved internal pad system for easy adjustment and improved wearer comfort * Air gap between pads and shell provides excellent ventilation and improved sweat management * Non magnetic, non corrosive parts * Multiple point adjustable harness * Quick release buckles * Colour: Blue | 79 |
| **08** | **Ballistic helmets/HIGH CUT BALLISTIC HELMET - Large - UK//EU/US standard size**   * NIJ Standard-0106.01 * Resistant level IIIA * Protection level NIJ IIIA * The helmet material shall be PE * Water, oil and vibration resistant * Temperature, altitude and pressure stable * Improved internal pad system for easy adjustment and improved wearer comfort * Air gap between pads and shell provides excellent ventilation and improved sweat management * Non magnetic, non corrosive parts * Multiple point adjustable harness * Quick release buckles * Colour: Blue | 75 |
| **09** | **Ballistic helmets/HIGH CUT BALLISTIC HELMET - Medium - UK//EU/US standard size**   * NIJ Standard-0106.01 * Resistant level IIIA * Protection level NIJ IIIA * The helmet material shall be PE * Water, oil and vibration resistant * Temperature, altitude and pressure stable * Improved internal pad system for easy adjustment and improved wearer comfort * Air gap between pads and shell provides excellent ventilation and improved sweat management * Non magnetic, non corrosive parts * Multiple point adjustable harness * Quick release buckles * Colour: Blue | 75 |

1. **Delivery requirements and Comparative Data Table:**

| **UNOPS Requirements** | | **Is quotation compliant?** Bidder to complete | **Details**  Bidder to complete |
| --- | --- | --- | --- |
| **Delivery time** | Bidder shall deliver the goods within 12 weeks after Contract signature (including export license permit approval). | ☐ Yes ☐ No | Insert details |
| **Delivery place and Incoterms rules** | CPT (Incoterm 2020) to Kabul International airport. | ☐ Yes ☐ No | Insert details |
| **Consignee details** | UNOPS office, UNOCA Compound, Kabul Afghanistan. | ☐ Yes ☐ No | Insert details |
| **Manufacturer's Authorization** | If a Bidder does not manufacture the goods it offers to supply, he/she shall submit the Manufacturer’s Authorization using the form included in Section III: Returnable Bidding Forms (Form G) to demonstrate that it has been duly authorized by the manufacturer or producer of the goods to supply these goods in the country of destination. | ☐ Yes ☐ No | Insert details |
| **Environmental sustainability - Product life cycle extension** | The bidder shall demonstrate that packaging material includes recycled content (e.g. recycled cardboard) and that use of single-use plastic is avoided or minimised. Bidder shall provide a written statement that includes the applicable parts that are replaceable. A guarantee of the continued availability of spare parts. | ☐ Yes ☐ No | Insert details |
| **UNOPS Right to vary requirements** | At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- 20%, without any change in the unit prices or other terms and conditions of the RFQ. | ☐ Yes ☐ No | Insert details |