**Section II: Schedule of Requirements**

1. **Technical specifications for Goods**

| **Lot No** | **Required Item** | **Quantity** | **Required Specifications** | **Equivalent Sample Pictures for Guidance Only** |
| --- | --- | --- | --- | --- |
| 1 | Mechanical body weight scale | 4,710 units | **Material:** Durable steel construction | Mechanical Bathroom Weight Scale (LC NZOO 11) |
| Size:  **Length**: Between 28cm to 33cm  **Width**: Between 28cm to 33cm  **Thickness**: Between 5cm to 6cm |
| **Measuring weight** in/Display in: Kg |
| **Loading capacity**/Capacity for holding weight up to: 130Kg |
| **Readout Screen**/Display: Analog display (mechanical display) for monitoring weight with clear, reliable and easy-to-read readout/screen.  **Note:** **Scale with digital readout/display** **will not be accepted.** |
| **Usage**: For taking body weight |
| **Structure color**: Any color |
| The Labels and instruction of use shall be in English language. |
| **Product Catalogue**: Bidder is required to provide the catalogue of the offered product with the bid submitted. |
| **Sample:** Bidder is required to provide a sample of the offered product.  The sample shall be delivered to UNOPS within 05 working days from the bid submission deadline. |
| Bidder is required to provide brand name and country of manufacture of the offered product. |
| 2 | Digital medical thermometer | 3,260 units | **Measurement rage**: Min. 32°C to 42°C | \\unopskh540001\userhome$\youklint\Desktop\Capture-.PNG  \\unopskh540001\userhome$\youklint\Desktop\Therm.PNG |
| **Accuracy**: ±0.1°C |
| Display Unit: 0.1°C |
| **Memory**: Last temperature memory function (see last recorded temperature) |
| **Taking time**: 10-60seconds (Take max. 60 seconds to measure body temperature), preferably less than 30sec. |
| With beeping sound (buzzer) allowing to know when measurement is complete. |
| **Auto shut-off** (Automatic Power Off System: Less than 30 minutes. |
| Operated with one 1.5V battery (LR41).  Each thermometer shall come **with a battery** in it, which will allow for instant operation |
| The thermometer shall allow for **easy change of battery** – (this shall be assed at sample review) |
| **With low battery indication** |
| **Battery life**: 4000 takes (±500 takes) |
| **Size**: 128mm x 17mm x 8mm (±5mm)  (Length x Width x Height or thickness) |
| **Usage**: For measuring body temperature |
| **Accessory**: Each thermometer shall have a full hard plastic protection box. |
| The Labels and instruction of use shall be in English language. |
| **Product Catalogue**: Bidder is required to provide the catalogue of the offered product with the bid submitted. |
| **Sample**: Bidder is required to provide a sample of the offered product.  The sample shall be delivered to UNOPS within 05 working days from the bid submission deadline.  Provide brand name and country of manufacture |
| 3 | Hard plastic box for storing medical items | 1,450 units | **Item** Description– Clear hard plastic box with cover |  |
| **Materia**l – Heavy duty moulded clear plastic |
| **Basic Product Colour** – Transparent |
| IMG_20170706_144034**Lid Colour:** Any colour |
| **Features** - Carrying Handle, Lid, Clip Handle |
| **Size:**  Length: Between 29cm to 32cm  Width: Between 19cm to 22 cm  Height: Between 17cm to 20cm |
| **Inside the box:** The inside shall have **no** **divider nor** **tray** |
| **Picture:** Bidder is required to provide picture of the offered product with the bid submitted. |
| 4 | Digital Alarm Timer | 3,260 units | **Material**: Hard plastic | \\unopskh540001\userhome$\youklint\Desktop\Capture.PNG |
| **Interval of time**: From 0 second to 99 minutes 59 seconds |
| **Size**: Minimum L 7.5cm X W5.2 cm |
| Others: The digital alarm timer shall be supplied **with battery** required for operation for each timer. |
| The Labels and instruction of use shall be in English language. |
| **Product Catalogue**: Bidder is required to provide the catalogue of the offered product with the bid submitted. |
| **Sample:** Bidder is required to provide a sample of the offered product.  The sample shall be delivered to UNOPS within 05 working days from the bid submission deadline. |
| Bidder is required to provide brand name and country of manufacture of the offered product. |

**B- Delivery Requirements:**

|  |  |
| --- | --- |
| **UNOPS Requirements** | |
| **Delivery time** | Bidder shall deliver the goods within 8-10 weeks after Contract signature. |
| **Delivery place** | Phnom Penh, Cambodia |
| **Incoterms rules (2010)** | CPT, Phnom Penh, Cambodia. |
| **Consignee details** | Name:  National Center for Parasitology, Entomology and Malaria Control (CNM)  Address:  Corner Street 92, Trapeing Svay, Sangkat Phnom Penh Thmey, Khan Sen Sok, Phnom Penh, Cambodia. |
| **UNOPS Right to vary requirements** | At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- 20%, without any change in the unit prices or other terms and conditions of the RFQ. |

**C- Documents Required from the Awarded Bidder:**

|  |  |
| --- | --- |
| **UNOPS Requirements** | |
| **Manufacturer’s Authorization**  **(mandatory for successful bidder for Lot 1)** | The successful bidder is required to provide the Manufacturer’s Authorization at the stage of contracting – this applies to Lot 1 only.  Use form included in Section III: Returnable Bidding Forms |
| **Shipping documents required**  **(mandatory for successful bidder for any Lot)** | The following documents shall be provided;   1. Commercial Invoice: 1 original and 2 certified copies.   These should indicate the United Nations Office for Project Services Cambodia as the Purchaser, the PO number, Goods description, quantity, unit price, and total amount. Invoices must be signed in original and stamped, or sealed with the company seal.   1. Airway Bill/Bill of Lading: 1 original and 2 copies 2. Packing List: 1 original and 2 copies 3. Certificate of Origin: 1 original and 2 copies   Scanned copies of the above mentioned shipping documents are required to be emailed to the office of UNOPS Cambodia within 10 working days prior to arrival of goods – to aid the customs clearance process. |